;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J528 - Roof Electronics (#38)
;
; P/N: 4E0-910-135-???
;
; includes measuring blocks, adaptation, coding and selective output test
;
; created on 06/Jun/2006 by Sebastian Stange (Sebastian@Ross-Rech.com)
;
; last modification on 02/Nov/2011
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30),Specification: 8.5...15.5 V
001,2,Switched Supply,for Outputs
; xxx? = Interior Mirror/Light Sensor
; xx?x = Humidity Sensor
; x?xx = Humidity Sensor Heater
; ?xxx = Sunroof Rotation Switch
;
002,0,,
002,1,Interior Light,Buttons
; xxxxxx? = Front ON Button
; xxxxx?x = Front OFF Button
; xxxx?xx = Front AUTO Button
; xxx?xxx = Rear ON Button
; xx?xxxx = Rear OFF Button
; x?xxxxx = Rear AUTO Button
; ?xxxxxx = Light Profile Button
002,2,Front Interior,Light Dimming,Range: 0.0...100.0 %
002,3,Rear Interior,Light Dimming,Range: 0.0...100.0 %
002,4,Reading Light,Buttons
; xxx? = Front Right Reading Light Button
; xx?x = Front Left Reading Light Button
; x?xx = Rear Right Reading Light Button
; ?xxx = Rear Left Reading Light Button
;
003,0,Automatic Day/Night Interior Mirror
003,1,Light Sensor,Signal Status,Range: ON/OFF/Invalid
003,2,Mirror,Dimming Value,Range: 0.0...100.0 %
;
004,0,Sunroof
004,1,Sunroof Buttons
; xxx? = Sunroof Open Button
; xx?x = Sunroof Close Button
; x?xx = Audi-Coding
; ?xxx = Sunroof Standardization
004,2,Potentiometer,Voltage,Range: 0.1...4.9 V
004,3,Reference,Voltage,Range: 0.1...4.9 V
;
005,0,Climate Sensor
005,1,Thermopile Signal,,Range: 0.1...4.9 V
005,2,Reference,Temp. Signal,Range: 0.1...4.9 V
005,3,Solid Body,Temp. Signal,Range: 0.1...4.9 V
005,4,Humidity,Frequency Signal,Range: 50...85 ms
;
006,1,Garage Door,Opener Status,0 = OFF / 1 = ON
; xx? = Garage Door Opener 1
; x?x = Garage Door Opener 2
; ?xx = Garage Door Opener 3
006,2,Rear/Side Shades,Buttons,0 = OFF / 1 = ON
; xx? = Left Side Shades Button
; x?x = Right Side Shades Button
; ?xx = Rear Shades Button
006,3,Sunshade Switches,,0 = OFF / 1 = ON
; x? = Sunshade Switch (Mirror) Front Right
; ?x = Sunshade Switch (Mirror) Front Left
;
007,0,Lights
007,1,Function LED,Dimming,Range: 0.0...100.0 %
007,2,Rear Background,Light Dimming,Range: 0.0...100.0 %
007,3,Interior Light,Auto Rear,Range: ON/OFF
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Interior Monitoring Sensitivity
A001,5,Interior Monitoring Sensitivity
A001,6,Range: 50...100 %
A001,7,Standard: 100 %
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Roof Electronics (J528) Coding
C01,+0000001 = Standard/Basic Equipment
C02,+0000002 = Steel/Alloy Sunroof (PR-3FD) installed
C03,+0000004 = Glass Sunroof (PR-3FE) installed
C04,+0000006 = Solar Sunroof (PR-3FR) installed
C05,+0000008 = Sunroof Air Recirculation active
C06,+0000016 = Rear Shades installed (PR-3Y2/3Y5) installed
C07,+0000032 = Rear/Side Shades installed (PR-3Y8) installed
C08,+0000064 = Driver Identification (PR-4K5/4K6) installed
C09,+0000128 = Light Profile (PR-QQ1/QQ3) activ
C10,+0000256 = Garage Door Opener (PR-VC1) installed
C11,+0000512 = Light Sensor (G399) (PR-8K7) installed
C12,+0001024 = Automatic Day/Night Interior Mirror (PR-4L6) installed
C13,+0002048 = Climate Sensor installed
C14,+0032768 = Right Hand Steering (PR-L0R)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1487,System Function Test
;
