;
; VCDS Label File
;
; Copyright © 2001+ Ross-Tech, LLC
;
; Seat Leon/Toledo (1M) / Skoda Octavia (1U) / VW Bora/Golf (1J)
; VW New Beetle (1C/9C) / VW Passat (3B) / VW Polo Classic (9V)
;
; Component: J393 - Comfort System (#46) - Generation II (< MY 2002)
;
; P/N: 1J0-959-799-???
;
; includes measuring blocks, adaptation and coding
;
; based on 1J0-959-799.lbl by Mike Sauve (www.alientech.net)
; updated/enhanced on 28/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 14/Nov/2013
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General (Driver Side)
001,1,Child Safety Lock,Button (E319),Range: Yes/No/Not Installed
001,2,Interior Locking,Button (E150),Range:  Lock/Unlock/Not Oper./Not Installed
001,3,Window Regulator,Hall Signal,Range: Rotating/Stop
;
002,0,Window Regulator Buttons (Driver's Door)
002,1,WR-Button (E40),Driver Door,Range: auto. open/auto. close/man. open/man. close/close not operated/implausible
002,2,WR-Button (E81),Passenger Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
002,3,WR-Button (E53),Rear Left Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
002,4,WR-Button (E55),Rear Right Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
;
003,0,Central Locking (Driver Door)
003,1,Central Locking,Key Switch Drv.,Range: open/closed/not operated/implausible
003,2,Rotary Latch &,Thermal-Protection,0x = Rotary Latch/Door closed\n1x = Rotary Latch/Door open\nx0 = Thermal Protection active\nx1 = Thermal Protection inactive
003,3,Central Locking,Feedback Driver,Range: Locked/Unlocked
003,4,Safe Feedback,Driver Door,Range: safe/not safe
;
004,0,Mirror Adjustment && Folding
004,1,Mirror Adjustment,Switch Driver (E43),Range: Pos X+/Pos X-/Pos Y+/Pos Y-/not operated
004,2,Mirror Selection,Switch Driver (E48,Range: left/right/fold/not operated
004,3,Mirror Folding,Switch (E263),Range: released/engaged/not installed
;
005,0,General (Passenger Side)
005,1,WR-Button (E107),Passenger Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
005,2,Interior Locking,Switch Pass. (E198),Range: Lock/Unlock/Not Oper./Not Installed\n\Note: North American Region (NAR) only
005,3,Mirror Folding,Switch (E263),Range: released/engaged/not installed
;
006,0,Central Locking (Passenger Door)
006,1,Central Locking,Key Switch Pass.,Range: open/closed/not operated/implausible
006,2,Rotary Latch &,Thermal-Protection,0x = Rotary Latch/Door closed\n1x = Rotary Latch/Door open\nx0 = Thermal Protection active\nx1 = Thermal Protection inactive
006,3,Central Locking,Feedback Pass.,Range: Locked/Unlocked
006,4,Safe Feedback,Passenger Door,Range: safe/not safe
;
007,0,Central Locking (Rear Right Door)
007,1,WR-Button (E54),Rear Right Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
007,2,Rotary Latch &,Thermal-Protection,0x = Rotary Latch/Door closed\n1x = Rotary Latch/Door open\nx0 = Thermal Protection active\nx1 = Thermal Protection inactive
007,3,Central Locking,Feedback Rear Right,Range: Locked/Unlocked
007,4,Safe Feedback,Rear Right Door,Range: safe/not safe
;
008,0,Central Locking (Rear Left Door)
008,1,WR-Button (E52),Rear Left Door,Range: autom. open/autom. close/man. open/man. close/not operated/implausible
008,2,Rotary Latch &,Thermal-Protection,0x = Rotary Latch/Door closed\n1x = Rotary Latch/Door open\nx0 = Thermal Protection active\nx1 = Thermal Protection inactive
008,3,Central Locking,Feedback Rear Left,Range: Locked/Unlocked
008,4,Safe Feedback,Rear Left Door,Range: safe/not safe
;
009,1,Illuination,(Terminal 58d),Range: 0...100 %
009,2,Vehicle Speed,,Steps: 2 km/h
009,3,Remote Control,Button,Range: Open/Closed/Rear Lid Release/Panic
009,4,Interior Monitoring,Sensor (G273),Range: Yes/No/Not Installed
;
010,1,Terminal S,Status,Range: operated/not operated
010,2,Mirror heating,(E231),Range: on/off/not installed
010,3,Rear Lid/Tailgate,Key Switch (E165),Range: open/closed/not operated/implausible
010,4,Terminal 15,Status,Range: Terminal 15 ON/Terminal 15 OFF
;
011,0,Engine Hood && Rear Lid
011,1,Hood Contact,Switch (F120),Range: operated/not operated/not installed
011,2,Rear Lid/Tailgate,Contact Sw. (F124),Range: open/closed
011,3,Sliding/Tilting,Sunroof released,Range: Yes/No
;
012,0,CAN-Databus Communication
012,1,CAN-Databus,Status,Specification: 2-wire
012,2,Door Control,Modules (Front),Range: Driver/Passenger
012,3,Door Control,Modules (Rear),Range: RL/RL and RR/RR
012,4,Additional,Equipment,Range: Memory
;
013,0,Remote Control
013,1,Permanent Code,known,Range: OK/n.OK
013,2,Code within,effective Range,Range: OK/n.OK
013,3,Algorithm,Status,Range: OK/n.OK
013,4,Remote Control,Key Number,Range: 0...4 (0 = not operated)
;
014,1,Supply Voltage,(Terminal 30)
014,2,Rear Lid Button (E188),Rear Lid Handle (E234),Range: not operated/remote switch/lid lever/implausible
014,3,Interior Monitoring,Switch-Off (E267),Range: on/off/not installed
014,4,Central Locking,Thermal Protection,?xxxx = Drivers Side\nx?xxx = Passengers Side\nxx?xx = Rear Left (RL)\nxxx?x = Rear Right (RR)\nxxxx? = Rear Lid\n\nRange: 0 = inactive / 1 = active
;
015,0,Alarm Source
; Rear Left/Right Value may be reversed based on Control Module Version. Check Measuring Value Blocks (MVB) if in Doubt!
;   1 = Rear Lid/Tailgate Contact Switch
;   2 = Rear Right OR Rear Left Rotary Latch Switch
;   4 = Rear Left OR Rear Right Rotary Latch Switch
;   8 = Passenger Door Rotary Latch Switch
;  16 = Ignition
;  17 = Immobilizer
;  32 = Interior Monitoring
;  64 = Engine Hood Contact Switch
; 128 = Driver's Door Rotary Latch Switch
; 255 = No Alarm
015,1,1st Alarm Source,,1 = Rear Lid/Tailgate Contact Switch\n2 = Rear Right OR Rear Left Rotary Latch Switch\n4 = Rear Left OR Rear Right Rotary Latch Switch\n8 = Passenger Door Rotary Latch Switch\n16 = Ignition\n17 = Immobilizer\n32 = Interior Monitoring\n64 = Engine Hood Contact Switch\n128 = Driver's Door Rotary Latch Switch\n255 = No Alarm\n\nRear Left/Right Value may be reversed based on Control Module Version. Check Measuring Value Blocks (MVB) if in Doubt!
015,2,2nd Alarm Source,,1 = Rear Lid/Tailgate Contact Switch\n2 = Rear Right OR Rear Left Rotary Latch Switch\n4 = Rear Left OR Rear Right Rotary Latch Switch\n8 = Passenger Door Rotary Latch Switch\n16 = Ignition\n17 = Immobilizer\n32 = Interior Monitoring\n64 = Engine Hood Contact Switch\n128 = Driver's Door Rotary Latch Switch\n255 = No Alarm\n\nRear Left/Right Value may be reversed based on Control Module Version. Check Measuring Value Blocks (MVB) if in Doubt!
015,3,3rd Alarm Source,,1 = Rear Lid/Tailgate Contact Switch\n2 = Rear Right OR Rear Left Rotary Latch Switch\n4 = Rear Left OR Rear Right Rotary Latch Switch\n8 = Passenger Door Rotary Latch Switch\n16 = Ignition\n17 = Immobilizer\n32 = Interior Monitoring\n64 = Engine Hood Contact Switch\n128 = Driver's Door Rotary Latch Switch\n255 = No Alarm\n\nRear Left/Right Value may be reversed based on Control Module Version. Check Measuring Value Blocks (MVB) if in Doubt!
015,4,4th Alarm Source,,1 = Rear Lid/Tailgate Contact Switch\n2 = Rear Right OR Rear Left Rotary Latch Switch\n4 = Rear Left OR Rear Right Rotary Latch Switch\n8 = Passenger Door Rotary Latch Switch\n16 = Ignition\n17 = Immobilizer\n32 = Interior Monitoring\n64 = Engine Hood Contact Switch\n128 = Driver's Door Rotary Latch Switch\n255 = No Alarm\n\nRear Left/Right Value may be reversed based on Control Module Version. Check Measuring Value Blocks (MVB) if in Doubt!
;
016,1,Immobilizer,Key Recognition,Range: yes/no/not installed
016,2,Automatic,Lock/Unlock Switch,Range: operated/not oper./implausible
016,3,Rear Lid,first Detent,Range: open/closed/not installed
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,Central Locking (2-Power Windows):
C02,00256 = Selective unlocking
C03,00257 = Unlocking of all doors
C04, 
C05,Central Locking (2-Power Windows and Memory Seats):
C06,00258 = Selective unlocking
C07,00259 = Unlocking of all doors
C08, 
C09,Central Locking (4-Power Windows):
C10,04096 = Selective unlocking
C11,04097 = Unlocking of all doors
C12, 
C13,Central Locking (4-Power Windows and Memory Seats):
C14,04098 = Selective unlocking
C15,04099 = Unlocking of all doors
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Remote control adaptation
A01,5,Remote control adaptation
A01,6,Enter the number of keys that should be adapted. Save.
A01,7, 
A01,8,Now press button 1 or 2 on every remote that
A01,9,should be adapted for at least 1 second.
A01,10, 
A01,11,Note #1: All keys must be adapted in one procedure.
A01,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
A003,0,Auto-Lock
A003,5,Auto-Lock
A003,6,The doors will lock automatically when the
A003,7,vehicle reaches a speed of 15 km/h or 10 mph.
A003,8, 
A003,9,Range: 0 = OFF / 1 = ON
;
A004,0,Auto-Unlock
A004,5,Auto-Unlock
A004,6,The doors will unlock automatically when the key
A004,7,is removed from the ignition switch.
A004,8, 
A004,9,Range: 0 = OFF / 1 = ON
;
A005,0,Interior Monitoring
A005,5,Interior Monitoring
A005,6,Activation of interior monitoring system.
A004,7, 
A004,8,Range: 0 = OFF / 1 = ON
;
A006,0,Unlock Horn
A006,5,Unlock Horn
A006,6,Horn beep when unlocking via remote control.
A006,7, 
A006,8,Range: 0 = OFF / 1 = ON
;
A007,0,Lock Horn
A007,5,Lock Horn
A007,6,Horn beep when locking via remote control.
A007,7, 
A007,8,Range: 0 = OFF / 1 = ON
;
A008,0,Unlock Blink
A008,5,Unlock Blink
A008,6,Blink when unlocking via remote control.
A008,7, 
A008,8,Range: 0 = OFF / 1 = ON
;
A009,0,Lock Blink
A009,5,Lock Blink
A009,6,Blink when locking via remote control.
A009,7, 
A009,8,Range: 0 = OFF / 1 = ON
;
A010,0,Country Setting
A010,5,Country Setting
A010,6,Country setting for Alarm Horn.
A010,7, 
A010,8,1 = Rest of World (RoW)
A010,9,2 = Germany (DE)
A010,10,3 = Great Britain (GB)
;
