;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A2 (8Z) / Audi A3 (8L) / Audi A4 (8E) / Audi A6 (4B)
; Audi A8 (4D) / Audi TT (8N)
;
; Component: R - Radio (#56) Generation II
;
; P/N: 8E0-035-1??-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8E-56.LBL
; 8H-56.LBL
; 8L-56.LBL
; 8E0-035-1xx-56.LBL
;
; created on 25/Aug/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 11/Jul/2012
;
; requires VCDS 11.11.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Information
001,1,Supply Voltage,(Terminal 30),Specification: 5...18 V
001,2,Amplifier,Control Output,Display Range: OK/Short Circuit
001,3,Telephone,Mute
001,4,Telephone,Mute,Display Range: ON/OFF
;
002,0,Loadspeaker Status
002,1,Front,Loadspeaker
002,2,Status Front,Loadspeaker,Display Range: OK/Short Circuit/Open Circuit
;
003,0,Condition of Remote feed Antenna
003,1,Type
003,2,Component
003,3,Status,,Display Range: OK/Short Circuit/Open Circuit
;
004,0,Communication Status CD-Changer (R41)
004,1,Component
004,2,Status,,Display Range: OK/not OK
;
005,0,Status IF-Output
005,1,IF-Output
005,2,Status,IF-Output,Display Range: OK/Short Circuit/Open Circuit
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,VIN & Radio Serial Number
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A004,0,Volume
A004,5,Volume
A004,6,Range: 0...30 dB
A004,7, 
A004,8,The selected Volume will stay active
A004,9,after closing the Diagnostic Session.
;
A005,0,Signal Position
A005,5,Signal Position
A005,6,0 = Fader Center / Balance Center
A005,7,1 = Fader Front / Balance Left
A005,8,2 = Fader Front / Balance Right
A005,9,3 = Fader Rear / Balance Left
A005,10,4 = Fader Rear / Balance Right
;
A055,0,External Tuner
A055,5,External Tuner
A055,6,+1 = Satellite Tuner (SDARS) installed
A055,7,+2 = Digital Radio Tuner (DAB) installed
;
A066,0,GALA
A066,5,GALA
A066,6,0 = GALA active
A066,7,1 = GALA inactive (or Bose Audio Pilot installed)
;
A088,0,Long-Wave Band
A088,5,Long-Wave Band
A088,6,0 = Long-Wave Band active
A088,7,1 = Long-Wave Band inactive 
;
A099,0,Transport Mode
A099,5,Transport Mode
A099,6,0 = Transport Mode inactive
A099,7,1 = Transport Mode active
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,?xxxx: Options
C02,+1 = Front Speaker Diagnosis inactive
C03,x?xxx: Tone Characteristics (< MY 2001)
C04,0 = Linear Tone Characteristics (All Radios)
C05,x?xxx: Tone Characteristics (MY 2002 >)
C06,0 = Tone Characteristics for all other Models and all Radio Chorus
C07,1 = Tone Characteristics for A4 (8E)
C08,2 = Tone Characteristics for A6 (4B) & Audi A2 (MY 2005 >)
C09,3 = Tone Characteristics for A4 Cabriolet (8H)
C10,4 = Tone Characteristics for TT (8N)
C11,5 = Tone Characteristics for A3 (8L) 
C12,xx?xx: Fader/BOSE/Amplifier
C13,+1 = Fader-Display OFF
C14,+2 = BOSE-Display ON
C15,+4 = Mute Amplifier when using Phone
C16,xxx?x: Installation Options I
C17,+1 = Navigation installed
C18,+2 = Telephone installed
C19,+4 = Voice Control installed 
C20,xxxx?: Installation Options II
C21,+1 = Diversity Antenna installed
C22,+2 = CD-Changer installed
C23,+4 = Multifunction Steering Wheel installed
;
