;
; VAG-COM Label File
;
; VW Passat (3B)
;
; Component: J393 - Comfort System (#46) - Generation I (< MY 1997)
;
; P/N: 3B0-959-79?-???
;
; includes measuring blocks, coding and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3B-46.LBL
; 3B0-959-79x-46.LBL
;
; created on 22/Jun/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 22/Jun/2007
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Child Safety,Switch (E39),Range: Yes/No/not installed
001,2,Interior Locking,Driver Sw. (E150),Range: lock/unlock/not operated/implausible)
001,3,Electric Window,Hall Signal,Range: rotating/stop
;
002,0,Driver's door (driver's switch for window regulators)
002,1,WR-Button (E40),Drivers Side,Display Range: auto. open/auto. close/man. open/man. close/close not operated/implausible
002,2,WR-Button (E81),Passenger Side,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
002,3,WR-Button (E53),Rear Left,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
002,4,WR-Button (E55),Rear Right,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
;
003,0,Driver Door
003,1,Driver Door,Key Switch,Display Range: implausible/open/closed/not operated
003,2,Driver Door,Rotary Switch,Display Range: Door open/Door closed
003,3,CL-Feedback,Drivers Side,Display Range: locked/unlocked
003,4,Safe-Feedback,Drivers Side,Display Range: safe/not safe
;
004,0,Driver Door (Mirror)
004,1,Mirror adjustment,switch driver (E43),Display Range: Pos X+/Pos X-/Pos Y+/Pos Y-/not operated
004,2,Mirror selection,switch driver (E48,Display Range: left/right/fold/not operated
004,3,Mirror folding,switch (E263),Display Range: released/engaged/not installed
;
005,0,Passenger Door
005,1,WR-Button (E107),Passenger Side,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
005,2,Interior locking,passenger switch,E198 - USA only (Display Range: lock/unlock/not operated/implausible)
005,3,Mirror folding,switch (E263),Display Range: released/engaged/not installed
;
006,0,Passenger Door
006,1,Central Locking,Key Switch Pass.,Display Range: open/closed/not operated/implausible
006,2,Thermal-Protection,Rotary Latch,Display Range (Rotary Latch): 0x = door closed / 1x = door open\nDisplay Range (Thermal-Protection): x0 = active / x1 = inactive
006,3,CL-Feedback,Passenger Side,Display Range: locked/unlocked
006,4,Safe-Feedback,Passenger Side,Display Range: safe/not safe
;
007,0,Door Rear Right
007,1,WR-Button (E54),Rear Right,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
007,2,Thermal-Protection,Rotary Latch,Display Range (Rotary Latch): 0x = door closed / 1x = door open\nDisplay Range (Thermal-Protection): x0 = active / x1 = inactive
007,3,CL-Feedback,Rear Right,Display Range: locked/unlocked
007,4,Safe-Feedback,Rear Right,Display Range: safe/not safe
;
008,0,Door Rear Left
008,1,WR-Button (E52),Rear Left,Display Range: autom. open/autom. close/man. open/man. close/not operated/implausible
008,2,Thermal-Protection,Rotary Latch,Display Range (Rotary Latch): 0x = door closed / 1x = door open\nDisplay Range (Thermal-Protection): x0 = active / x1 = inactive
008,3,CL-Feedback,Rear Left,Display Range: locked/unlocked
008,4,Safe-Feedback,Rear Left,Display Range: safe/not safe
;
009,1,Instrument,illumination,Display Range: 0...100 %
009,2,Speed Signal,,Steps: 2 km/h
009,3,Remote control,button,Display Range: open/closed/RLR/panic (RLR = rear lid release)
009,4,Interior monitor,sensor (G273),Display Range: yes/no/not installed
;
010,1,S-Terminal,,Display Range: operated/not operated
010,2,Mirror heating,(E231),Display Range: on/off/not installed
010,3,Rear lid/tailgate,key switch (E165),Display Range: open/closed/not operated/implausible
010,4,Ignition,,Display Range: Terminal 15 on/Terminal 15 off
;
011,1,Hood contact,switch (F120),Display Range: operated/not operated/not installed
011,2,Rear lid/tailgate,contact sw. (F124),Display Range: open/closed
011,3,Sliding/tilting,sunroof released,Display Range: yes/no
011,4,Central Locking,Thermal Prot.,Range:: Yes/No
;
012,0,CAN-Databus Communication
012,1,Status,CAN-Databus,Specification: 2-wire
012,2,Door Control,Modules (front),Display Range: Driver/Passenger
012,3,Door Control,Modules (rear),Display Range: rl/rl and rr/rr
012,4,Additional,Equipment,Display Range: Memory
;
013,0,Remote Control
013,1,Permanent code,known,Display Range: OK/n.OK
013,2,Code within,effective range,Display Range: OK/n.OK
013,3,Algorithm,,Display Range: OK/n.OK
;
014,0,Remote Control
014,1,Key number,,Display Range: 0...4 (0 = not operated)
;
015,0,Alarm source
;   1 - Rear lid/tailgate contact switch
;   2 - Rear left rotary latch switch
;   4 - Rear right rotary latch switch
;   8 - Front passenger rotary latch switch
;  16 - Ignition
;  17 - Immobilizer
;  32 - Interior monitoring
;  64 - Engine hood contact switch
; 128 - Driver's rotary latch switch
; 255 - No alarm
015,1,Last source
015,2,2nd last source
015,3,3rd last source
015,4,4th last source
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,Central Locking (2-Power Windows):
C02,00256 - Selective unlocking
C03,00257 - Unlocking of all doors
C04, 
C05,Central Locking (2-Power Windows and Memory Seats):
C06,00258 - Selective unlocking
C07,00259 - Unlocking of all doors
C08, 
C09,Central Locking (4-Power Windows):
C10,04096 - Selective unlocking
C11,04097 - Unlocking of all doors
C12, 
C13,Central Locking (4-Power Windows and Memory Seats):
C14,04098 - Selective unlocking
C15,04099 - Unlocking of all doors
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Remote control adaptation
A01,5,Remote control adaptation
A01,6,Enter the number of keys that should be adapted. Save.
A01,7, 
A01,8,Now press button 1 or 2 on every remote that
A01,9,should be adapted for at least 1 second.
A01,10, 
A01,11,Note #1: All keys must be adapted in one procedure.
A01,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
