;
; VCDS Label File
;
; Copyright © 2014+ Ross-Tech, LLC
;
; Audi Cabrio (8G)
;
; Component: J255 - Heating/Air Conditioning (#08)
;
; P/N: 4A0-919-579-???
;
; includes measuring blocks
;
; created on 20/Oct/2014 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 20/Oct/2014
;
; requires VCDS 12.12.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Compressor,Shut-Off,Specification: 0/1/6\n\n0 = Compressor ON\n1 = Compressor OFF: Start Delay/Engine Start OR Engine Speed too Low\n2 = Compressor OFF: Pressure Switch (F118) open OR Ambient Temperature below 5 °C OR Ambient Temperature Switch (F38) open\n3 = Compressor OFF: Coolant Temperature too High\n4 = Compressor OFF: Compressor Cut-In active\n5 = Compressor OFF: Belt Slip too High (1x > 60 % OR 10x 30...60 %) OR Control Module for Solenoid Coupling (J153) incorrect OR Compressor Speed not recognized\n6 = Compressor OFF: Kick-Down recognized (Shut-Off for 12 Seconds)\n7 = Compressor OFF: Kick-Down Switch (F8) closed statically
; 0 = Compressor ON
; 1 = Compressor OFF: Start Delay/Engine Start OR Engine Speed too Low
; 2 = Compressor OFF: Pressure Switch (F118) open OR Ambient Temperature below 5 °C OR Ambient Temperature Switch (F38) open
; 3 = Compressor OFF: Coolant Temperature too High
; 4 = Compressor OFF: Compressor Cut-In active
; 5 = Compressor OFF: Belt Slip too High (1x > 60 % OR 10x 30...60 %) OR Control Module for Solenoid Coupling (J153) incorrect OR Compressor Speed not recognized
; 6 = Compressor OFF: Kick-Down recognized (Shut-Off for 12 Seconds)
; 7 = Compressor OFF: Kick-Down Switch (F8) closed statically
001,2,Engine Speed
001,3,Compressor,Speed
001,4,Compresor,Belt Slip,Range: 0.0...100.0 %\n\n< 30.0 % = permitted/OK\n30.0...60.0 % = Compressor Cut-In for 10 Seconds OR permanently if detected multiple times\n> 60.0 % = Permanent Compressor Shut-Off
;
