;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; VW Passat (3C)
;
; Component: J521/J136 - Seat Adjustment (#06/#36)
;
; P/N: 3C0-959-760-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3C-06.LBL
; 3C-36.LBL
; 3C0-959-760.LBL
;
; includes measuring blocks and adaptation
;
; created on 17/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 21/Feb/2013
;
; requires VCDS 11.11.5 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Current Values (Longitudinal && Backrest Rake Adjustment)
001,1,Longitudinal Seat,Adjustment Button
001,2,Longitudinal Seat,Adjustment,Display Range: 0...65535
001,3,Backrest Rake,Adjustment Button
001,4,Backrest Rake,Adjustment,Display Range: 0...65535
;
002,0,Current Values (Seat Height && Seat Rake Adjustment)
002,1,Seat Height,Adjustment Button
002,2,Seat Height,Adjustment,Display Range: 0...65535
002,3,Seat Rake,Adjustment Button
002,4,Seat Rake,Adjustment,Display Range: 0...65535
;
003,0,Current Values (Lumbar Height && Lumbar Fore/Aft Adjustment)
003,1,Lumbar Height,Adjustment Button
003,2,Lumbar Height,Adjustment,Display Range: 0...65535
003,3,Lumbar Fore/Aft,Adjustment Button
003,4,Lumbar Fore/Aft,Adjustment,Display Range: 0...65535
;
006,0,Easy Entry
006,1,Easy Entry,Switch,Range: ON/OFF
006,2,Easy Entry,Function,Range: Active/Not Active\n\nSee Adaptation Channel 060.
;
007,0,Seat Memory I
007,1,Memory Position,Button 1 (E218),Display Range: Operated/Not Oper.
007,2,Memory Position,Button 2 (E219),Display Range: Operated/Not Oper.
007,3,Memory Position,Button 3 (E220),Display Range: Operated/Not Oper.
007,4,Memory Position,Button 4 (E282),Display Range: Operated/Not Oper.
;
008,0,Seat Memory II
008,1,Memory,Set-Button,Display Range: Operated/Not Oper.
008,2,Memory Function,,Display Range: Active/Not Active
008,4,Initialisation,,Display Range: Learned/Erased
;
009,0,Terminal Status
009,1,Voltage,Terminal 30,Specification: 9.0...15.25 V
009,2,Status,Terminal X,Display Range: ON/OFF
009,3,Status,Terminal 15,Display Range: Term 15 On/Term 15 Off
009,4,Status,Terminal S,Display Range: ON/OFF
;
010,1,Driver Door,,Display Range: Open/Closed
010,2,Key Number
010,3,Steering Type,,Display Range: Left/Right
010,4,Vehicle Speed
;
011,0,Current Values (Seat Depth)
011,1,Seat Depth,Adjustment Button
011,2,Seat Depth,Adjustment,Display Range: 0...65535
;
012,0,Massage
012,1,Massage Button,,Display Range: ON/OFF
012,2,Massage Function,,Display Range: Not Active/Active
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Reset Learned Values
A000,5,Reset Learned Values
A000,6,All learned Values have to be cleared when:
A000,7,A) The Motors can not be adjusted due to functional Problems.
A000,8,B) The following Parts have been replaced:
A000,9,- Seat Motor(s) or Sensor(s) or Mirror Motor(s)
A000,10,- Seatbelt Height Adjustment Motor(s) or Sensor(s)
A000,11,- Steering Column Adjustment Motor(s) or Sensor(s)
A000,12, 
A000,13,Once the Reset has been performed all Motors have to be manually
A000,14,ran from/to their Minimum and Maximum Positions. Once that is finished
A000,15,the Positions/Keys can be programmed again.
A000,16, 
A000,17,Note: Before replacing the above Components the Basic Settings
A000,18,has to be performed to avoid unnecessary Installation/Work.
;
A060,0,Easy Entry
A060,5,Easy Entry
A060,6,0 = Easy Entry Function inactive
A060,7,1 = Easy Entry Function active
;
