;
; VCDS Label File
;
; Copyright © 2004-2011 Ross-Tech, LLC
;
; VW Touareg (7LA)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 7L6-920-???-???
;
; includes coding, adaptation, measuring blocks
;          and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7L-17.LBL
; 7L6-920-xxx-17-7L6.LBL
; 7L6-920-xxx-17-7LA.LBL
;
; created on 13/Dec/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Aug/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuaring blocks
;
;---------------------------------------------------
;
;
001,0,Common Informations
001,1,Vehicle Speed,,via CAN from brake control module
001,2,Engine Speed,,via CAN from transmission control module
001,3,Oil Pressure,,Specified Value: Oilpr.2 i.O.
001,4,Clock
;
002,0,Common Informations
002,1,Mileage
002,2,Fuel Tank Content
002,4,Ambient,Temperature,Display Range: -45...+65 °C | +70 °C = short circuit | -50 °C = open circuit
;
003,0,Coolant && Oil Temperature
003,1,Coolant,Temperature,via CAN from engine control module
003,2,Oil Level
003,3,Oil Temperature
;
004,1,Battery Voltage
;
005,1,Fuel Gauge
005,2,Fuel Supply,Sensor 3
;
006,1,Tank Content,(Main Chamber)
006,2,Tank Content,(Side Chamber)
;
050,0,Common Informations
050,1,Mileage
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
060,0,Installation Information (Senders && Sensors)
;
061,0,Checking Installation Information
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbag
;
127,0,CAN-Databus Communication (Powertrain)
127,2,All wheel,drive (AWD)
;
128,0,CAN-Databus Communication (Powertrain)
128,2,Electrical Ignition
128,3,Level Control
;
130,0,CAN-Databus Communication (Comfort)
130,1,Comfort-CAN,Condition
130,2,Comfortsystem
130,3,Driver Door
130,4,Passenger Door
;
131,0,CAN-Databus Communication (Comfort)
131,1,Rear/Left Door
131,2,Rear/Right Door
131,3,Driver,Memory Seat
131,4,Electrical System
;
132,0,CAN-Databus Communication (Comfort)
132,2,Steering Wheel
132,3,Climate
132,4,Tire Pressure
;
133,0,CAN-Databus Communication (Comfort)
133,2,Passenger,Memory Seat
133,4,Parking Aid
;
134,0,CAN-Databus Communication (Comfort)
134,2,Electrical Ignition
;
140,0,CAN-Databus Communication (Infotainment)
140,1,Infotainment-CAN,Condition
140,3,Radio/Navigation
140,4,Telephone
;
141,0,CAN-Databus Communication (Infotainment)
141,3,TV-Tuner
;
143,0,CAN-Databus Communication (Infotainment)
143,1,Digital,Sound Package
143,3,Parking Heater
143,4,Roof Electronics
;
201,1,K-Value
201,2,Wheel,Circumference
201,3,Starting impulse,recognized
;
202,1,Engine Hood,Switch
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??xx1: Options
C02,+01 = Brakepad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,00xx?x1: Country
C06,1 = Europe / 2 = USA / 3 = Canada/Mexico/Latin America
C07,4 = Great Britain (GB) / 5 = Japan / 6 = Saudi Arabia / 7 = Australia
C08,00xxx?1: Service Intervals
C09,0 = fixed Service Intervals (PR-QG0) without Oil Level/Temperature Sensor
C10,1 = flexible Service Intervals with Oil Level/Temperature Sensor (PR-QG1)
C11,2 = fixed Service Intervals with Oil Level/Temperature Sensor (PR-QG2)
C12,3 = without Service Intervals (USA/Canada)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,8 = Czech
;
A09,0,Mileage
A09,5,Mileage shown in instrument cluster
A09,6,Mileage can only be changed once until it
A09,7,is not over 100 km/mi. On some instrument
A09,8,clusters you do not need any login/security
A09,9,code to change the value.
;
A30,0,Tank sensor
A30,5,Tank sensor
A30,6,Tank sensor can be adjusted by
A30,7,steps of 1 from 108 to 148.
;
A35,0,Undocumented
;
A60,0,Undocumented (DATA-BUS Engine)
;35951
;
A61,0,Undocumented (DATA-BUS Comfort)
;447
;
A62,0,Undocumented (DATA-BUS Infotainment)
;28752 = 111000001010000
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,1000,DIST
RD,43,ST_MADTS,1000,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
RC,0,0,The Service Reminder Reset Function is neither necessary nor possible on 
RC,0,1,North American Region (NAR) Models since there is no Service Reminder.
;
