;
; VCDS Label File
;
; Copyright © 2009+ Ross-Tech, LLC
;
; Audi R8 (42)
;
; Component: J104 - Brake Electronics (#03) - Bosch 8.0
;
; P/N: 420-910-517-???
;
; includes measuring blocks, basic setting, coding and security access
;
; created on 27/Aug/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 02/Oct/2014
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Steering Angel Sensor (G85) Alignment
B001,1,Steering Angel,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,1,Brake Test Switch,,0 = not operated\n1= operated
002,2,Brake Light Switch,,0 = not operated\n1= operated
002,3,Parking Brake,,0 = not operated\n1= operated
002,4,ESP-Button,,0 = not operated\n1= operated
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,,Display Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
005,2,Rotation Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,,Display Range: ON/OFF
006,4,Work Shop Code
;
007,0,Installation Position
007,1,Installation,Front Left (G47),Range: invalid/OK/Not OK (invalid at standstill)
007,2,Installation,Front Right (G45),Range: invalid/OK/Not OK (invalid at standstill)
007,3,Installation,Rear Left (G46),Range: invalid/OK/Not OK (invalid at standstill)
007,4,Installation,Rear Right (G44),Range: invalid/OK/Not OK (invalid at standstill)
;
008,0,Direction of Rotation
008,1,Rotat. Direction,Front Left (G47),Range: invalid/forward/reverse (invalid at standstill)
008,2,Rotat. Direction,Front Right (G45),Range: invalid/forward/reverse (invalid at standstill)
008,3,Rotat. Direction,Rear Left (G46),Range: invalid/forward/reverse (invalid at standstill)
008,4,Rotat. Direction,Rear Right (G44),Range: invalid/forward/reverse (invalid at standstill)
;
009,1,Brake Test Switch,,0 = not operated\n1= operated
009,2,Brake Light Switch,,0 = not operated\n1= operated
009,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
;
010,1,Transverse,Accel. (Raw Value),Specification: -1.25...+1.25 m/s²
010,2,Transverse,Accel. (Zero Value),Specification: -1.25...+1.25 m/s²
;
014,0,Airbag Coding Info (not relevant)
;
015,0,Engine Coding Info (not relevant)
;
016,0,Signals of Electro-Mechanical Parking Brake (not relevant)
;
021,0,ESP Sensor Unit (G419) Data
021,4,HW/SW Number
;
022,0,Steering Angle Sensor Data
;
023,0,Data Variant Coding
023,1,Data Variant,Coding
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor,Specification: Steer. ang. 1
125,2,Engine,,Specification: Engine 1
125,3,Automatic,Transmission,Specification: Transm. 1
125,4,Instrument Cluster,,Specification: Instruments 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Distance,Regulation (ACC),Specification: Distance 1
126,2,CAN-Gateway,,Specification: Gateway 1
126,3,Electric Parking,Brake (EPB),Specification: Park Brake 1
126,4,ESP Sensor,Cluster,Specification: ESP Sens. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,1,Level Control,,Specification: Level 1
127,2,Airbag,,Specification: Airbag 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Steering Angle,Sensor
225,2,Engine
225,3,Transmission
225,4,Instrument Cluster
;
226,0,CAN-Databus Time-Out (Powertrain)
226,2,CAN-Gateway
226,4,ESP Sensor,Cluster
;
227,0,CAN-Databus Time-Out (Powertrain)
227,2,Airbag
;
253,0,CAN-Databus Communication
253,2,ESP Sensor,Cluster (G419)
;
;
;---------------------------------------------------
;
; Codierung
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
C05,To request a proper Coding Value for this Control Module please
C06,Email Ross-Tech or your local Distrubutor. Make sure to include
C07,a complete Auto-Scan (full VIN as well) of the Vehicle as well
C08,as a short Description of what happened to the Car.
C09, 
C10,http://www.Ross-Tech.com/contact.html
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Brake Electronics (J104) Security Access
S01,40168 = Basic Setting Enabling
;
