;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi A4 Cabriolet (8HE)
;
; Component: J234 - Airbag (#15)
;
; P/N: 8H0-959-655-???
;
; includes measuring blocks, basic setting, security access, coding and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8H-15.LBL
; 8H0-959-655-84.LBL (Airbag 8.4)
; 8H0-959-655-94.LBL (Airbag 9.4x)
;
; created on 15/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 03/Jul/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Belt Tensioner,Rear Center,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Pyrotechnic Igniter,Battery Separating,Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch
010,1,Passenger,Airbag Status,Range: ON/OFF
010,2,Key Switch,Logic Contact 1,Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,Logic Contact 2,Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Ingniters V (Front Airbags Stage 2 && Front Knee Airbags)
011,1,Airbag (Stage 2),Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Airbag (Stage 2),Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Knee Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,4,Knee Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
012,0,Ingniters VI (Roll-Over Bars)
012,1,Roll-Over Bar,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
012,2,Roll-Over Bar,Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
012,3,Roll-Over Bar,Trigger Counter
012,4,Work Shop Code,Counter Reset
;
016,0,Seat Occupied Recognition Control Module (J706) I
016,1,Serial Number,(1/2)
016,2,Serial Number,(3/4)
016,3,Serial Number,(5)
016,4,Calibration Status
;
018,0,Seat Occupied Recognition Control Module (J706) II
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration,Sensor
;
019,0,Seat Occupied Recognition Control Module (J706) III
019,1,Workshop Code,(Last Coding)
019,2,Workshop Code,(Last 0-Balance)
;
020,1,Battery Separating
;
021,0,Igniter Resistance I (Front Airbags Stage 1 && Front Belt Tensioners)
021,1,Airbag (Stage 1),Driver Side
021,2,Airbag (Stage 1),Passenger Side
021,3,Belt Tensioner,Driver Side
021,4,Belt Tensioner,Passenger Side
;
022,0,Igniter Resistance II (Rear Belt Tensioners)
022,1,Belt Tensioner,Rear Left
022,2,Belt Tensioner,Rear Right
022,3,Belt Tensioner,Rear Center
022,4,Pyrotechnic Igniter,Battery Separating,
;
025,0,Igniter Resistance III (Side Airbags)
025,1,Side Airbag,Driver Side
025,2,Side Airbag,Passenger Side
025,3,Side Airbag,Rear Left
025,4,Side Airbag,Rear Right
;
031,0,Igniter Resistance V (Front Airbags Stage 2 && Front Knee Airbags)
031,1,Airbag (Stage 2),Driver Side
031,2,Airbag (Stage 2),Passenger Side
031,3,Knee Airbag,Driver's Side
031,4,Knee Airbag,Passenger Side
;
032,0,Igniter Resistance VI (Roll-Over Bars)
032,1,Roll-Over Bar,Driver Side
032,2,Roll-Over Bar,Pass. Side
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Instrument Cluster,(J285),Specification: Instruments 1\Range: Instruments 1/Instruments 0
125,2,Brake Electronics,(J104),Specification: ABS 1\Range: ABS 1/ABS 0
;
225,0,CAN-Databus Powertrain (TimeOut)
225,1,Instrument Cluster
225,2,Brake Electronics,(J104)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
;20324 = Seat Occupied Recognition Basic Setting/Zero Balancing (Siemens)
;30475 = Seat Occupied Recognition Basic Setting/Zero Balancing (Bosch)
S01,30475 = Basic Setting/Zero Balancing Enabling
S02,31415 = Output Test Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 = Front Passenger Airbag enabled (Standard)
A001,7,1 = Front Passenger Airbag disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,5,Front Driver Airbag Deactivation
A002,6,0 = Front Driver Airbag enabled (Standard)
A002,7,1 = Front Driver Airbag disabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 = Front Passenger Side Airbag enabled (Standard)
A003,7,1 = Front Passenger Side Airbag disabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 = Front Driver Side Airbag enabled (Standard)
A004,7,1 = Front Driver Side Airbag disabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
A005,0,Front Passenger Belt Tensioner Deactivation
A005,1,Front Passenger,Belt Tensioner
A005,2,Current Status
A005,5,Front Passenger Belt Tensioner Deactivation
A005,6,0 = Front Passenger Belt Tensioner enabled (Standard)
A005,7,1 = Front Passenger Belt Tensioner disabled
A005,8, 
A005,9,Note: Refer to Service Manual!
;
A006,0,Front Driver Belt Tensioner Deactivation
A006,1,Front Driver,Belt Tensioner
A006,2,Current Status
A006,5,Front Driver Belt Tensioner Deactivation
A006,6,0 = Front Driver Belt Tensioner enabled (Standard)
A006,7,1 = Front Driver Belt Tensioner disabled
A006,8, 
A006,9,Note: Refer to Service Manual!
;
A011,0,Rear Passenger Belt Tensioner Deactivation
A011,1,Rear Passenger,Belt Tensioner
A011,2,Current Status
A011,5,Rear Passenger Belt Tensioner Deactivation
A011,6,0 = Rear Passenger Belt Tensioner enabled (Standard)
A011,7,1 = Rear Passenger Belt Tensioner disabled
A011,8, 
A011,9,Note: Refer to Service Manual!
;
A012,0,Rear Driver Belt Tensioner Deactivation
A012,1,Rear Driver,Belt Tensioner
A012,2,Current Status
A012,5,Rear Driver Belt Tensioner Deactivation
A012,6,0 = Rear Driver Belt Tensioner enabled (Standard)
A012,7,1 = Rear Driver Belt Tensioner disabled
A012,8, 
A012,9,Note: Refer to Service Manual!
;
A021,0,Roll-Over Bar Deactivation
A021,1,Roll-Over Bars
A021,2,Current Status
A021,5,Roll-Over Bar Deactivation
A021,6,0 = Roll-Over Bars enabled (Standard)
A021,7,1 = Roll-Over Bars disabled
A021,8, 
A021,9,Note: Refer to Service Manual!
;
A050,0,ESP-Data (Powertrain)
A050,1,Powertrain
A050,5,ESP-Data (Powertrain)
A050,6,1 = Front-Wheel-Drive (FWD)
A050,7,2 = All-Wheel-Drive (AWD)
;
A051,0,ESP-Data (Brakes)
A051,1,Brake
A051,5,ESP-Data (Brakes)
A051,6,02 = Front: C54 / Rear: C38 (PR-1LZ+1KD)
A051,7,04 = Front: FN3 15" / Rear: C38 (PR-1LB/1LE+1KD)
A051,8,06 = Front: FN3 16" / Rear: C38 (PR-1LT/1LF+1KP)
A051,9,12 = Front: FNR G60 16" / Rear: CII 41 (PR-1LA/1LC/1LD-1KW)
A051,10,14 = Front: FNR G60 17" / Rear: CII 43 (PR-1LJ+1KE)
A051,11,20 = Front: Brembo M6 19" / Rear: CII 43 (PR-1LU+1KY)
A051,12,22 = Front: Brembo M8 18" / Rear: CII 43 (PR-1LP+1KY or PR-1LV+2EG)
;
A081,0,Learned Values (Vehicle Data)
A081,5,Learned Values (Vehicle Data)
A081,6,To start the process for vehicle data (VIN)
A081,7,learning enter/save 02905 as new value.
;
