;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; VW Bora/Golf/Jetta (1J)
;
; Component: J217 - Automatic Transmission (#02) - 09A
;
; P/n: 09A-927-750-??
;
; includes measuring blocks and coding
;
; created on 26/Mar/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 28/Jan/2011 by Dana Smetanick (Dana@Ross-Tech.com)
; updated on 07/Feb/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 09/Oct/2012
;
; requires VCDS 10.6.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,1,Vehicle Speed,,Display Range: 0...255 km/h
001,2,Transmission,Speed (G182),Display Range: 0...7650 RPM
001,3,Engine Speed,,Display Range: 0...7650 RPM
001,4,Driving Mode
;
002,1,Accelerator,Pedal,Display Range: 0...99 %
002,2,Solenoid,Valve 6 (N93),Display Range: 0...95 %
002,3,ATF Temperature,,Display Range: -40...+170 °C
002,4,Battery Voltage,,Display Range: 0...26 V
;
003,1,Vehicle Speed,,Display Range: 0...255 km/h
003,2,Accelerator,Pedal,Display Range: 0...99 %
003,3,Driving Mode
003,4,Solenoid,Valve 4 (N91),Display Range: 4...94 %
;
004,1,Selector Lever,Position
004,2,Multi-Function,Switch,1xx-xxxx = Tiptronic down (-)\nx1x-xxxx = Shift lever in Tiptronic mode\xx1-xxxx = Tiptronic up (+)\nxxx-1xxx = Multi-function switch 1\nxxx-x1xx = Multi-function switch 2\nxxx-xx1x = Multi-function switch 3\nxxx-xxx1 = Multi-function switch 4\n----1010 = P\n----0010 = R\n----0110 = N\n----0100 = D (Tiptronic)\n----0101 = 4\n----0001 = 3\n----1001 = 2
; 1xx-xxxx = Tiptronic down (-)
; x1x-xxxx = Shift lever in Tiptronic mode
; xx1-xxxx = Tiptronic up (+)
; xxx-1xxx = Multi-function switch 1
; xxx-x1xx = Multi-function switch 2
; xxx-xx1x = Multi-function switch 3
; xxx-xxx1 = Multi-function switch 4
; ----1010 = P
; ----0010 = R
; ----0110 = N
; ----0100 = D (Tiptronic)
; ----0101 = 4
: ----0001 = 3
; ----1001 = 2
004,3,Multi-Function,Switch 3
004,4,Condition of,Solenoid Valves,1xxxxxxx - Solenoid Valve 4 (N91)\nx1xxxxxx - Solenoid Shift Lock\nxx1xxxxx - Solenoid Valve 9 (N282)\nxxx1xxxx - Solenoid Valve 8 (N281)\nxxxx1xxx - Solenoid Valve 3 (N90)\nxxxxx1xx - Solenoid Valve 5 (N92)\nxxxxxx1x - Solenoid Valve 2 (N89)\nxxxxxxx1 - Solenoid Valve 1 (N88)
; 1xxxxxxx - Solenoid Valve 4 (N91)
; x1xxxxxx - Solenoid Shift Lock
; xx1xxxxx - Solenoid Valve 9 (N282)
; xxx1xxxx - Solenoid Valve 8 (N281)
; xxxx1xxx - Solenoid Valve 3 (N90)
; xxxxx1xx - Solenoid Valve 5 (N92)
; xxxxxx1x - Solenoid Valve 2 (N89)
; xxxxxxx1 - Solenoid Valve 1 (N88)
;
005,1,Selector Lever,Position
005,2,Tiptronic Mode,Condition
005,3,Driving Mode
005,4,Multi-Function,Switch,1xx-xxxx = Tiptronic down (-)\nx1x-xxxx = Shift lever in Tiptronic mode\xx1-xxxx = Tiptronic up (+)\nxxx-1xxx = Multi-function switch 1\nxxx-x1xx = Multi-function switch 2\nxxx-xx1x = Multi-function switch 3\nxxx-xxx1 = Multi-function switch 4\n----1010 = P\n----0010 = R\n----0110 = N\n----0100 = D (Tiptronic)\n----0101 = 4\n----0001 = 3\n----1001 = 2
; 1xx-xxxx = Tiptronic down (-)
; x1x-xxxx = Shift lever in Tiptronic mode
; xx1-xxxx = Tiptronic up (+)
; xxx-1xxx = Multi-function switch 1
; xxx-x1xx = Multi-function switch 2
; xxx-xx1x = Multi-function switch 3
; xxx-xxx1 = Multi-function switch 4
; ----1010 = P
; ----0010 = R
; ----0110 = N
; ----0100 = D (Tiptronic)
; ----0101 = 4
: ----0001 = 3
; ----1001 = 2
;
007,1,Engine Speed,,Display Range: 0...7650 RPM
007,2,Transmission,Speed (G182),Display Range: 0...7650 RPM
007,3,Intermediate,Engine Speed,Display Range: 0...7650 RPM
007,4,Vehicle Speed,,Display Range: 0...255 km/h
;
008,1,Accelerator,Pedal,Display Range: 0...99 %
008,2,Main Pressure of,Solenoid Valve,Display Range: 0...95
008,3,Brake Pressure,,Display Range: 0...100
008,4,Driving Mode
;
