;
; VAG-COM label file
;
; Audi TT (8N) / VW Golf/Jetta (1J/9B/9M) / VW New Beetle (1C)
;
; component: Engine (#01) - AWW
;
; p/n: 06A 906 032 ??
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 06-01.LBL
; 8L-01.LBL
; 8N-01.LBL
; 06A-906-032-AWw.LBL (1.8l TE  @ 150 HP - AWW)
;
; based on 06A-906-032.LBL by Andy Smith
; modified to 06A-906-032-HF.LBL by Don Jones (dcjones@ccis.com)
; updated/enhanced to 06A-906-032-AWW.LBL by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 24/Apr/2008
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
001,2,Coolant,Temperature,Specification: 85.0...110.0 °C
001,3,Lambda,Controller,Specification: -10.0...+10.0
001,4,Basic Setting,Requirements,Specification: 1x111111
; xxxxxxx1 - Coolant temperature below 80 °C
; xxxxxx1x - Engine speed below 2000 RPM
; xxxxx1xx - Throttle valve closed
; xxxx1xxx - Lambda regulation correct
; xxx1xxxx - State of idle
; xx1xxxxx - A/C system compressor deactivated
; x1xxxxxx - Catalyst temperature over 350 °C
; 1xxxxxxx - No malfunctions detected
;
002,0,Basic Functions (Mass Air Flow)
002,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
002,2,Engine Load,,Specification: 15.0...25.0 %
002,3,Injection,Timing,Specification: 2.0...4.0 ms
002,4,Intake Air Mass,,Specification: 2.0...4.5 g/s
;
003,0,Basic Functions (Mass Air Flow)
003,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
003,2,Intake Air Mass,,Specification: 2.0...4.5 g/s
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.2....4.0 %
003,4,Ignition,Timing Angle,Specification: 6...12 °BTDC
;
004,0,Basic Functions
004,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
004,2,Voltage Supply,,Specification: 12.0...15.0 V
004,3,Coolant,Temperature,Specification: 60...110 °C
004,4,Intake Air,Temperature,Specification: -48.0...+110.0 °C
;
005,0,Basic Functions
005,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
005,2,Engine Load,,Specification: 15.0...25.0 %
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
006,2,Engine Load,,Specification: 15.0...25.0 %
006,3,Intake Air,Temperature,Specification: -48.0...+110.0 °C
006,4,Altitude,Correction Factor,Specification: -50.0...20.0 %
;
008,0,Basic Functions (Vacuum Pump for Brakes)
008,1,Brake Condition
008,2,Vacuum Pump,Condition
008,3,Vacuum of,Brake Booster
;
010,0,Ignition
010,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
010,2,Engine Load,,Specification: 10.0...25.0 %
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.3...4.0 %
010,4,Ignition,Timing Angle,Specification: 5..15 °BTDC
;
014,0,Ignition (Misfire Recognition)
014,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
014,2,Engine Load,,Specification: 10.0...25.0 %
014,3,Misfire,(total),Specification: 0
014,4,Misfire,recognition,Specification: active | Display Range: active/inactive
;
015,0,Misfire Recognition
015,1,Cylinder 1
015,2,Cylinder 2
015,3,Cylinder 3
015,4,Malfunction,Recognition,Display Range: activated/blocked
;
016,0,Misfire Recognition
016,1,Cylinder 4
016,4,Malfunction,Recognition,Display Range: activated/blocked
;
022,0,Ignition (Knock Control - Cyl 1 && 2)
022,1,Engine Speed,,Specification (manual): 700...6800 RPM | Specification (automatic): 640...6800 RPM
022,2,Engine Load,,Specification: 10.0...150.0 %
022,3,Cylinder 1 Ignition,Angle Delay,Specification: 0.0...12.75 °CA
022,4,Cylinder 2 Ignition,Angle Delay,Specification: 0.0...12.75 °CA
;
023,0,Ignition (Knock Control - Cyl 3 && 4)
023,1,Engine Speed,,Specification (manual): 700...6800 RPM | Specification (automatic): 640...6800 RPM
023,2,Engine Load,,Specification: 10.0...150.0 %
023,3,Cylinder 3 Ignition,Angle Delay,Specification: 0.0...12.75 °CA
023,4,Cylinder 4 Ignition,Angle Delay,Specification: 0.0...12.75 °CA
;
028,0,Knock Sensor Test (Short Trip)
028,1,Engine Speed,,Specification: 2200...6800 RPM
028,2,Engine Load,,Specification: 15.0...175.0 %
028,3,Engine Coolant,Temperature,Specification: 40.0...110.0 °C
028,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,Specification: 111
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
030,2,Bank 1,Sensor 2,Specification: 110
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
;
032,0,Lambda Regulation
032,1,Lambda (Idle),Self-Adaptation,Specification: -10...+10 %
032,2,Lambda (Partial),Self-Adaptation,Specification: -10...+10 %
;
033,0,Lambda Regulation (befor Catalyst)
033,1,Bank 1,Lambda Control,Specification: -10.0...+10.0 %
033,2,Bank 1 Voltage,of Oxygen Sensors,Specification: 0.00...5.00 V
;
034,0,Lambda Regulation (befor Catalyst - Basic Setting: Aging Check)
034,1,Engine Speed,,Specification: 1800...2200 RPM
034,2,Catalytic Converter,Temperature,Specification: 350...500 °C
034,3,Period,Duration Sensor,Specification: 0.5...2.5 s
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK
;
036,0,Lambda Regulation (after Catalyst)
036,1,Bank 1 Sensor 2,Voltage,Specification: 0.10...0.90 V
036,2,Result,Lambda Availability,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK
;
037,0,Lambda Regulation (after Catalyst - Basic Setting)
037,1,Engine Load,,Specification: 10...150.0 %
037,2,Bank 1 Sensor 2,Voltage,Specification: 0.10...0.90 V
037,3,Lambda Regulator,Dwell Period,Specification: -0.02...+0.02 ms
037,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
041,0,Lambda Regulation (Lambda Probe Heating)
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition,,Specification: Htg.bC.ON
041,3,Resistance,Bank 1 Sensor 2,Specification: 0.0...2.0 kOhm
041,4,Heater Condition,,Specification: Htg.aC.ON
;
043,0,Oxygen Sensor Control (Basic Setting: Sensor After Catalyst - Aging Check)
043,1,Engine Speed,,Specification: 1800...2200 RPM
043,2,Catalyst,Temperature,Specification: > 300 °C
043,3,Lambda Sensor,Voltage (B1-S1),Specification: 0.1...0.9 V
043,4,Result,Aging Check,Specification: B1-S2 OK | Display Range: Test OFF/Test ON/B1-S2 OK/B1-S2 nOK
;
046,0,Oxygen Sensor Control (Basic Setting: Catalytic Conversion Test)
046,1,Engine Speed,,Specification: 1800...2200 RPM
046,2,Catalyst,Temperature,Specification: > 440 °C
046,3,Amplitude Ratio,,Specification: 0.00...0.32
046,4,Result,Catalyst Test,Specification: Cat B1 OK | Display Range: Test OFF/Test ON/Cat B1 OK/Cat B1 nOK
;
050,0,Speed Regulation
050,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
050,2,Engine Speed,(specified),Specification (manual): 760 RPM | Specification (automatic): 700 RPM
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
054,0,Speed Regulation
054,1,Engine Speed,,Specification (manual): 700...2520 RPM | Specification (automatic): 640...2520 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Specification: 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed,,Specification: 740...820 RPM
055,2,Idle Regulator,,Specification: -4.30...+12.20 %
055,3,Idle Stabilization,Self-Adaptation,Specification (A/C High): -6.0...+6.0 % | Specification (A/C Low): -3.0...+3.0 %
055,4,Load Status,,see labelfile
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed,,Specification (manual): 700...820 RPM | Specification (automatic): 640...760 RPM
056,2,Engine Speed,(specified),Specification (manual): 760 RPM | Specification (automatic): 700 RPM
056,3,Idle Regulator,,Specification: -4.30...+12.20 %
056,4,Load Status
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on
;
060,0,Speed Regulation (Basic Setting: Throttle Body Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
060,3,Learn Step,Counter,Specification: 0...8
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
061,0,Speed Regulation (EPC)
061,1,Engine Speed,,Specification (manual): 700...6800 RPM | Specification (automatic): 640...6800 RPM
061,2,Voltage Supply,,Specification: 12.0...15.0 V
061,3,Activation Throttle,Position Actuator,G186 (Specification: 0...100 %)
061,4,Operating,Condition
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on
;
062,0,Speed Regulation (Basic Setting: EPC Adaptation)
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
062,3,Throttle Position,Sensor (G79),Specification: 12...97 %
062,4,Accelerator Pedal,Position Sensor 2,G185 (Specification: 0...100 %)
;
063,0,Speed Regulation (Basic Setting: Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79),Display Range: 0...100 %
063,2,Accelerator Pedal,Position Sensor 2,G185 (Specification: 0...100 %)
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP runs/ADP OK/ADP ERROR
;
066,1,Cruise Cntrol System
066,2,Brake switch,clutch and CCS,Specification: 1000
; 1xxx - Cruise control system active
; x1xx - Clutch depressed (always 1 in automatic transmission)
; xx1x - Brake depressed (brake pedal switch)
; xxx1 - Brake depressed (brake light switch)
066,3,Specified Speed
066,4,CCS Control,Positions,Specification: 0000
; 1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; x1xx - SET button pressed
; xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; xxx1 - CCS slide handle on OFF
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve (Open),Specification: 0...100 %
070,2,Lambda Regulator,Deviation,Specification: -7.0...+7.0 %
070,3,Evap. Emissions,Sol. Valve (Flow),Specification: 0.00...0.100 %
070,4,Result,Evap. Emissions,Display Range: Test ON/Test OFF/TEV OK/TEV not OK
;
071,0,Exhaust Reduction (Basic Setting: Leak Diagnostic System)
071,1,Reed Contact,Condition,Display Range: Reed closed/Reed open
071,2,Malfunction Display,,Display Range: minor leak/significant leak/Open circuit
071,3,Diagnostic Status,,Display Range: System test/Measurement end
071,4,Result,Leak Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
077,0,Emission Reduction (Basic Setting: Secondary Air System Diagnostic)
077,1,Engine Speed,,Specification (automatic): 640...760 RPM | Specification (manual): 700...820 RPM
077,2,Mass Air Flow,,Specification: 5.0...12.0 g/s
077,3,Secondary Air,System Air Mass,Specification: -100...+100 %
077,4,Diagnostic,Result,Specification: Sys. OK | Display Range: Test ON/Test OFF/Syst. OK/Syst. nOK
;
089,0,Trip Odometer (MIL On)
089,1,Trip Distance,with MIL on
089,2,Tank empty,,Display Range: OK/too small
;
091,0,Camshaft Adjustment
091,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
091,2,Engine Load,,Specification: 10...150 %
091,3,Camshaft,Adjustment,Display Range: On/Off
091,4,Active camshaft,adjustment angle,Specification: -3.0...+25.0 °CA
;
094,0,Camshaft Adjustment (Basic Setting)
094,1,Engine Speed,,Specification: 1080...2600 RPM
094,2,Camshaft,adjustment,Specification: CAM-ADJ.ON | Display Range: CAM-ADJ.ON/CAM-ADJ.OFF
094,3,Diagnostic,Result,Specification: Syst. OK  | Display Range: Test OFF/Test ON/Syst.OK/Syst. nOK
;
099,0,Oxygen Sensor Control (Basic Setting: Oxygen Sensor Operating Condition)
099,1,Engine Speed,,Specification (automatic): 640...760 RPM | Specification (manual): 700...820 RPM
099,2,Coolant,Temperature,Specification: 80.0...110.0 °C
099,3,Lambda Sensor,Control,Specification: -10.0...+10.0 %
099,4,Lambda Sensor,Condition,Specification: Lambda ON/OFF
;
100,0,Readiness
100,1,Readiness Bits,,see labelfile
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor heater
; xx1xxxxx - Oxygen sensors
; xxx1xxxx - A/C system
; xxxx1xxx - Secondary Air Injection (AIR) system
; xxxxx1xx - Activated charcoal system
; xxxxxx1x - Catalytic converter heater
; xxxxxxx1 - Catalytic converter
100,2,Coolant,Temperature,Specification: 80.0...110.0 °C
100,3,Time since,Engine Start
100,4,OBD-Status,,see labelfile
; 1-xxxxxx - MIL warning lamp on
; x-1xxxxx - Complete distance
; x-x1xxxx - At least one malfunction detected
; x-xx--1x - Heating cycle ended
; x-xx--x1 - Heating cycle not possible
;
107,0,Oxygen Sensor Control (Basic Setting: Diagnostic of Fuel System)
107,1,Engine Speed,,Specification (automatic): 640...760 RPM | Specification (manual): 700...820 RPM
107,2,Oxygen Sensor,Control Bank 1,Specification: -23.0...+23.0 %
107,4,Result,Lambda Control,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
111,0,Charge Pressure Control
111,1,RPM Range 1,,Specification: -15.0...160.0 %
111,2,RPM Range 2,,Specification: -15.0...160.0 %
111,3,RPM Range 3,,Specification: -15.0...160.0 %
111,4,RPM Range 4,,Specification: -15.0...160.0 %
;
113,0,Charge Pressure Control
113,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
113,2,Engine Load,,Specification: 10...150 %
113,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
113,4,Athmospheric,Pressure,Specification: 500...1200 mbar
;
114,0,Charge Pressure Control
114,1,Engine Load,(specified),Specification: < 150.0 %
114,2,Engine Load,(spec. corrected),Specification: < 150.0 %
114,3,Engine Load,(actual Value),Specification: 15.0...150.0 %
114,4,Wastegate (N75),Duty Cycle,Specification: 0...95 %
;
115,0,Charge Pressure Control
115,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
115,2,Engine Load,,Specification: 10...150 %
115,3,Boost Pressure,(specified),Specification : < 1800 mbar
115,4,Boost Pressure,(actual),Specification: < 1800 mbar
;
116,0,Charge Pressure Control
116,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700....6800 RPM
116,2,Fuel Correction,Factor,Specification: -27.0...+0.0 %
116,4,Intake Air,Correction Factor,Specification: -15.0...+7.0 %
;
117,0,Charge Pressure Control
117,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
117,2,Throttle Position,Sensor (G79),Display Range: 0...100 %
117,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
117,4,Boost Pressure,(specified),Specification : < 1800 mbar
;
118,0,Charge Pressure Control
118,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
118,2,Intake Air,Temperature,Specification: < 110.0 °C
118,3,Wastegate (N75),Duty Cycle,Specification: 0...95 %
118,4,Boost Pressure,(actual),Specification: < 1800 mbar
;
119,0,Charge Pressure Control
119,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
119,2,Charge Limit,,Specification: -15...+160 %
119,3,Wastegate (N75),Duty Cycle,Specification: 0...100 %
119,4,Boost Pressure,(actual),Specification: < 1800 mbar
;
120,0,Traction Control (ASR)
120,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
120,2,Engine Load,(specified),Specification: 0...440 Nm
120,3,Engine Load,(actual),Specification: 0...260 Nm
120,4,Status,,Specification: active/not active
;
122,0,Transmission (automatic only)
122,1,Engine Speed,,Specification (automatic): 640...6800 RPM | Specification (manual): 700...6800 RPM
122,2,Engine Load,(specified),Specification: 0...440 Nm
122,3,Engine Load,(actual),Specification: 0...260 Nm
122,4,Status,,Display Range: Engine interv./No engine interv.
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
125,4,A/C Electronics
;
126,0,CAN-Databus Communication (Powertrain)
126,3,Airbag
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,J220 - Engine Electronic (Motronic)
C1,??xxx: Country/Emission
C2,06 - TLEV
C3,07 - LEV
C4, 
C5,xx?xx: Drive/Additional Functions
C6,0 - Front-Wheel-Drive w/o databus
C7,2 - All-Wheel-Drive w/o databus
C8,4 - All-Wheel-Drive w/o traction control and with databus
C9,5 - Front-Wheel-Drive with traction control and databus
C10,6 - All-Wheel-Drive w/o anti-slip and with databus
C11,7 - All-Wheel-Drive with anti-slip and databus
C12, 
C13,xxx?x: Transmission
C14,0 - 5-speed manual transmission
C15,1 - 6-speed manual transmission
C16,3 - automatic transmission (01M)
C17,5 - automatic transmission (09A)
C18, 
C19,xxxx?: Vehicle Type
C20,0 - A-Class (e.g. VW Golf)
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
O,06A-906-032-AWW
;
