;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / VW Eos (1F)
; VW Golf/Jetta (1K/5M) / VW Passat (3C) / VW Touran (1T)
;
; Component: J745 - Cornering Lights Headlight Range Control (#55)
;
; P/N: 5M0-907-357
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 5M-55.LBL
; 5M0-907-357-V1.LBL
; 5M0-907-357-V2.LBL
;
; includes measuring blocks, basic setting, security access, adaptation and coding
;
; created on 17/Dec/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 04/May/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15)
001,2,Light Status,(Terminal 56b),Display Range: ON/OFF
001,3,Vehicle Speed
001,4,Steering Angle,Sensor (G85)
;
B001,0,Adjustment Position && Adjustment Learning
B001,1,Status
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,1,Sensor Signal,Front (G78/G289),Range: 0.0...100.0 %
002,2,Sensor Signal,Rear (G76/G77),Range: 0.0...100.0 %
002,3,Actuator Motor,Left Headlight,Range: 0.0...100.0 %
002,4,Actuator Motor,Right Headlight,Range: 0.0...100.0 %
;
003,0,Cornering Light
003,1,Static Cornering,Light Left
003,2,Static Cornering,Light Right
003,3,Dynamic Cornering,Light Left
003,4,Dynamic Cornering,Light Right
;
004,1,Sensor Signal,Front (G78),Range: 0.0...100.0 %\nSpecification: 12.5...50.0 %
004,2,Sensor Signal,Rear (G76),Range: 0.0...100.0 %\nSpecification: 50.0...87.5 %
004,3,Movement,Front Suspension,Display Range: -127.0...+128.0 mm
004,4,Movement,Rear Suspension,Display Range: -127.0...+128.0 mm
;
005,0,Voltage Supply
005,2,Sensor,Voltage Supply
005,3,Voltage Light,Module Left
005,4,Voltage Light,Module Right
;
006,1,Reverse Gear,engaged,Range: Reverse: No/Reverse: Yes
006,2,Cornering Light,deactived,Range: Yes/No
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,2,CAN-Gateway,(J533),Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
125,3,Power Steering,(J500),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
125,4,Engine,Electronics,Specification: Engine 1\Display Range: Engine 1/Engine 0
;
127,0,CAN-Databus Communication (Light)
127,1,Left Output,Stage (J667),Specification: LeiMo Left 1\nDisplay Range: LeiMo Left 1/LeiMo Left 0
127,2,Right Output,Stage (J668),Specification: LeiMo Right 1\nDisplay Range: LeiMo Right 1/LeiMo Right 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Cornering Lights Headlight Range Control (J745) Coding
C01,0000001 = VW Passat (3C) Left-Hand-Drive / Rest of World
C02,0000003 = VW Eos (1F) Left-Hand-Drive / Rest of World
C03,0000004 = VW Golf/Jetta (1K/5M) Left-Hand-Drive / Rest of World
C04,0000005 = VW Touran (1T) Left-Hand-Drive
C05,0000006 = VW Passat (3C) Right-Hand-Drive / Rest of World
C06,0000007 = VW Passat (3C) Left-Hand-Drive / North America
C07,0000010 = VW Eos (1F) Right-Hand-Drive / Rest of World
C08,0000011 = VW Eos (1F) Left-Hand-Drive / North America
C09,0000012 = VW Golf/Jetta (1K/5M) Right-Hand-Drive / Rest of World
C10,0000013 = VW Golf/Jetta (1K/5M) Left-Hand-Drive / North America
C11,0000014 = VW Touran (1T) Right-Hand-Drive
C12,0000015 = Seat Altea/Toledo (5P) and Leon (1P) Left-Hand-Drive
C13,0000016 = Seat Altea/Toledo (5P) and Leon (1P) Right-Hand-Drive
C14, 
C15,Note: In case an Output Stage is being replaced the Subsystem/Slave
C16,cannot be coded directly. Instead recode the Headlight Aim Control
C17,Module with the current Coding this will also code the Subsystems.
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Cornering Lights Headlight Range Control (J745) Security Access
S01,15284 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Travel/Tourist Mode
A002,5,Travel/Tourist Mode
A002,6,This Setting allows you to switch the Headlights between
A002,7,Left-Hand-Driving (LHD) and Right-Hand-Driving (RHD) when
A002,8,going into a Country which is opposite to what the Car was
A002,9,originally made for. While this Setting is active a Fault
A002,10,Code will be stored and the Indicator Lamp will flash for
A002,11,a short Time after the Ignition is switched on.
A002,12, 
A002,13,0 = Switch-Over for Travel/Tourist Mode NOT active
A002,14,1 = Switch-Over for Travel/Tourist Mode active
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1540,Headlight Range Control: Adjusting to Lowered Position
T1541,Headlight Range Control: Adjusting to Raised Position
T2625,Headlight Range Control: Adjusting to Delivery Position
T2623,Dynamic Cornering Light: Adjusting to Center Position
T2941,Dynamic Cornering Light: Position Left
T2942,Dynamic Cornering Light: Position Right
T2947,Static Cornering Light Left: up/bright
T2948,Static Cornering Light Left: down/dim
T2949,Static Cornering Light Right: up/bright
T2950,Static Cornering Light Right: down/dim
T2952,Control Circuit for Curve Lighting Warning Light
;
