;
; VCDS Label File
;
; Copyright © 2012 Ross-Tech, LLC
;
; Audi 100 (4A)
;
; Component: Engine (#01) - AAE < 02/1992
;
; P/N: 4A0-907-311-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4A-01.LBL
; 048-907-311-AAE1.LBL (2.0l SPI    @ 100 HP - AAE < 02/1992)
;
; includes measuring blocks and basic settings
;
; created on 28/Mar/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 28/Mar/2012
;
; requires VCDS 11.11.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
000,0,General (Decimal Values)
000,1,Coolant Temperature (G62),Range: -48.0...+143.0 °C\nSpecification (Warm): 22...11 (85.0...115.0 °C)
000,2,Throttly Valve Potentiometer (G69),Specification (Idle): 15...70 (1.6...7.6 °)
000,3,Engine Speed (G28),Specification (Idle): 30...40 (750...1000 RPM)
000,4,Intake Air Temperature,Specification: 97...46 (30...60 °C)
000,5,Lambda Control,Specification: 98...158 (fluctuating) / Average: 128
000,9,Supply Voltage,Specification: 170...220 (10.8...14.0 V)
;
B000,0,Idle Stabilization deactivated / Active Charcoal Valve closed
;
