;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; VW Passat (3C)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 3C0-920-???-???
;
; includes measuring blocks, adaptation, coding
;          security access and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3C-17.LBL
; 3C0-920-xxx-17.LBL
;
; created on 29/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Feb/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Display range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Mileage
002,2,Fuel Level,(G)
002,3,Fuel Level,Sender (G),Range: 67.0...278.0 Ohms\n\n~70.0 Ohms = Full Tank\n~270.0 Ohms = Empty Tank
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
003,2,Oil Level,,Range: OK/n.OK
003,3,Oil Temperature
;
004,0,General
004,1,Voltage,(Terminal 30)
;
005,0,Service Reminder
005,1,Service Exceeding,(Distance),in Kilometers (km)
005,2,Service Exceeding,(Time),in Days
005,3,Remaining to,Service (Distance),in Kilometers (km)
005,4,Remaining to,Service (Time),in Days
;
006,0,Service Reminder
006,1,Minimum Oil Level,in Service Interval
006,2,Maximum Oil Level,in Service Interval
006,3,Long Time Avarage,Oil Level Difference
;
007,0,Fuel Level Sender (G) Raw Data
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time,to Service,See Adaptation Channel 049
;
015,0,Adaptation Channel 045
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 045
;
016,0,Adaptation Channels 047 && 048
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 047
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 048
;
050,0,General
050,1,Mileage
050,2,Engine Speed
050,4,Coolant,Temperature
;
060,0,Installation Information I (Senders and Sensors)
;
061,0,Installation Information II (Board Computer Buttons)
;
062,0,Installation Information III (Shift Information)
;
065,0,Installation Information IV (Indicator Lamps)
;
066,0,Installation Information V (Indicator Lamps)
;
067,0,Installation Information VI (Indicator Lamps)
;
068,0,Installation Information VII (Indicator Lamps)
;
090,0,Dimming I
090,1,Dimming,(Terminal 58d)
090,2,Dimming,(Photo Transistor)
;
091,0,Dimming II
;
092,0,Dimming III
;
094,0,Dimming IV
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,,Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,2,Airbag,(J234),Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
126,3,Steering,,Specification: Steering 1\nDisplay Range: Steering 1/Steering 0
;
129,0,CAN-Databus Powertrain (Communication)
129,1,Parking Brake,,Specification: Parking 1\nDisplay Range: Parking 1/Parking 0
;
201,1,Distance Impulse,Number
201,2,Start Impulse,recognized,Display Range: Yes/No
;
202,2,Wheel,Circumference
;
203,1,Failed Logins
203,2,Lock-Time
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Engine
225,2,Transmission
225,3,Brake Electronics
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,CAN-Gateway
226,2,Airbag
226,3,Steering
;
229,0,CAN-Databus Powertrain (Time-Out)
229,1,Parking Brake
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??x05: Options
C02,+01 = Brake Pad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Low Washer Fluid Warning active
C05,00xx?05: Country
C06,1 = Europe (EU)
C07,2 = USA (US)
C08,3 = Canada (CDN)
C09,4 = Great Britain (GB)
C10,5 = Japan (JP)
C11,6 = Arabian States
C12,7 = Australia (AUS)
C13, 
C14,Note: Changing the region section of Coding (from US to UK for example) can
C15,have undesirable effects such as fault codes in ABS and Airbags.
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
;S00,Instrument Cluster (J285) Security Access
;S01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 - German
A004,7,2 - English
A004,8,3 - French
A004,9,4 - Italian
A004,10,5 - Spanish
A004,11,6 - Portuguese
A004,12,7 - Symbols
A004,13,8 - Czech
A004,14,9 - Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
;
A030,0,Tank Characteristic
A030,5,Tank Characteristic
A030,6,Parallel shift of tank characteristic by ± 6 °
A030,7,Standard Value: 128
A030,8,Value Range: 115...140
A030,9,Increments: 1 = 0.5 °
A030,8, 
A030,9,Adaptation should be performed after emptying the tank
A030,10,and filling it with 7 liters of fuel.
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,Standard: 0
A035,11,Range: 0...1000 U/min
A035,12,Increments: 250 U/min
;
A039,0,Oil Level and Temperature Sensor Installation
A039,5,Oil Level and Temperature Sensor Installation
A039,6,Determines if the Oil Level and Temperature Sensor is installed or not.
A039,7,0 = Oil Level and Temperature Sensor not installed
A039,8,1 = Oil Level and Temperature Sensor installed
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km or 1 = 100 mi
A040,7, 
A040,8,NOTE: Adaptation channels 40-49 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-49 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km or 1 = 100 mi
A042,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A042,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A042,9,or (if coded to miles)
A042,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A042,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A042,12, 
A042,13,NOTE: Adaptation channels 40-49 must be
A042,14,entered and stored in the following order:
A042,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km or 1 = 100 mi
A043,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A043,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A043,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A043,12, 
A043,13,NOTE: Adaptation channels 40-49 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 - fixed Service Intervals (w/o Longlife)
A044,8,00730 - flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-49 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 - fixed Service Intervals (w/o Longlife)
A045,7,2 - flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 40-49 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 40-49 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 40-49 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 40-49 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 - fixed Service Intervals (w/o Longlife)
A049,8,00730 - flexible Service Intervals (with Longlife)
A049,9, 
A049,10,NOTE: Adaptation channels 40-49 must be
A049,11,entered and stored in the following order:
A049,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A050,0,Basic Distance Value for Oil Change with fixed Service Interval
A050,5,Basic Distance Value for Oil Change with fixed Service Interval
A050,6,Increments: 1 = 100 km/mi
;
A051,0,Basic Time Value for Oil Change with fixed Service Interval
A051,5,Basic Time Value for Oil Change with fixed Service Interval
A051,6,Increments: 1 = 1 day(s)
A051,7,00372 = fixed Service Intervals (w/o Longlife)
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,100,DIST
RD,43,ST_MADTS,100,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
RD,50,ST_BDOC,100,DIST
RD,51,ST_BTOC,1,ST_D
;
RJ,0,0,General Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Readapt Service Interval to 10.000 mi after 2nd Service (USA only)
RJ,1,1,42,100
RJ,1,2,49,372
RJ,1,3,50,100
RJ,1,4,51,372
RC,1,0,After this Change has been performed VCDS will Display an Error Message but in any
RC,1,1,case the new Values will be correctly saved and the Error Message can be ignored.
;
RJ,2,0,Readapt Service Interval to 15.000 km after 2nd Service (Canada only)
RJ,2,1,42,150
RJ,2,2,49,372
RJ,2,3,50,150
RJ,2,4,51,372
RC,2,0,After this Change has been performed VCDS will Display an Error Message but in any
RC,2,1,case the new Values will be correctly saved and the Error Message can be ignored.
;
RJ,3,0,Change to Fixed Intervals (Kilometers),,
RJ,3,1,45,1
RJ,3,2,42,150
RJ,3,3,43,150
RJ,3,4,44,372
RJ,3,5,49,372
;
RJ,4,0,Change to Flexible Intervals (Kilometers/Diesel),,
RJ,4,1,45,2
RJ,4,2,42,150
RJ,4,3,43,300
RJ,4,4,44,744
RJ,4,5,49,744
;
RJ,5,0,Change to Flexible Intervals (Kilometers/Gasoline),,
RJ,5,1,45,2
RJ,5,2,42,150
RJ,5,3,43,300
RJ,5,4,44,744
RJ,5,5,49,372
;
RJ,6,0,Change to Fixed Intervals (Miles),,
RJ,6,1,45,1
RJ,6,2,42,50
RJ,6,3,43,50
RJ,6,4,44,372
RJ,6,5,49,372
;
RJ,7,0,Change to Flexible Intervals (Miles/Diesel),,
RJ,7,1,45,2
RJ,7,2,42,93
RJ,7,3,43,186
RJ,7,4,44,744
RJ,7,5,49,744
;
RJ,8,0,Change to Flexible Intervals (Miles/Gasoline),,
RJ,8,1,45,2
RJ,8,2,42,93
RJ,8,3,43,186
RJ,8,4,44,744
RJ,8,5,49,372
;
