;
; VCDS Label File
;
; Copyright © 2009-2011 Ross-Tech, LLC
;
; VW Touareg (7L6)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 7L6-920-???-???
;
; includes measuring blocks, coding, adaptation, 
;          selective output test and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7L-17.LBL
; 7L6-920-xxx-7L6.LBL
; 7L6-920-xxx-7LA.LBL
;
; created on 25/Mar/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Aug/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuaring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??xx1: Options
C02,+01 = Brakepad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,00xx?x1: Country
C06,1 = Europe
C07,2 = USA
C08,3 = Canada/Mexico/Latin America
C09,4 = Great Britain (GB)
C10,5 = Japan
C11,6 = Saudi Arabia
C12,7 = Australia
C13,00xxx?1: Service Intervals
C14,0 = All Engines (except 5.0l V10 TDI-Engine)
C15,1 = 5.0l V10 TDI-Engine only
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,IMPORTANT NOTE: If you need to reset the service reminder
A002,10,please use the Automatic Service Reset (under Applications).
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,8 = Czech
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once before
A009,10,the current value is not over 100 km/62 mi.
A009,11,After changing the value can be corrected
A009,12,within the next 5 km/3 mi.
;
A15,0,
;16
A15,1,
;Hour
A15,2,
;N/A
A15,3,
;N/A
A15,4,
;N/A
;
A16,0,
;3
A16,1,
;Minute
A16,2,
;N/A
A16,3,
;N/A
A16,4,
;N/A
;
A17,0,
;2009
A17,1,
;Year
A17,2,
;N/A
A17,3,
;N/A
A17,4,
;N/A
;
A18,0,
;10
A18,1,
;Month
A18,2,
;N/A
A18,3,
;N/A
A18,4,
;N/A
;
A19,0,
;1
A19,1,
;Day
A19,2,
;N/A
A19,3,
;N/A
A19,4,
;N/A
;
;A025,0,
;0
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A030,7, 
A030,8,Standard Value: 128
A030,9,Value Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A38,0,
;ERROR: Security
A38,3,
;access
A38,4,
;required
;
A39,0,
;
A39,1,
;ERROR:
A39,2,
;Security
A39,3,
;access
A39,4,
;required
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km/mi
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km/mi
A042,7,00150 = Standard (15.000 km)
A042,8,or (if coded to miles)
A042,9,00??0 = Standard (??.000 mi)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,00150 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,00300 = flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,11,00??0 = fixed Service Intervals (??.000 mi - w/o Longlife)
A043,13,00??0 = flexible Service Intervals (??.000 mi - with Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 = fixed Service Intervals (w/o Longlife)
A049,8,00365 = Gasoline Engine with flexible Service Intervals (with Longlife)
A049,9,00730 = Diesel Engine with flexible Service Intervals (with Longlife)
;
A050,0,Basic Distance Value for Oil Change with fixed Service Interval
A050,5,Basic Distance Value for Oil Change with fixed Service Interval
A050,6,Increments: 1 = 100 km/mi
A050,7,00150 = 15.000 km (Rest of World/Canada)
A050,8,or (if coded to miles)
A050,9,00090 = 9.000 mi (Great Britain)
A050,9,00160 = 16.000 mi (USA)
;
A051,0,Basic Time Value for Oil Change with fixed Service Interval
A051,5,Basic Time Value for Oil Change with fixed Service Interval
A051,6,Increments: 1 = 1 day(s)
A051,7,00372 = fixed Service Intervals (w/o Longlife)
;
;A060,0,
;0
;
;A061,0,
;5
;
;A062,0,
;5
;
;A063,0,
;5
;
;A064,0,
;10
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T662,Tachometer (G5)
T663,Speedometer (G21)
T664,Fuel Gauge
T499,Vehicle Voltage Display (Y11)
T500,Oil Temperature Display (Y12)
T626,Glow Plug Indicator Light (K29)
T661,Temperature Indicator
T665,Seat Belt Warning Light (K19)
T1047,Brake and Parking Brake Warning Light (K7)
T400,Turn Signal: Acoustic Return Message
T666,Gong
T1023,Buzzer/Chime (H3)
T798,Display: Segment Test
T3079,Display: Test Picture
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,1000,DIST
RD,43,ST_MADTS,1000,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
