;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J518 - Access/Start Authorization (#05)
;
; P/N: 4E0-910-131-???
;
; includes measuring blocks, coding and security access
;
; created on 08/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 07/Mar/2012
;
; requires VCDS 10.6.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Terminal Status
001,1,Status,Terminal 15,Range: Term 15 On/Term 15 Off
001,3,Status,Terminal 75X,Range: ON/OFF
001,4,Status,Terminal 50,Range: Term 50 On/Term 50 Off
;
002,0,Entry and Start Authorisation Buttons
002,1,Start Auth. Button,(E262) START1,Range: ON/OFF
002,2,Start Auth. Button,(E262) START2,Range: ON/OFF
002,3,Start Auth. Button,(E262) STOP1,Range: ON/OFF
002,4,Start Auth. Button,(E262) STOP2,Range: ON/OFF
;
003,0,Electric Ignition Lock (EIL)
003,1,Electric Ignition,Lock Supply Diag.,Range: ON/OFF
003,4,Electric Ignition,Lock Switch
;
004,0,Capacative Sensors
004,1,Capacative Sensor,Drivers Door,Range: Operated/Not Oper.
004,2,Capacative Sensor,Passenger Door,Range: Operated/Not Oper.
004,3,Capacative Sensor,Rear Left Door,Range: Operated/Not Oper.
004,4,Capacative Sensor,Rear Right Door,Range: Operated/Not Oper.
;
005,0,Sender Identification
005,1,Software Version,Current Sender,Version:Week:Year\n00:00:00 = Invalid
;
006,0,Sender Identification (Sender 1 - 4)
; 1xxxxxxx = Battery OK
; x1xxxxxx = Matched
; xx1xxxxx = Disabled
; xxx1xxxx = External Synchronisation
; xxxx1xxx = Rear Lid Release
; xxxxx1xx = Panic Button
; xxxxxx1x = Central Locking Unlock
; xxxxxxx1 = Central Locking Lock
006,1,Identification,Sender 1,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
006,2,Identification,Sender 2,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
006,3,Identification,Sender 3,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
006,4,Identification,Sender 4,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
;
007,2,Radio Signal,Range Reduction,Range: ON/OFF
;
008,0,Capacative Sensor Play Protection
008,1,Remaining Time,Shut-Off Driver
008,2,Remaining Time,Shut-Off Passeng.
008,3,Play Protection,Drivers Door
008,4,Play Protection,Passenger Door
;
009,0,Capacative Sensor Play Protection
009,1,Play Protection,Drivers Door,Range: ON/OFF
009,2,Play Protection,Passenger Door,Range: ON/OFF
009,3,Play Protection,Rear Left Door,Range: ON/OFF
009,4,Play Protection,Rear Right Door,Range: ON/OFF
;
010,1,Manufacturer,Hardware Status
;
021,0,Immobilizer I (Engine Control Unit = ECU Status)
021,1,Start permitted,Slave 1,Specification: Yes\nRange: Yes/No
021,2,ECU responds,Slave 1,Specification: Yes\nRange: Yes/No
021,3,Start permitted,Slave 2,Specification: Yes\nRange: Yes/No
021,4,ECU responds,Slave 2,Specification: Yes\nRange: Yes/No
;
022,0,Immobilizer II
022,1,Engine Start,permitted,Specification: Yes\nRange: Yes/No
022,2,Engine (ECU),responds,Specification: Yes\nRange: Yes/No
022,3,Key Status,OK,Specification: Yes\nRange: Yes/No
022,4,Number of,adapted Keys,Specification: 1...8
;
023,0,Immobilizer III
023,1,Variable Code,authorized,Specification: Yes\nRange: Yes/No
023,2,Key Status,(Transponder Lock),Range: Yes/No
023,3,Fixed Code,authorized,Specification: Yes\nRange: Yes/No
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)\n\n1 = End of Assembly Line: NEW (Delivery Condition of New Instrument Cluster)\n2 = End of Assembly Line: VIN adapted\n3 = End of Assembly Line: ECU adapted\n4 = Customer Service: NEW (Delivery Condition of Replacement Instrument Cluster)\n5 = Customer Service: Instrument Cluster adapted\n6 = Customer Service: Keys adapted (Normal Condition)\n7 = Customer Service: Key Adaptation active
; 1 = End of Assembly Line: NEW (Delivery Condition of New Instrument Cluster)
; 2 = End of Assembly Line: VIN adapted
; 3 = End of Assembly Line: ECU adapted
; 4 = Customer Service: NEW (Delivery Condition of Replacement Instrument Cluster)
; 5 = Customer Service: Instrument Cluster adapted
; 6 = Customer Service: Keys adapted (Normal Condition)
; 7 = Customer Service: Key Adaptation active
;
024,0,Immobilizer IV (Lock Time)
024,1,Login-Lock,Tester,wrong Login (Specification: 0)
024,2,Login-Lock,CAN-Bus,wrong PIN (Specification: 0)
024,3,Lock Time,Scan Protection,Key (Specification: 0)
024,4,Lock Time,after Adaptation,Specification: 0
;
025,0,Immobilizer V (Electric Steering Lock = ESL)
025,1,Electric Steering,Lock Authentication,Range: Valid/Invalid
025,2,Electric Steering,Lock Access,Range: Possible/Impossible
;
026,0,Immobilizer VI (Electric Steering Lock = ESL)
026,1,ESL Login,Lock Time,Specification: 0
026,2,Security Access,Lock Time,Specification: 0
026,3,PP_ESL Inhibit,HighSide
026,4,PP_ESL Inhibit,LowSide
;
050,0,CAN-Messages from Central Electronics (J519)
050,1,Tailgate Lock
050,2,Locked,(internal)
050,3,Locked,(external)
050,4,Safed,(external)
;
051,0,CAN-Messages from Driver's Door Control Unit (J386)
051,1,Driver's Door,Opened,Range: ON/OFF
051,2,Driver's Door,Locked,Range: ON/OFF
051,3,Driver's Door,Safed,Range: ON/OFF
;
052,0,CAN-Messages from Passenger Door Control Unit (J387)
052,1,Passenger Door,Opened,Range: ON/OFF
052,2,Passenger Door,Locked,Range: ON/OFF
052,3,Passenger Door,Safed,Range: ON/OFF
;
053,0,CAN-Messages from Rear Left Door Control Unit (J388)
053,1,Door Rear Left,Opened,Range: ON/OFF
053,2,Door Rear Left,Locked,Range: ON/OFF
053,3,Door Rear Left,Safed,Range: ON/OFF
;
054,0,CAN-Messages from Rear Right Door Control Unit (J389)
054,1,Door Rear Right,Opened,Range: ON/OFF
054,2,Door Rear Right,Locked,Range: ON/OFF
054,3,Door Rear Right,Safed,Range: ON/OFF
;
055,0,CAN-Messages from Door Control Units
055,1,Driver's Door,Opening,Range: 0.0...100.0 %
055,2,Passenger Door,Opening,Range: 0.0...100.0 %
055,3,Door Rear Left,Opening,Range: 0.0...100.0 %
055,4,Door Rear Right,Opening,Range: 0.0...100.0 %
;
056,0,CAN-Messages from Roof Module
056,1,Roof Opening,,Range: 0.0...100.0 %
056,2,Roof installed,,Range: ON/OFF
;
057,1,CAN-Diagnosis 1,Unlearn Counter
057,2,CAN-Diagnosis 1,Error-Bit Mileage
057,3,CAN-Diagnosis 1,Error-Bit Time
;
058,1,CAN-Diagnoses 1,Time/Date
;
059,1,CAN-Diagnoses 1,Mileage,
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Identification Number (VIN) & Serial Number
;
082,0,Advanced Control Module Identification III
;
083,0,Advanced Control Module Identification IV
;
090,0,CAN-Gateway
090,1,Engine 1 Old,,Range: ON/OFF
090,2,Clutch Switch,,Range: ON/OFF
090,3,Brake Light Switch,,Range: ON/OFF
090,4,Brake Test Switch,,Range: ON/OFF
;
091,0,CAN-Gateway
091,1,Vehicle Speed
091,2,Selector Lever,Position
091,3,Brake 1 Old,,Range: ON/OFF
091,4,Gearbox 1 Old,,Range: ON/OFF
;
128,0,Terminals
128,1,Status,Terminal S,Range: ON/OFF
128,3,Status,Terminal P,Range: ON/OFF
;
129,0,Gear Status
129,2,Gear P,,Range: ON/OFF
129,3,Gear PN,,Range: PN Inactive/PN Active
129,4,Digital Switch,Brakes,Range: ON/OFF
;
130,1,Terminal 15,Diagnosis Status,Range: ON/OFF
130,2,Terminal 50,Diagnosis Status,Range: ON/OFF
130,3,Voltage Supply
;
131,1,Voltage Supply,Driver Sensor,Range: ON/OFF
131,2,Voltage Supply,Pass./Rear Sens.,Range: ON/OFF
131,3,Last Trigger,Passive Entry,\n1 = Capacitive Sensor Driver Door\n2 = Capacitive Sensor Front Passenger Door\n3 = Capacitive Sensor Rear Left Door\n4 = Capacitive Sensor Rear Right Door\n5 = Lock Button Driver Door\n6 = Lock Button Front Passenger Door\n7 = Lock Button Rear Left door\n8 = Lock Button Rear Right door\n9 = Door Handle Driver Door pulled\n10 = Door Handle Front Passenger Door pulled\n11 = Door Handle Rear Left Door pulled\n12 = Door Handle Rear Right Door pulled\n13 = Rear Lid/Trunk Release Button\n14 = Rear Lid/Trunk closed\n16 = Lock with RK\n17 = Passive Go\n18 = Event Search\n19 = Passive Go Special Function
;  1 = Capacitive Sensor Driver Door
;  2 = Capacitive Sensor Front Passenger Door
;  3 = Capacitive Sensor Rear Left Door
;  4 = Capacitive Sensor Rear Right Door
;  5 = Lock Button Driver Door
;  6 = Lock Button Front Passenger Door
;  7 = Lock Button Rear Left door
;  8 = Lock Button Rear Right door
;  9 = Door Handle Driver Door pulled
; 10 = Door Handle Front Passenger Door pulled
; 11 = Door Handle Rear Left Door pulled
; 12 = Door Handle Rear Right Door pulled
; 13 = Rear Lid/Trunk Release Button
; 14 = Rear Lid/Trunk closed
; 16 = Lock with RK
; 17 = Passive Go
; 18 = Event Search
; 19 = Passive Go Special Function
;
133,0,Sender Identification (Sender 5 - 8)
; 1xxxxxxx = Battery OK
; x1xxxxxx = Matched
; xx1xxxxx = Disabled
; xxx1xxxx = External Synchronisation
; xxxx1xxx = Rear Lid Release
; xxxxx1xx = Panic Button
; xxxxxx1x = Central Locking Unlock
; xxxxxxx1 = Central Locking Lock
133,1,Identification,Sender 5,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
133,2,Identification,Sender 6,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
133,3,Identification,Sender 7,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
133,4,Identification,Sender 8,1xxxxxxx = Battery OK\nx1xxxxxx = Matched\nxx1xxxxx = Disabled\nxxx1xxxx = External Synchronisation\nxxxx1xxx = Rear Lid Release\nxxxxx1xx = Panic Button\nxxxxxx1x = Central Locking Unlock\nxxxxxxx1 = Central Locking Lock
;
135,0,Key Authentication
135,1,Last Key auth. for,Passive Entry
135,2,Last Key auth. for,Passive Go,Advance Key
135,3,Keys found in last,interior search
135,4,Keys found in last,exterior search
;
136,1,Original,Data Version
136,2,Data Version,altered
136,3,Current,Data Version
;
148,0,Immobilizer
148,1,Start permitted,Slave 3,Specification: Yes\nRange: Yes/No
148,2,ECU responds,Slave 3,Specification: Yes\nRange: Yes/No
148,3,Start permitted,Transmission,Specification: Yes\nRange: Yes/No
148,4,ECU responds,Transmission,Specification: Yes\nRange: Yes/No
;
153,0,Electric Steering Lock (ESL)
153,1,ESL Voltage,Supply LowSide,Range: ON/OFF
153,2,ESL Voltage,Supply HighSide,Range: ON/OFF
153,3,ESL Voltage Supp.,LowSide Diagnos.,Range: ON/OFF
153,4,ESL Voltage Supp.,HighSide Diagnos.,Range: ON/OFF
;
177,0,Intelligent Load Management (ILM)
177,1,ILM Rear 1,Softtouch pressed,Range: ON/OFF
;
178,0,CAN-Messages from Driver's Door Control Unit (J386)
178,1,Driver's Door,Keyswitch Close,Range: ON/OFF
178,2,Driver's Door,Tag Pressed,Range: ON/OFF
178,3,Driver's Door,Lock Button,Range: ON/OFF
;
179,0,CAN-Messages from Passenger Door Control Unit (J387)
179,2,Passenger Door,Tag Pressed,Range: ON/OFF
179,3,Passenger Door,Lock Button,Range: ON/OFF
;
180,0,CAN-Messages from Rear Left Door Control Unit (J388)
180,2,Door Rear Left,Tag Pressed,Range: ON/OFF
180,3,Door Rear Left,Lock Button,Range: ON/OFF
;
181,0,CAN-Messages from Rear Right Door Control Unit (J389)
181,2,Door Rear Right,Tag Pressed,Range: ON/OFF
181,3,Door Rear Right,Lock Button,Range: ON/OFF
;
217,0,CAN-Messages from Gateway (J533)
217,1,Starter enabled,,Range: ON/OFF
217,2,Starter disengage,,Range: ON/OFF
217,3,Engine Speed
217,4,Engine 2 Old,,Range: ON/OFF
;
218,0,CAN-Messages from Gateway (J533) && Battery/Energy Manager
218,1,CAN-Powertrain,Sleep-Ack,Range: ON/OFF
218,2,Shut-Off Stage
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Start/Access Authorization (J518) Coding
C01,+0000512 = Japan/South Korea (Antennas for Reduced Power Transmitters)
C02,+0001024 = Comfort Function: Closing
C03,+0002048 = Right-Hand-Drive (RHD)
C04,+0004096 = 2 Second Trunk Opening Delay (MY 2006+)
C05,+0016384 = Steering Column Lock active with Locking via Remote
C06,+0131072 = Audi Advanced Key
C07,+0262144 = Standard (ALWAYS SET)
;
;
;---------------------------------------------------
;
; login/coding-2
;
;---------------------------------------------------
;
;
L00,Start/Access Authorization (J518) Coding-2
L01,19795 = Coding Enabling
;
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
;S00,Start/Access Authorization (J518) Security Access
;S01,19795 = Coding Enabling
;
