;
; VCDS Label File
;
; Copyright © 2015+ Ross-Tech, LLC
;
; VW T2C/Kombi (7X)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 7X0-920-???-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7X-17.LBL
; 7X0-920-xxx-17.LBL
;
; created on 11/Jun/2015 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 11/Jun/2015
;
; requires VCDS 14.10.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,4,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;Component:A0-KOMBIINSTR. VDO V05 , Coding:01040
;
C00,Instrument Cluster (J285) Coding
;C01,00040 = All Other Engine Variants
C01,01040 = 1.4l MPI/FLEX (BTJ)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
;
;A16,0,
;2015
;;
;
;A17,0,
;2015
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 9 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 108...148 (-5.0...+5.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
