;
; VCDS Label File
;
; Copyright © 2004+ Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J393 - Comfort System (#46)
;
; P/N: 4E0-910-289-???
;
; includes measuring blocks, adaptation, coding and selective output tests
;
; created on 26/Sep/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 04/Jun/2015 by Sebastian Stange (Sebastian@Ross-Tech.com) // Converted Coding added
;
; last modification on 04/Jun/2015
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Status (Driver's Door)
001,1,Door Contact,Switch,Range: Door Open/Door Closed
001,2,Central Locking,Interior Button,Range: Lock/Unlock/Not Oper.
001,3,Lock Feedback,,Range: Locked/Unlocked
001,4,Safe Feedback,,Range: Safe/Not Safe
;
002,0,Status (Passenger Door)
002,1,Door Contact,Switch,Range: Door Open/Door Closed
002,2,Central Locking,Interior Button,Range: Lock/Unlock/Not Oper.
002,3,Lock Feedback,,Range: Locked/Unlocked
002,4,Safe Feedback,,Range: Safe/Not Safe
;
003,0,Status (Rear Left Door)
003,1,Door Contact,Switch,Range: Door Open/Door Closed
003,2,Central Locking,Interior Button,Range: Lock/Unlock/Not Oper.
003,3,Lock Feedback,,Range: Locked/Unlocked
003,4,Safe Feedback,,Range: Safe/Not Safe
;
004,0,Status (Rear Right Door)
004,1,Door Contact,Switch,Range: Door Open/Door Closed
004,2,Central Locking,Interior Button,Range: Lock/Unlock/Not Oper.
004,3,Lock Feedback,,Range: Locked/Unlocked
004,4,Safe Feedback,,Range: Safe/Not Safe
;
005,0,Window Regulators
005,1,Window Regulator,Normalization,Specification: 11111 (0 = Not OK / 1 = OK)\n\n?xxxx = Sunroof\nx?xxx = Front Left\nxx?xx = Front Right\nxxx?x = Rear Left\nxxxx? = Rear Right
005,2,Window Regulator,Thermal Protection,Specification: 000 (0 = Inactive / 1 = Active)\n\n?xxx = Front Left\nx?xx = Front Right\nxx?x = Rear Left\nxxx? = Rear Right
005,3,Interior Monitoring,Button,Range: Operated/Not Oper.
005,4,Inclination Sensor,Button,Range: Operated/Not Oper.
;
006,1,Rear Lid,Remote Switch,Range: Operated/Not Oper.
006,2,Rear Lid,Contact Switch,Range: Lid Open/Lid Closed
006,3,Rear Lid,Softtouch,Range: Operated/Not Oper.
006,4,Rear Lid,Opening Switch,Range: Operated/Not Oper./Not Installed
;
007,1,Window Regulator,Enabling,Range: ON/OFF
007,2,Trunk Light,,Range: ON/OFF
007,3,Fuel Lid,Remote Switch,Range: Operated/Not Oper.
007,4,Rear Lid,Key Switch,Range: Open/Close/Not Oper.
;
008,0,General
008,1,Vehicle Speed
008,2,Engine Speed
008,3,Interior,Temperature
008,4,Fuel Cap,,Range: Recognized/Not Recognized
;
009,1,Status,Terminal S,Range: ON/OFF
009,2,Terminal 15,(Hardware Input),Range: Term. 15 On/Term. 15 Off
009,3,Terminal 15,(CAN Input),Range: Term. 15 On/Term. 15 Off
009,4,Key Number,(KESSY)
;
010,1,Terminal 30,(Right)
010,2,Terminal 30,(Left)
010,3,Rear Window,Heater,Range: R.wn.h.ON/R.wn.h.OFF
010,4,Hood Contact,Switch,Range: Lid Closed/Lid Open
;
011,0,Light Status
011,1,Backup Lights,,Range 0 = OFF / 1 = ON\n\n?x = Left\nx? = Right
011,2,Turn Signals,,Range 0 = OFF / 1 = ON\n\n?x = Left\nx? = Right
011,3,Rear Fog Lights,,Range 0 = OFF / 1 = ON\n\n?x = Left\nx? = Right
011,4,Tail Lights,,Range 0 = OFF / 1 = ON\n\n?x = Left\nx? = Right
;
012,1,Brake Test Switch,,Range 0 = OFF / 1 = ON\n\n?xx = Brake Test Sw. (CAN)\nx?x = Brake Test Sw. (CAN/Term. 54)\nxx? = Brake Test Sw. (Hardware/Term. 54)
012,2,Brake ECD,,Range 0 = OFF / 1 = ON\n\n?x = Brake ECD (Hardware)\nx? = Brake ECD (CAN)
012,3,Brake Lights,,Range 0 = OFF / 1 = ON\n\n?xx = Left\nx?x = Center \nxx? = Right
;
013,1,Rear Window,Shades,Range: ON/OFF/Not Installed
013,2,Trunk,Closing Aid,Range: Locked/Unlocked/Not Installed
;
014,0,Rear Lid Control Module
014,1,Rear Lid,Feedback
; ?xxxxxxx = Rear Lid Movement: Closing
; x?xxxxxx = Rear Lid Movement: Opening
; xx?xxxxx = Rear Lid Position (Binary)
; xxx?xxxx = Rear Lid Position (Binary)
; xxxx?xxx = Rear Lid Position (Binary)
; xxxxx?xx = Rear Lid Position (Binary)
; xxxxxx?x = Rear Lid Closed
; xxxxxxx? = Rear Lid Open
014,2,Rear Lid,System Status
; ?xxxxxxx = Rear Lid Control Module Voltage Supply: Out of Spec.
; x?xxxxxx = Rear Lid Control Module Voltage Supply: Out of Spec.
; xx?xxxxx = Rear Lid Control Module defective
; xxx?xxxx = Rear Lid Control Module defective
; xxxx?xxx = Rear Lid Button defective
; xxxxx?xx = Rear Lid Button defective
; xxxxxx?x = Pinch Protection active
; xxxxxxx? = Rear Lid Button Operated
014,3,Rear Lid,Position,Range: 0.0...100.0 %
;
016,0,Alarm Sources
;  0 = Door Contact Driver's Door
;  1 = Door Contact Passenger Door
;  2 = Door Contact Rear Left
;  3 = Door Contact Rear Right
;  4 = Engine Hood Contact
;  5 = Rear Lid Contact
;  6 = Terminal 15
;  7 = Interior Monitoring
;  8 = Non-Authorized Key (Thatcham)
;  9 = Backup-Horn (Wire Monitoring)
; 10 = Inclination Sensor
; 11 = Door Control Module Driver's Side: Not Connected to Databus
; 12 = Door Control Module Passenger Side: Not Connected to Databus
; 13 = Door Control Module Rear Left: Not Connected to Databus
; 14 = Door Control Module Rear Right: Not Connected to Databus
016,1,Last,Alarm Source
016,2,2nd Last,Alarm Source
016,3,3rd Last,Alarm Source
016,4,4th Last,Alarm Source
;
017,0,Inclination Sensor
017,1,X-Axis,(absolute)
017,2,X-Axis,(difference),only active when armed
017,3,Y-Axis,(absolute)
017,4,Y-Axis,(difference),only active when armed
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Personalization - Key 1
A001,5,Personalization - Key 1
A001,6,+00001 = Passenger Door
A001,7,+00002 = Rear Left Door
A001,8,+00004 = Rear Right Door
A001,9,+00008 = Luggage Compartment
A001,10,+00016 = Drivers Door
A001,11,+00256 = Auto-Lock/Unlock
A001,12,+00512 = Comfort Opening: Front Window Regulators
A001,13,+01024 = Comfort Opening: Rear Window Regulators
A001,14,+02048 = Comfort Opening: Sunroof
A001,15,+04096 = Rear Shades automatically
;
A002,0,Personalization - Key 2
A002,5,Personalization - Key 2
A002,6,+00001 = Passenger Door
A002,7,+00002 = Rear Left Door
A002,8,+00004 = Rear Right Door
A002,9,+00008 = Luggage Compartment
A002,10,+00016 = Drivers Door
A002,11,+00256 = Auto-Lock/Unlock
A002,12,+00512 = Comfort Opening: Front Window Regulators
A002,13,+01024 = Comfort Opening: Rear Window Regulators
A002,14,+02048 = Comfort Opening: Sunroof
A002,15,+04096 = Rear Shades automatically
;
A003,0,Personalization - Key 3
A003,5,Personalization - Key 3
A003,6,+00001 = Passenger Door
A003,7,+00002 = Rear Left Door
A003,8,+00004 = Rear Right Door
A003,9,+00008 = Luggage Compartment
A003,10,+00016 = Drivers Door
A003,11,+00256 = Auto-Lock/Unlock
A003,12,+00512 = Comfort Opening: Front Window Regulators
A003,13,+01024 = Comfort Opening: Rear Window Regulators
A003,14,+02048 = Comfort Opening: Sunroof
A003,15,+04096 = Rear Shades automatically
;
A004,0,Personalization - Key 4
A004,5,Personalization - Key 4
A004,6,+00001 = Passenger Door
A004,7,+00002 = Rear Left Door
A004,8,+00004 = Rear Right Door
A004,9,+00008 = Luggage Compartment
A004,10,+00016 = Drivers Door
A004,11,+00256 = Auto-Lock/Unlock
A004,12,+00512 = Comfort Opening: Front Window Regulators
A004,13,+01024 = Comfort Opening: Rear Window Regulators
A004,14,+02048 = Comfort Opening: Sunroof
A004,15,+04096 = Rear Shades automatically
;
A014,0,Inclination Sensor (Alarm Threshold)
A014,5,Inclination Sensor (Alarm Threshold)
A014,6,200 = 100% = 0.0°
A014,7,180 = 90% = 0.1°
A014,8,160 = 80% = 0.2°
A014,9,140 = 70% = 0.3°
A014,10,120 = 60% = 0.4°
A014,11,100 = 50% = 0.5°
;
A060,0,Personalization
A060,5,Personalization
A060,6,Activates the Settings/Changes in the CAR-Menu (Central Locking/Windows)
A060,7,from the Multi Media Interface (MMI).
;
A061,0,Comfort Functions
A061,5,Comfort Functions
A061,6,+00001 = Comfort Closing: Window Regulators via Remote Control
A061,7,+00002 = Comfort Opening: Window Regulators via Remote Control
A061,8,+00004 = Comfort Closing: Sunroof via Remote Control
A061,9,+00008 = Comfort Opening: Sunroof via Remote Control
A061,10,+00016 = Comfort Closing: Window Regulators via Window Regulator Switch
A061,11,+00032 = Comfort Opening: Window Regulators via Window Regulator Switch
A061,12,+00064 = Comfort Closing: Sunroof via Window Regulator Switch
A061,13,+00128 = Comfort Opening: Sunroof via Window Regulator Switch
A061,14,+00256 = Comfort Closing: Window Regulators via Door Lock
A061,15,+00512 = Comfort Closing: Sunroof via Door Lock
;
A062,0,Central Locking Functions
A062,5,Central Locking Functions
A062,6,+1 - Locking Confirmation (Blink)
A062,7,+2 - Unlocking Confirmation (Blink)
A062,8,+4 - Terminal 87 (USA Logic)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,+0000001 = Alarm Setting: Great Britain/Ireland (10 Tamper Alarms - PR-B09)
C02,+0000002 = Lock Cylinder unlocks electrically (OFF = Unlocked Door only / ON = All doors)
C03,+0000004 = Selective Locking (PR-4K2/4K6/4K7)
C04,+0000008 = Anti-Theft Warning System installed (PR-7AH/7AL)
C05,+0000016 = Inclination Sensor installed (PR-7AL/7AN)
C06,+0000032 = Rear Lid Control Module installed (J605 - PR-4E7/4E9)
C07,+0000064 = Comfort Function via Remote active (PR-A8S+B0A/B0L/B1C/B1P)
C08,+0000128 = Right-Hand-Drive (PR-L0R)
C09,+0000512 = Rear Shades (PR-3Y2/3Y5/3Y8)
C10,+0001024 = Anti-Theft Warning System Confirmation via Horn (PR-A8U)
C11,+0002048 = SAE Rear Lights (PR-A8U)
C12,+0004096 = Footwell Lights (PR-QQ1/QQ3)
C13,+0008192 = No SAFE-Motors (PR-A8U)
C14,+0016384 = Fuel Cap Recognition active (PR-A8S)
C15,+0032768 = Interior Monitoring inactive/not installed (PR-7AL/7AH)
;
;
;---------------------------------------------------
;
; converted coding
; (short coding displayed as long coding for easier modifications)
;
;---------------------------------------------------
;
;
LC,02,0,Alarm Setting: Great Britain/Ireland (10 Tamper Alarms - PR-B09)
LC,02,1,Lock Cylinder unlocks electrically (OFF = Unlocked Door only / ON = All doors)
LC,02,2,Selective Locking (PR-4K2/4K6/4K7)
LC,02,3,Anti-Theft Warning System installed (PR-7AH/7AL)
LC,02,4,Inclination Sensor installed (PR-7AL/7AN)
LC,02,5,Rear Lid Control Module installed (J605 - PR-4E7/4E9)
LC,02,6,Comfort Function via Remote active (PR-A8S+B0A/B0L/B1C/B1P)
LC,02,7,Right-Hand-Drive (PR-L0R)
LC,01,0=,Additional Coding Details can be found in Byte 02!
LC,01,1,Rear Shades (PR-3Y2/3Y5/3Y8)
LC,01,2,Anti-Theft Warning System Confirmation via Horn (PR-A8U)
LC,01,3,SAE Rear Lights (PR-A8U)
LC,01,4,Footwell Lights (PR-QQ1/QQ3)
LC,01,5,No SAFE-Motors (PR-A8U)
LC,01,6,Fuel Cap Recognition active (PR-A8S)
LC,01,7,Interior Monitoring inactive/not installed (PR-7AL/7AH)
LC,00,3=,Coding Details can be found in Byte 01 && Byte 02!
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1134,Alarm Horn (H12)
T42,Left Parking Light (M43)
T43,Right Parking Light (M44)
T987,Left Brake Light (M9)
T988,Right Brake Light (M10)
T1503,3rd Brake Light (M25)
T1501,Rear Left Blinker (M6)
T1505,Rear Right Blinker (M8)
T1502,Rear Left Fog Light (L46)
T1506,Rear Right Fog Light (L47)
T1518,Left Back-Up Light (M16)
T1519,Right Back-Up Light (M17)
T1565,Luggage Compartment Light (W3)
T1696,Rear Left Footwell Light (W45)
T1697,Rear Right Footwell Light (W46)
T1828,Left Tail Light
T1829,Right Tail Light
T1551,Central Locking: Lock
T1223,Central Locking: Unlock
T1148,Central Locking: Safe Activation
T959,Centrol Locking: Safe Indicator Lamp (K133)
T1483,Centrol Locking: Rear Lid Remote Unlocking
T332,Central Locking: Open Tank Flap
T2107,Trunk or Luggage Compartment Opening Motor (V254)
T2106,Rear Window Shade Motor (V91)
T834,Heated Rear Window Activation
;
