;
; VCDS Label File
;
; Copyright © 2007+ Ross-Tech, LLC
;
; Audi A3 (8L) / Audi A4 (8D) / Audi A6 (4B) / Audi A8 (4D)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 4B0-919-283-??? / 8D0-919-283-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8D-76.LBL
; 4B0-919-283.LBL
;
; includes measuring blocks, adaptation and coding
;
; created on 15/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 22/Jul/2014
;
; requires VCDS 11.11.5 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Distance (Rear)
001,1,Rear Left,Sensor (G203),Specification: 10...60 cm (255 cm = no obstacle recognized)
001,2,Rear Left Center,Sensor (G204),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Rear Right Center,Sensor (G205),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,4,Rear Right,Sensor (G206),Specification: 10...60 cm (255 cm = no obstacle recognized)
;
002,0,Resulting Distance / Vehicle Speed && Voltage
002,1,Resulting,Distance Rear,Specification: 0...160 cm (255 cm = no obstacle recognized)
002,2,Vehicle Speed,,Range: 0.0...255.0 km/h
002,3,Confirmation,Sound,Range: Sound Off/Sound On
;
003,0,Input Signals
003,1,Supply Voltage,(Terminal 30)
003,2,Reverese Gear,engaged,Range: Reverse: Yes/Reverse: No
003,3,Trailer hitched,,Range: Trailer: Yes/Trailer: No
;
004,0,Oscillation Time (Rear)
004,1,Rear Left,Sensor (G203)
004,2,Rear Left Center,Sensor (G204)
004,3,Rear Right Center,Sensor (G205)
004,4,Rear Right,Sensor (G206)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,0?xxx: Transmission
C02,0 = Manual Transmission
C03,1 = Automatic Transmission
C04,0x?xx: Confirmation Sound
C05,0 = Reverse Gear Confirmation Sound inactive
C06,1 = Reverse Gear Confirmation Sound active
C07,0xx?x: Chassis
C08,0 = Limousine (Rest of World)
C09,1 = Avant/Wagon (Rest of World)
C10,2 = Limousine (North America)
C11,3 = Avant/Wagon (North America)
C12,4 = S/RS-Variante Limousine (Rest of World)
C13,5 = S/RS-Variante Avant/Wagon (Rest of World)
C14,6 = S/RS-Variante Limousine (North America)
C15,7 = S/RS-Variante Avant/Wagon (North America)
C16,8 = Allroad
C17,0xxx?: Model
C18,3 = Audi A3 (8L)
C19,4 = Audi A4 (8D)
C20,6 = Audi A6 (4B)
C21,8 = Audi A8 (4D)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Rear Buzzer Volume
A001,1,Current Value
A001,5,Rear Buzzer Volume
A001,6,Adaptation of the Rear Warning Buzzer Volume.
A001,7, 
A001,8,Range: 2...7 (quiet...loud)
;
A002,0,Rear Buzzer Frequency
A002,1,Current Value
A002,5,Rear Buzzer Frequency
A002,6,Adaptation of the Rear Warning Buzzer Frequency.
A002,7, 
A002,8,Range: 0...4 (0.5...2 kHz)
;
