;
; VCDS Label File
;
; Copyright © 2014+ Ross-Tech, LLC
;
; VW Transporter/Multivan (7H/7J)
;
; Component: J364 - Parking/Auxiliary Heater (#18)
;
; T/N: 7H0-819-008-??? / 7H0-815-071
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7H-18.LBL
; 7H0-819-008.LBL
;
; includes measuring blocks, basic settings and adaptation
;
; created on 13/Apr/2014 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 01/May/2014
;
; requires VCDS 12.12.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,0,Voltage/Power Supply
001,1,Voltage,(Terminal 30)
001,2,Coolant Temp.,(calculated)
;
B003,0,Heater Start (Customer Service)
; Starts the Auxiliary Heater for a Test
; Deactivation via BS/MVB 002
; Equivalent to Activating the System via CAN
; Maximum Duration 60 Minutes
B001,1,Operating,Status,Range: OFF/Start/Full Load/Partial Load/Ctrl. Pause/After-Run/Malfunction/Locked
B001,2,Coolant Temp.,Aux. Heater (G18)
B001,11,Starts the Auxiliary/Parking Heater for Test/Service Purposes
B001,12,lower on HIGH & Temperature on HIGH
B001,13,Deactivation via Basic Setting in MVB 002!
;
B002,0,Heater or Metering Pump Deactivation
; Deactivates the Heater or Metering Pump after BS/MVB 001
B002,11,Deactivation for Heater/Metering Pump Tests.
;
003,1,Combustion Air,Blower (V6),Range: ON/OFF
003,2,Glow Plug (Q8),Flame Monitoring,Range: ON/OFF
003,3,Metering Pump,(V54),Range: ON/OFF
003,4,Heater Coolant,Shut-Off Valve (N279),Range: ON/OFF
;
004,1,Recirc. Pump,(V55),Range: Pump ON/Pump OFF
;
005,1,Line Filling,performed,Range: 1 = Yes/0 = No
;
006,1,Operating,Status,Range: OFF/Start/Full Load/Partial Load/Ctrl. Pause/After-Run/Malfunction/Locked
006,2,Shut-Off Condit.,Aux. Heater,11111111 = Additional Heater Request active (Activation possible)\n\nxxxxxxx0 = Aux. Heater OFF: Crash Signal\nxxxxxx0x = Aux. Heater OFF: No Request from Climatronic (J255)\nxxxxx0xx = Aux. Heater OFF: Engine NOT running\nxxxx0xxx = Aux. Heater OFF: Coolant Temperature too high\nxxx0xxxx = Aux. Heater OFF: Control Pause (i.e. due to Coolant Temperature)\nxx0xxxxx = Aux. Heater OFF: Ignition OFF (Terminal 15 missing)\nx0xxxxxx = Aux. Heater OFF: Fuel Level Warning active\n0xxxxxxx = Aux. Heater OFF: Fault stored
; 11111111 = Additional Heater Request active (Activation possible)
; xxxxxxx0 = Aux. Heater OFF: Crash Signal
; xxxxxx0x = Aux. Heater OFF: No Request from Climatronic (J255)
; xxxxx0xx = Aux. Heater OFF: Engine NOT running
; xxxx0xxx = Aux. Heater OFF: Coolant Temperature too high
; xxx0xxxx = Aux. Heater OFF: Control Pause (i.e. due to Coolant Temperature)
; xx0xxxxx = Aux. Heater OFF: Ignition OFF (Terminal 15 missing)
; x0xxxxxx = Aux. Heater OFF: Fuel Level Warning active
; 0xxxxxxx = Aux. Heater OFF: Fault stored
006,3,Ambient Temp.,(G17)
006,4,Main Switch,,Range: ON/OFF
;
007,1,Remote Control,Status,Range: ON/OFF/active/inactive
007,2,Combustion,Duration,Full- and Partial Load (in Hours)
007,3,Operating,Duration,Full/Partial Load and Pause (in Hours)
007,4,Pre-Heat or,Start Cycles
;
008,1,Error Counter
008,2,Opeation Time,curr. Heat. Cycle,in Seconds
008,3,Remaining Time,until Shut-Off,in Minutes or Seconds
;
009,1,Glow Plug (Q8),Flame Monitoring,Range: 0.0...100.0 %
009,2,Metering Pump,(V54),Range: 0.0...100.0 %
009,3,Recirc. Pump,(V55),Range: 0.0...100.0 %
009,4,Fresh Air,Blower (V2),Range: ON/OFF
;
010,1,Fuel Type
;
012,1,Heater Coolant,Shut-Off Valve (N279),Range: ON/OFF
012,2,Heater Lock,,Range: ON/OFF
012,3,Low Voltage,Shut-Off,Range: ON/OFF
012,4,Low Voltage,Error Counter,Range: ON/OFF
;
0013,0,Telestart Remote Control I
0013,1,Identification,1st Remote
;
014,0,Telestart Remote Control II
014,1,Identification,2nd Remote
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
082,0,Advanced Control Module Identification III
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A003,0,Heater Unlock
A003,5,Heater Unlock
A003,6,If a Fault Code is detected (i.e. no Flame or Flame extinguished) multiple
A003,7,times without a fully functional run the Heater is being locked.
A003,8, 
A003,9,To unlock the heater save '1' as new Value. The saved Value will
A003,10,immediately reverts back to '0' after Saving/Unlocking the Heater.
;
