;
; VAG-COM Label File
;
; Audi A6 (4F) / Audi A8 (4E) / Audi Q7 (4L)
;
; Component: R36 - Telephone Preperation (#77) PR-9ZF/9ZG/9W5
;
; P/N: 4E0-910-336-???
;      4F0-910-336-???
;
; includes measuring blocks, coding and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4F-77.LBL
; 4E0-910-336.LBL
;
; created on 12/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 28/Nov/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltage
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
;
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
005,0,Input Signals
005,1,Input Signals,,1xxx = Communication to Mobile Phone active\nx1xx = Mobile Phone Switched ON\nxx1x = Mobile Phone inserted\nxxx1 = Push-To-Talk (PTT) Button pressed
;
010,0,Signal Strengths
010,1,Signal Strengths
010,2,Reception,Signal Strengths,Display Range: -113.0...33.0 dBm\n128.0 dBM = No Communication with Mobile Phone
;
011,0,Main Antenna
011,1,Main Antenna
011,2,Main Antenna,Status,Display Range: OK/Short Circuit/Open Circuit/Not Possible
;
014,0,Bluetooth Devices
014,1,Bluetooth Devices
014,2,Connected,Bluetooth Devices
;
019,0,Microphone Input
019,1,Microphone Input,Voltage
019,2,Microphone Input,Status
;
020,0,Connected Bluetooth Devices && Reception Signal Strength
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
133,0,Bluetooth Antenna
133,1,Bluetooth Antenna
133,2,Bluetooth Antenna,Status
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Telephone Preperation (R36) Coding
C01,00?0xx0: MMI System
C02,1 = MMI High
C03,2 = MMI Standard
C04, 
C05,00x0?x0: Installation List
C06,9 = Vehicle with MOST-Databus
C07, 
C08,00x0x?0: Voice Control Language
C09,0 = Voice Control OFF
C10,1 = German (Rest of World)
C11,2 = English (United Kingdom)
C12,3 = French (Rest of World)
C13,4 = Italian (Rest of World)
C14,5 = Spanish (Rest of World)
C15,6 = Spanish (USA)
C16,7 = English (USA)
C17,8 = French (Canada)
C18,9 = Speaker depend Voice Selection
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
A128,0,Volume Output
;
A129,0,Afterrun Time
A129,5,Afterrun Time
A129,6,The time the mobile phone plate is active after "Ignition OFF".
A129,7, 
A129,8,Range: 0...6 (30 Seconds to 30 Minutes)
A129,9,Increments: 1 = 5 Minutes (0 = 30 Seconds)
;
A130,0,Delay Time
A130,5,Delay Time
A130,6,Adjustment of the delay times to compensate the
A130,7,audio component delay and acoustic running times.
A130,8, 
A130,9,Range: 0...12 ms
;
A131,0,Microphone Sensitivity
;
A133,0,Bluetooth
A133,5,Bluetooth
A133,6,0 = Bluetooth OFF
A133,7,1 = Bluetooth ON
;
A134,0,Hands Free Function
A134,5,Hands Free Function
A134,6,0 = Hands-free active while Bluetooth connection is active but without cell phone engaged
A134,7,1 = Hands-free only active with cell phone engaged
;
A135,0,Bluetooth Pass Key
A135,5,Bluetooth Pass Key
A135,6,Set the 4-digit Bluetooth pass key using this channel.
;
