;
; VCDS Label File
;
; Copyright © 2004-2010 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia (1Z)
; VW Caddy (2K) / VW Eos (1F) / VW Golf/Jetta (1K/5M) / VW Touran (1T) / VW Scirocco (13)
;
; Component: J285 - Instrument Cluster (#17)
;
; includes measuring blocks, adaptation, coding, security access,
;          selective output test and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-17.LBL
; 1T-17.LBL
; 1Z-17.LBL
; 2K-17.LBL
; 5P-17.LBL
; 1K-25.LBL
; 1T-25.LBL
; 1Z-25.LBL
; 2K-25.LBL
; 5P-25.LBL
; 1K0-920-xxx-17.LBL
; 1K0-920-xxx-25.LBL
;
; created on 19/Oct/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 30/Sep/2010 by Jille Berends (jjberends@gmail.com)
; updated on 04/Oct/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Feb/2016
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch (0.9 bar)
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level (l)
002,3,Fuel Sender,Resistance
002,4,Ambient,temperature
;
003,0,Coolant and Oil
003,1,Coolant,Temperature
003,2,Oil Level,,Range: OK/n.OK
003,3,Oil Temperature
;
004,0,Voltage supply
004,1,Voltage
;
005,0,Service reminder informations
005,1,Service,timeout
005,2,Service,timeout
005,3,Remaining,distance
005,4,Remaining,time
;
006,0,Service reminder informations (oil) [SI = service interval]
006,1,Min. oil,in last SI
006,2,Max. oil,in last SI
006,3,Long Time,avarage,Oil level difference
;
007,0,Fuel Gauge
007,1,Fuel Gauge 1,Resistance
007,2,Fuel Gauge 1,Pad Resistance
007,3,Fuel Gauge 2,Resistance,All-Wheel-Drive (AWD) only
007,4,Fuel Gauge 2,Pad Resistance,All-Wheel-Drive (AWD) only
;
012,0,Mileage/Days since last service
012,1,Adaptation,channel
012,2,Mileage,since service
012,3,Adaptation,channel
012,4,Days,since service
;
013,0,Mileage minimum/maximum (Service reminder limit)
013,1,Adaptation,channel
013,2,Mileage,minimum
013,3,Adaptation,channel
013,4,Mileage,maximum
;
014,0,Days minimum/maximum (Service reminder limit)
014,1,Adaptation,channel
014,2,Maximum,in days
014,3,Adaptation,channel
014,4,Minimum,in days
;
015,0,Oil quality
015,1,Adaptation,channel
015,2,Oil quality
;
016,0,Soot quantity && thermal load
016,1,Adaptation,channel
016,2,Soot quantity
016,3,Adaptation,channel
016,4,Thermal,load
;
50,0,Misc
50,1,Odometer
50,2,Engine Speed
50,3,Oil,temperature
50,4,Coolant,temperature
;
60,0,Installation Information I
60,1,Installation,Information
60,2,Installation,Information
60,3,Installation,Information
;
061,0,Installation Information II
061,1,MFA/MFD,Buttons
;
062,0,Installation Information III
062,1,Installation,Information
;
065,0,Installation Information IV
065,1,Installation,Information
;
066,0,Installation Information V
066,1,Installation,Information
;
067,0,Installation Information VI
067,1,Installation,Information
;
068,0,Installation Information VII
068,1,Installation,Information
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
082,0,Advanced Control Module Identification III
082,1,Advanced,Identification III
;
125,0,CAN-Databus Powertrain
125,1,Engine,electronics,no Display/0/1/S
125,3,Brake,electronics,no Display/0/1/S
;
126,0,CAN-Databus Powertrain
126,1,CAN-Gateway,,no Display/0/1/S
126,2,Airbag,,no Display/0/1
126,3,Steering,Assistant,no Display/0/1/S
;
201,1,Distance Impulse,Number
;
202,2,Wheel,Circumference
;
203,0,Immobilizer
203,1,Login,Failed attempts
203,2,Remaining,Lock Time
;
205,0,Fuel Gauge
205,1,Fuel Gauge 1
205,2,Fuel Gauge 2,,All-Wheel-Drive (AWD) only
;
221,0,Service Interval date VI
221,1,Service Interval,in theory
221,2,Years of driving
221,3,Short-term average Filling level difference
221,4,Total filling level
;
222,0,Service Interval date VII
222,1,Max. lower limit Service interval, in 100km
222,2,Max. upper limit Service interval, in 100km
222,3,Max. lower limit Service interval, in days
222,4,Max. upper limit Service interval, in days
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Motor electronics
225,2,Drivetrain
225,3,Brake-electronics
;
226,0,CAN-Databus Powertrain (Timeout)
226,1,CAN-Gateway
226,2,Airbagsystem
226,3,Steering assistance
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T663,Speedometer (G21)
T662,Tachometer (G5)
T664,Fuel Gauge
T661,Temperature Indicator
T754,Coolant Temperature Warning
T798,Display: Segment Test
T3079,Display: Test Sequence/Picture
T400,Blinker Signal (Acoustic)
T666,Chime/Buzzer/Gong
T1023,Buzzer/Gong/Chime (H3)
T755,Oil Pressure Warning Light (K3)
T501,Oil Level Warning Light (K38)
T1047,Brake and Parking Brake Warning Light (K7)
T1046,Brake Pad Warning Light (K32)
T1082,Fuel Reserve Warning Light (K105)
T502,Immobilizer Warning Light (K115)
T665,Seat Belt Warning Light (K19)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
;S00,Instrument Cluster (J285) Security Access
;S01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language (Error Messages and Navigation)
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,7 = Symbols (No Text)
A004,13,8 = Czech
A004,14,9 = Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once before
A009,10,the current value is not over 100 km/62 mi.
A009,11,After changing the value can be corrected
A009,12,within the next 5 km/3 mi.
;
A15,0,Time Setup (Hour)
;
A16,0,Time Setup (Minute)
;
A022,0,Production Mode
A022,5,Production Mode
A022,6,When Production Mode is active "Pro" is shown in the MFA/MFD
A022,7,and/or the blue High Beam Light flashes. Production Mode can
A022,8,only be deactivated once and not be activated again.
A022,9, 
A022,10,0 = Production Mode NOT active
A022,11,1 = Production Mode active
;
A025,0,Seatbelt Warning
A025,1,Seatbelt Warning
A025,6,0 = Variant 2
A025,7,1 = Variant 3 (icon shows and goes off again after some time)
;
A30,0,Fuel gauge adaptation
A30,1,Current,value
A30,5,Fuel gauge adaptation
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-49 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-49 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 100 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-48 must be
A42,9,entered and stored in the following order:
A42,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 100 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-48 must be
A43,9,entered and stored in the following order:
A43,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-49 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 40-49 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 40-49 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 40-49 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 40-49 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 - fixed Service Intervals (w/o Longlife)
A049,8,00365 - Gasoline Engine with flexible Service Intervals (with Longlife)
A049,9,00730 - Diesel Engine with flexible Service Intervals (with Longlife)
A049,10, 
A049,11,NOTE: Adaptation channels 40-49 must be
A049,12,entered and stored in the following order:
A049,13,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A050,0,Basic Distance Value for Oil Change with fixed Service Interval
A050,5,Basic Distance Value for Oil Change with fixed Service Interval
A050,6,Increments: 1 = 100 km/mi
;
A051,0,Basic Time Value for Oil Change with fixed Service Interval
A051,5,Basic Time Value for Oil Change with fixed Service Interval
A051,6,Increments: 1 = 1 day(s)
A051,7,00372 = fixed Service Intervals (w/o Longlife)
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??x0x: Options
C02,+00 = No Options
C03,+01 = Brake Pad Warning
C04,+02 = Seatbelt Warning
C05,+04 = Washer Fluid Warning
C06,+16 = Sedan (only VW Jetta)
C07,00xx?0x: Country
C08,1 = Europe (EU) / 2 = USA (US)
C09,3 = Canada (CDN) / 4 = Great Britain (GB)
C10,5 = Japan (JP) / 6 = Saudi Arabia (SA)
C11,7 = Australia (AUS)
C12,00xxx0?: Distance Impulse Number
C13,1 = 22188 / 2 = 22076
C14,3 = 21960 / 4 = 21848
C15,5 = 22304 / 6 = 22420
C16,7 = 22532
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,100,DIST
RD,43,ST_MADTS,100,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
RD,50,ST_BDOC,100,DIST
RD,51,ST_BTOC,1,ST_D
;
RJ,0,0,General Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Readapt Service Interval to 10.000 mi after 2nd Service (USA only)
RJ,1,1,42,100
RJ,1,2,49,372
RJ,1,3,50,100
RJ,1,4,51,372
RC,1,0,After this Change has been performed VCDS will Display an Error Message but in any
RC,1,1,case the new Values will be correctly saved and the Error Message can be ignored.
;
RJ,2,0,Readapt Service Interval to 15.000 km after 2nd Service (Canada only)
RJ,2,1,42,150
RJ,2,2,49,372
RJ,2,3,50,150
RJ,2,4,51,372
RC,2,0,After this Change has been performed VCDS will Display an Error Message but in any
RC,2,1,case the new Values will be correctly saved and the Error Message can be ignored.
;
RJ,3,0,Change to Fixed Intervals (Kilometers),,
RJ,3,1,45,1
RJ,3,2,42,150
RJ,3,3,43,150
RJ,3,4,44,372
RJ,3,5,49,372
;
RJ,4,0,Change to Flexible Intervals (Kilometers/Diesel),,
RJ,4,1,45,2
RJ,4,2,42,150
RJ,4,3,43,300
RJ,4,4,44,744
RJ,4,5,49,744
;
RJ,5,0,Change to Flexible Intervals (Kilometers/Gasoline),,
RJ,5,1,45,2
RJ,5,2,42,150
RJ,5,3,43,300
RJ,5,4,44,744
RJ,5,5,49,372
;
RJ,6,0,Change to Fixed Intervals (Miles),,
RJ,6,1,45,1
RJ,6,2,42,50
RJ,6,3,43,50
RJ,6,4,44,372
RJ,6,5,49,372
;
RJ,7,0,Change to Flexible Intervals (Miles/Diesel),,
RJ,7,1,45,2
RJ,7,2,42,93
RJ,7,3,43,186
RJ,7,4,44,744
RJ,7,5,49,744
;
RJ,8,0,Change to Flexible Intervals (Miles/Gasoline),,
RJ,8,1,45,2
RJ,8,2,42,93
RJ,8,3,43,186
RJ,8,4,44,744
RJ,8,5,49,372
;
