;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi A6 (4F)
;
; Component: J525 - Sound System (#47) - Bose
;
; P/N: 4L0-910-223-???
;
; includes measuring blocks, coding, adaptation and selective output test
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4F-47.LBL
; 4L0-910-223-BO.LBL
; 4L0-910-223-ST.LBL
; 4L0-910-7xx-47.LBL
;
; created on 30/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 20/Jan/2011
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltages
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,0000xxx1 = Term. S active\n0000xx1x = Term. 15 active\n0000x1xx = Term. X active\n00001xxx = Term. 50 active
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
002,4,Send Diode,Temperature
;
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,1,Temperature,Analog Circuit
004,2,Temperature,Digital Circuit
004,3,Fan Speed
004,4,Switch/Mute Status,(via Databus)
;     100,Temperature,
;
005,1,Voltage,Microphone 1
005,2,Voltage,Microphone 2
005,3,Voltage,Analog Input
005,4,Vehicle Speed
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Sound System (J525/Bose) Coding
C01,00000?x: Microphone
C02,1 = 1 Microphone for Volume Control
C03,2 = 2 Microphones for Volume and Voice Control
C04,4 = 1 Microphone for Volume Control and Analog Input (AUX)
C05,5 = 2 Microphones for Volume and Voice Control and Analog Input (AUX)
C06, 
C07,00000x?: Equipment
C08,1 = Right-Hand-Drive with Fabric Trim and Diesel Engine
C09,2 = Left-Hand-Drive with Leather Trim and Diesel Engine
C10,3 = Right-Hand-Drive with Leather Trim and Diesel Engine
C11,4 = Left-Hand-Drive with Fabric Trim and Petrol Engine
C12,5 = Right-Hand-Drive with Fabric Trim and Petrol Engine
C13,6 = Left-Hand-Drive with Leather Trim and Petrol Engine
C14,7 = Right-Hand-Drive with Leather Trim and Petrol Engine
C15,8 = Left-Hand-Drive with Fabric Trim and Diesel Engine
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
; See Adaptation Channels 112, 113, 114, 115 & 116 for further Details.
;
T870,Bass Speaker Front Left (R21)
T871,Bass Speaker Front Right (R23)
T874,Treble Speaker Front Left (R20)
T875,Treble Speaker Front Right (R22)
T876,Treble Speaker Rear Left (R14)
T877,Treble Speaker Rear Right (R16)
T2246,Center Midrang/Treble Speaker (R158)
T2558,Rear Left Midrange/Woofer Loudspeaker (R159)
T2559,Rear Right Midtange/Woofer Loudspeaker (R160)
T419,Midrange Speaker Front Left (R103)
T420,Midrange Speaker Front Right (R104)
T3044,Midrange Speaker Rear Left (R105)
T3045,Midrange Speaker Rear Right (R106)
T2247,Subwoofer (R148)
T1609,Cooling Fan in Control Module
;
