;
; VAG-COM label file 3D0-919-146.lbl
;
; VW Phaeton (3D)
; VW Bentley Continental GT (3W)
;
; component: TV Tuner (R78) (#57)
;
;       p/n: 3D0 919 146  Component: TV Tuner H07 1205  Coding: as shown below (Same PN for Phaeton or Bentley Continental GT)
;
;
; created by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; updated by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 23/September/2005 (Michael)
; - remark added at top and bottom of coding
; - additional PN and component information added above, Bentley information added
; last modification: 16/October/2005 (Michael) MVBs added
; last modification: 23/November/2005 (Michael) MVB 004/3 corrected.
; last modification: 23/September/2006 (Michael) MVB 006/1 and 2 corrected.
:                    Thanks to Niels Ezerman for reporting the error.
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;NOTE - normally these codes are changed by the driver, from the Front Information Display and Control Module. 
;It should not be necessary to use a VAG-COM to change the codes, although it can be done that way if desired.
;
C00,Phaeton (3D) - TV Tuner (R78) Coding
C01,00010  Central Europe	PAL B/G 
C02,00020  Italy		PAL B/G 
C03,00030  England,Ireland	PAL I 
C04,00040  Eastern Europe	SECAM D/K 
C05,00110  Eastern Europe	PAL D/K 
C06,00050  France		SECAM L 
C07,00060  North America    	NTSC M 
C08,00070  Australia		PAL B/H 
C09,00080  Brazil		PAL M 
C10,00090  Argentina		PAL M 
C11,00100  New Zealand		PAL B 
C12,00120  China		PAL D/K 
C13,00130  Africa		PAL I 
C14,00150  Africa     		SECAM K1 
C15,00140  Greece or Egypt	SECAM D/K 
C16,00160  Japan          	NTSC M
;
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
001,1,Monitor 2,Status,Possible Display:On or Off
001,2,Term 30,voltage,Possible Display:Between 6 and 15 volts
;
002,1,TV Antenna,number 1,
002,2,TV Antenna,number 1,Possible Display:OK - Kurzschl. - Unterbr.
002,3,TV Antenna,number 2,
002,4,TV Antenna,number 2,Possible Display:OK - Kurzschl. - Unterbr.
;
003,1,TV Antenna,number 3,
003,2,TV Antenna,number 3,Possible Display:OK - Kurzschl. - Unterbr.
003,3,TV Antenna,number 4,
003,4,TV Antenna,number 4,Possible Display:OK - Kurzschl. - Unterbr.
;
004,3,Navigation,connection,Possible Display:OK - Kurzschl. - Unterbr.
;
006,1,External,Input AV1,Possible Display:AV1 in use/ AV1 open
;
006,2,External,Input AV2,Possible Display:AV2 in use/ AV2 open