;
; VAG-COM Label File
;
; VW Golf/Jetta (1J/9M) / VW Passat (3B)
;
; Component: R - Radio (#56) - MFD
;
; includes measuring blocks and coding
;
; created on 22/Feb/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 22/Feb/2007
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,GALA-Signal,,0 = Signal not recognized\n1 = Signal recognized
001,2,Supply Voltage,(Terminal 30)
001,3,Illumination,(Terminal 58d)
001,4,Status,S-Contact,Range: ON/OFF
;
002,0,Speakers
002,1,Speakers,Front
002,2,Status,,Specification: OK/Short/Open
002,3,Speakers,Rear
002,4,Status,,Specification: OK/Short/Open
;
003,0,Antenna
003,1,Antenna Type,,Range: Active/Passive
003,2,Antenna
003,3,Status,,Range: OK/Short/Open
;
004,0,Amplifier / Telephone-Mute
004,1,Amplifier,Output,Range: 0 = OK / 1 = Short to Ground
004,3,Telephone,Mute
004,4,Mute Status,,Range: ON/OFF
;
005,0,CD-Player/Changer
005,1,Component
005,2,Status,,Range: OK/n.OK
;
006,0,External Display
006,1,Component
006,2,Status,,Range: OK/n.OK
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,??xxx: Sound-Adjustment
C02,00 = Standard/Other / 01 = Golf (1J)
C03,02 = Bora/Jetta (1J/9M) / 03 = Golf/Bora Variant/Wagon (1J) 
C04,04 = Passat Sedan (3B) / 05 = Passat Variant/Wagon (3B)
C05,06 = Lupo/Polo (6X/9N) / 07 = Golf-Cabriolet (1E)
C06,08 = Sharan (7M) & New Beetle (1C)
C07,09 = Transporter/Caravelle/Multivan/Eurovan (7D)
C08,xx?xx: Speakers
C09,0 = No passive Speakers (Sound System)
C10,2 = 2 passive Speakers (Front)
C11,3 = 2 passive Speakers (Rear)
C12,4 = 4 passive Speakers (Front and Rear)
C13,xxx?x: Sound System Correction
C14,0 = Sound System not installed (No Correction)
C15,1 = Sound System (Bose) installed
C16,2 = Sound-System (DSP) installed
C17,xxxx?: Configuration
C18,+1 = Active/Remote Supplied Antenna
C19,+2 = CD-Player/Changer
C20,+4 = Secondary Display (Instrument Cluster)
;
