;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A6 (4B)
;
; Component: J234 - Airbag (#15) - AIRBAG 8.4
;
; P/N: 4B0-959-655-???
;
; includes measuring blocks and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4B-15.LBL
; 4B0-959-655-AI7.LBL
; 4B0-959-655-AI8.LBL
; 4B0-959-655-AI84.LBL
;
; created on 30/Apr/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 10/Mar/2015
;
; requires VCDS 14.10.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Igniter Status (Airbag && Tensioner)
001,1,Driver Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Passenger Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Driver Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Passenger Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Igniter Status (Tensioner && Battery Disconnect)
002,1,Rear Left Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Rear Right Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Rear Center Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Battery Disconnect,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,1,Voltage supply,,Display Range: Correct/Signal too Low/Signal too High
003,2,Seat Occupation,Detection Passenger,Display Range: Child Seat/Light Adult/Medium Adult/Heavy Adult/Not Occup./Short to Ground/Short to Plus/Not Installed
003,3,Belt Inquiry,Driver,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Passenger,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry (Rear)
004,1,Belt Inquiry,Rear Left,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Right,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
006,0,Igniter Status (Side Airbag)
006,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,3,Rear Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,4,Rear Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
008,0,Igniter Status (Head Airbag)
008,3,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
008,4,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
009,0,Key Switch Status
009,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Airbag 8.4 (J234) Coding
C01,Standard: Front Airbags/Front Belt Tensioners
C02,Note: New/Replacement Modules MUST use the Service Coding Values!
C03, 
C04,0?x0x: Key Switch for Pass. Airbag Deactivation
C05,0 = Pass. Airbag Deactivation Switch NOT installed
C06,1 = Pass. Airbag Deactivation Switch installed
C07,0x?0x: Side & Curtain/Head Airbags
C08,0 = No Side AND/OR Curtain/Head Airbags
C09,1 = Front Side Airbags
C10,2 = Front Side Airbags & Rear Side Airbags (Factory)
C11,3 = Front Side Airbags & Curtain/Head Airbags (Factory)
C12,4 = Front Side Airbags & Rear Side Airbags & Curtain/Head Airbags (Factory)
C13,5 = Front Side Airbags & Rear Side Airbags (Service)
C14,6 = Front Side Airbags & Curtain/Head Airbags (Service)
C15,7 = Front Side Airbags & Rear Side Airbags & Curtain/Head Airbags (Service)
C16,0xx0?: Rear Belt Tensioners
C17,4 = 2 Rear Belt Tensioners (Rest of World)
C18,5 = 2 Rear Belt Tensioners (North America)
C19,6 = 3 Rear Belt Tensioners (Rest of World)
C20,7 = 3 Rear Belt Tensioners (North America)
;
