;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; Audi A3 (8P) / Audi A4 (8EC/8ED) / Audi A6 (4F) / Audi A8 (4E)
; Audi Q7 (4L) / Audi TT (8J) / Seat Exeo (3R)
;
; Component: J431 - Headlight Range (#55)
;
; P/N: 4F0-910-357-??? / 4L0-910-357-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4L-55.LBL
; 4F0-910-357.LBL
;
; includes measuring blocks, basic setting, adaptation, coding, security access and selective output tests
;
; created on 11/Jul/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 14/Apr/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15)
001,2,Time Constant
001,3,Vehicle,Acceleration
;
B001,0,Adjustment Position && Adjustment Learning
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Sensors
002,1,Front,Sensor Signal
002,2,Rear,Sensor Signal
002,3,PWM Sensors,Voltage Supply
;
003,0,CAN Signals I
003,1,Light,(Terminal 56b)
003,2,Vehicle Speed
003,3,Steering Angle,(CAN Signal)
003,4,Engine Status,(CAN Signal)
;
004,0,CAN Signals II
004,1,Left Light,(CAN Signal)
004,2,Right Light,(CAN Signal)
004,3,Brake Switch,(CAN Signal)
004,4,Back-Up Light,(CAN Signal)
;
005,0,Specified Positions
005,1,Headlight,Range Control
005,2,Dynamic Cornering,Left Light
005,3,Dynamic Cornering,Right Light
;
007,0,Positions && Malfunctions
007,1,Position,Left Adjuster
007,2,Position,Right Adjuster
007,3,Malfunction,Left Module
007,4,Malfunction,Right Module
;
008,1,Operation,(Left/Right)
008,2,Comm. Status,Left Module
008,3,Comm. Status,Right Module
;
009,0,Readiness Bit's
009,1,Readiness Bit,Left AFS Module
009,2,Readiness Bit,Right AFS Module
009,3,Readiness Bit,Control Module
009,4,Readiness Bit,CAN-Powertrain
;
010,0,Additional Functions
010,1,Brake Function,,Range: enabled/disabled
010,2,Highway Function,,Range: enabled/disabled
010,3,Schowroom Effect,,Range: enabled/disabled
;
011,0,Sensor Values
011,1,Front,Sensor Value
011,2,Rear,Sensor Value
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Brake Electronics,(J104),Specification: ABS 1\nRange: ABS 1/ABS 0
125,2,CAN-Gateway,(J533),Specification: Gateway 1\nRange: Gateway 1/Gateway 0
125,3,Power Steering,(J500),Specification: Steer. ang. 1\nRange: Steer. ang. 1/Steer. ang. 0
125,4,Engine,Electronics,Specification: Engine 1\nRange: Engine 1/Engine 0
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Level Control,System (J197)
126,2,Start/Access,Control (J518)
;
225,0,Electro Magnetic Compatibility (EMC) Counter
225,1,Brake Electronics,(J104),Specification: 0
225,2,CAN-Gateway,(J533),Specification: 0
225,3,Power Steering,(J500),Specification: 0
225,4,Engine,Electronics,Specification: 0
;
226,0,Electro Magnetic Compatibility (EMC) Counter
226,1,Level Control,System (J197),Specification: 0
226,2,Start/Access,Control (J518),Specification: 0
;
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Headlight Range Control (J431) Coding
C01,0000016 = Audi A6 (4F) with Steel Suspension (AFS1/PR-8Q5)
C02,0000017 = Audi A6 (4F) with Air Suspension (AFS1/PR-8Q5)
C03,0000018 = Audi A8 (4E)
C04,0000019 = Audi A4 (8E) & Audi A4 Cabriolet (8H)
C05,0000020 = Audi A3 (8P) with Steel Suspension
C06,0000021 = Audi Q7 (4L) with Steel Suspension
C07,0000022 = Audi Q7 (4L) with Air Suspension
C08,0000023 = Audi TT (8J) with Steel Suspension and Front Wheel Drive (FWD)
C09,0000024 = Audi TT (8J) with Steel Suspension and All Wheel Drive (AWD)
C10,0000025 = Audi TT (8J) with Magnetic Ride
C11,0000026 = Audi A6 (4F) with Steel Suspension (AFS2/PR-8Q6)
C12,0000027 = Audi A6 (4F) with Air Suspension (AFS2/PR-8Q6)
C13,0000028 = Audi A3 (8P) Cabriolet
C14,0000029 = Audi A3 (8P) with Magnetic Ride
C15,0000030 = Seat Exeo (3R)
C16,0000031 = Audi Q7 (4L) with Steel Suspension (AFS2/PR-8Q7)
C17,0000032 = Audi Q7 (4L) with Air Suspension (AFS2/PR-8Q7)
C18, 
C19,Note: Perform Security Access before Coding!
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1540,Headlight Range Control: Adjusting to Lowered Position
T1541,Headlight Range Control: Adjusting to Raised Position
T2625,Headlight Range Control: Adjusting to Delivery Position
T2632,Headlight Range Control: Adjusting to Specified Position
T2621,Dynamic Cornering Light: Adjusting to Outer Position
T2622,Dynamic Cornering Light: Adjusting to Inner Position
T2623,Dynamic Cornering Light: Adjusting to Center Position
T2624,Dynamic Cornering Light: Adjusting to Steering Angle Dependent Position
T2237,Stationary Cornering Lamp
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Headlight Range Control (J431) Security Access
S01,02000 = General Coding "Enabling"
S02,02000 > 03000 > 04000 > 05000 = General Adaptation "Enabling" (Enter one after another)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Unknown
A001,5,Unknown
A001,6,Standard: 0
;
A002,0,Unknown
A002,5,Unknown
A002,6,Standard: 2
;
A003,0,Unknown
A003,5,Unknown
A003,6,Standard: 1
;
A004,0,Unknown
A004,5,Unknown
A004,6,Standard: 0
;
A005,0,Unknown
A005,5,Unknown
A005,6,Standard: 1
;
A006,0,Unknown
A006,5,Unknown
A006,6,Standard: 2
;
A007,0,Unknown
A007,5,Unknown
A007,6,Standard: 16
;
A008,0,Unknown
A008,5,Unknown
A008,6,Standard: 1
;
A009,0,Unknown
A009,5,Unknown
A009,6,Standard: 0
;
A011,0,Unknown
A011,5,Unknown
A011,6,Standard: 0
;
A012,0,Unknown
A012,5,Unknown
A012,6,Standard: 0
;
A013,0,Unknown
A013,5,Unknown
A013,6,Standard: 3
;
A014,0,Unknown
A014,5,Unknown
A014,6,Standard: 5
;
A015,0,Unknown
A015,5,Unknown
A015,6,Standard: 0
;
A016,0,Unknown
A016,5,Unknown
A016,6,Standard: 1
;
A017,0,Unknown
A017,5,Unknown
A017,6,Standard: 0
;
A018,0,Unknown
A018,5,Unknown
A018,6,Standard: 0
;
A018,0,Unknown
A018,5,Unknown
A018,6,Standard: 8
;
A019,0,Unknown
A019,5,Unknown
A019,6,Standard: 0
;
A020,0,Showroom Effect
A020,5,Showroom Effect
A020,6,After activating the showroom effect the dynamic cornering light
A020,7,at vehicle standstill can be demonstrated to the customer.
A020,8,The showroom effect remains active until the showroom effect
A020,9,is deactivated via the function program.
A020,10, 
A020,11,0 = Disabled
A020,12,1 = Enabled
;
A021,0,Unknown
A021,5,Unknown
A021,6,Standard: 20
;
A022,0,Unknown
A022,5,Unknown
A022,6,Standard: 0
;
A023,0,Tourist Solution
A023,5,Tourist Solution
A023,6,When driving in countries where driving is performed on the
A023,7,opposite side as in the native country the headlights must
A023,8,be changed over to avoid blinding the oncoming traffic.
A023,9, 
A023,10,0 = Disabled
A023,11,1 = Enabled
;
