;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A6 (4F)
;
; Component: J644 - Battery Regulation (#61)
;
; P/N: 4F0-910-181-???
;
; includes measuring blocks and selective output tests
;
; created on 30/Jun/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 30/Aug/2016
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Generator Voltage,(specified)
001,2,Battery Voltage,(actual)
001,3,Dynamic-Field,Signal
001,4,Load,Response Time,Display Range: 0...9 sec
;
002,0,Battery Temperatures && Shut-Off Stages
002,1,Rail Temperature,(actual)
002,2,Battery Temp.,(valuation)
002,3,Emergency,Shut-Off
002,4,Static-Current,Shut-Off Stage
;
003,0,Battery Status I
003,1,Battery Condition,,same as MMI
003,2,Internal Battery,Resistance
003,3,Qv,(Battery Aging)
;
004,0,Battery Status II
004,1,Current Value,from Battery,Display Range: -400...+100 A\n\npositive current = generator charges battery\nnegative current = battery not charged by generator
004,2,Static-Current,Mean Value,Display Range: 0.01...1.00 A (mean value of all static-current measurements)
004,3,Total Energy,Balance,Display Range: -10000...55025 Ah
004,4,Total Energy,Throughput,Display Range: 0...65025 Ah
;
005,0,Last Standing Time && Last Driving Cycle I
005,1,Static-Current,Mean Value
005,2,Total-Current,Mean Value
005,3,Duration last,Standing Time
005,4,Duration last,Driving Cycle
;
006,0,Last Standing Time && Last Driving Cycle II
006,1,Duration last,Standing Time,with increased static-current (higher than 20 mA)
006,2,Energy Balance,of last Drive,Display Range: -120.00...+120.00 Ah
006,3,Battery State,of Charge (SOC)
;
010,0,Generator
010,1,Generator Voltage,(specified)
010,2,Dynamic-Field,Signal,Generator excitation
010,3,Generator,Interface,Display Range: OK/not OK
010,4,Generator,,Display Range: OK/not OK
;
;
;---------------------------------------------------
;
; selective output tests
;
;---------------------------------------------------
;
;
T2374,Generator: Specified Generator Voltage 15.0 V
T2375,Generator: Specified Generator Voltage 13.5 V
T2376,Generator: Specified Generator Voltage 0.0 V (No Excitation)
;
