;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Audi A6 (4F)
;
; Component: J525 - Sound System (#47) - 6-Channel DSP
;
; P/N: 4F0-910-223-???
;
; includes measuring blocks and coding
;
; created on 01/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 01/Dec/2005
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltages
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,0000xxx1 = Terminal S active\n0000xx1x = Terminal 15 active\n0000x1xx = Terminal X active\n00001xxx = Terminal 50 active
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
002,4,Send Diode,Temperature
;
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,1,Send Diode,Temperature
004,2,Switch & Mute,Status,x1x = Lock SET\nxx0 = Muting OFF
004,3,Vehicle Speed
;
005,0,Microphones
005,1,Voltage,Microphone 1
005,2,Voltage,Microphone 2
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Sound System (J525) Coding
C01,0000xx?: Equipment
C02,1 = Right-Hand-Drive with Fabric Trim and Diesel Engine
C03,2 = Left-Hand-Drive with Leather Trim and Diesel Engine
C04,3 = Right-Hand-Drive with Leather Trim and Diesel Engine
C05,4 = Left-Hand-Drive with Fabric Trim and Petrol Engine
C06,5 = Right-Hand-Drive with Fabric Trim and Petrol Engine
C07,6 = Left-Hand-Drive with Leather Trim and Petrol Engine
C08,7 = Right-Hand-Drive with Leather Trim and Petrol Engine
C09,8 = Left-Hand-Drive with Fabric Trim and Diesel Engine (Standard)
C10,0000x?x: Microphone
C11,0 = Microphone not installed
C12,1 = Microphone for Voice Control
C13,0000?xx: Chassis
C14,0 = Limousine (Sedan)
C15,1 = Avant (Wagon)
;
