;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; VW Touareg (7L)
;
; Component: J393 - Central Module Comfort System (#46)
;
; P/N: 7L0-959-933-???
;
; includes measuring blocks, adaptation and coding
;
; created on 19/Nov/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 29/May/2015 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 29/May/2015
;
; requires VCDS 804.0 or higher
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Driver's Door
001,1,WR-Button (E40),Driver Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
001,2,Window Regulator,Therm. Prot. (V147),Range: Yes/No
001,3,Driver Door,Lock Butt. (E308),Range: Not Oper./Locking/Unlocking/Implausible
001,4,Driver Door Outside,Lock Butt. (E369),Range: Not Oper./Operated/Not Installed
;
002,0,Window Regulator Buttons (Driver Door)
002,1,WR-Button (E81),Passenger Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
002,2,WR-Button (E53),Rear Left Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
002,3,WR-Button (E55),Rear Right Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
;
003,1,Driver Door,Key Switch,Range: Not Oper./Open/Close/Implausible
003,2,Interior Door,Hand Button,Range: Not Oper./Operated
003,3,Outside Door,Hand Button,Range: Not Oper./Operated
;
004,1,Driver Child,Safety Lock Switch,Range: Range: Not Oper./Operated/Not Installed
4,2,,,
;ubetjent, ,
004,3,Rear Left Child,Safety Lock Status,Range: Yes/No/Not Installed
004,4,Rear Right Child,Safety Lock Status,Range: Yes/No/Not Installed
;
005,0,Mirror Adjustment/Heating
005,1,Mirror Adjustment,Switch (E43),Range: Pos X+/Pos X-/Pos Y+/Pos Y-/Not Oper./Not Installed
005,2,Mirror Selector,Switch (E48),Range: Left/Right/Not Oper.
005,3,Mirror Heater,Switch (E231),Range: ON/OFF/Not Installed
;
006,0,Defrost Buttons
006,1,Driver Door,Defrost Button,Range: Not Installed
006,2,Passenger Door,Defrost Button,Range: Not Installed
;
007,0,Passenger Door
007,1,WR-Button (E107),Passenger Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
007,2,Window Regulator,Therm. Prot. (V148),Range: Yes/No
007,3,Lock Butt. (E309),Passenger Door,Range: Not Oper./Locking/Unlocking/Implausible
007,4,Passenger Outside,Lock Butt. (E370),Range: Not Oper./Operated/Not Installed
;
008,0,Rear Left Door
008,1,WR-Button (E52),Rear Left Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
008,2,Window Regulator,Therm. Prot. (V26),Range: Yes/No
008,3,Lock Butt. (E310),Rear Left Door,Range: Not Oper./Locking/Unlocking/Implausible
008,4,Rear Left Outside,Lock Butt. (E371),Range: Not Oper./Operated/Not Installed
;
009,0,Rear Right Door
009,1,WR-Button (E54),Rear Right Door,Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
009,2,Window Regulator,Therm. Prot. (V27),Range: Yes/No
009,3,Lock Butt. (E311),Rear Right Door,Range: Not Oper./Locking/Unlocking/Implausible
009,4,Right Left Outside,Lock Butt. (E372),Range: Not Oper./Operated/Not Installed
;
010,0,Central Locking Units
010,1,Driver Door,Status (F220),Range: Locked/Unlocked/Safe/Implausible
010,2,Passenger Door,Status (F221),Range: Locked/Unlocked/Safe/Implausible
010,3,Rear Left Door,Status (F222),Range: Locked/Unlocked/Safe/Implausible
010,4,Rear Right Door,Status (F223),Range: Locked/Unlocked/Safe/Implausible
;
011,0,Door Contact Switches
011,1,Driver Door,Door Contact (F2),Range: Door Closed/Door Open
011,2,Passenger Door,Door Contact (F3),Range: Door Closed/Door Open
011,3,Rear Left Door,Door Contact (F10),Range: Door Closed/Door Open
011,4,Rear Right Door,Door Contact (F11),Range: Door Closed/Door Open
;
12,0,,
12,1,,,
; 1 1 1  ,Bin. Bits,
;
013,1,Voltage,(Terminal 30),Specification: 9.0...14.5 V
013,2,Ignition,(Terminal 15),Range: Term 15 On/Term 15 Off
013,3,S-Contact,,Range: Activated
013,4,Vehicle Speed
;
014,1,Central Locking,Thermal Protection,Range: Yes/No
014,2,Hood Contact,Switch (F120),Range: Open/Closed
014,3,Brake Light,Switch (F45),Range: ON/OFF
014,4,Databus,Condition,Specification: 2-Wire\nRange: 1-Wire/2-Wire
;
015,0,CAN-Datenbus (Communication)
015,1,Control Module,Driver Door
015,2,Control Module,Passenger Door
015,3,Control Module,Rear Left Door
015,4,Control Module,Rear Right Door
;
16,0,,
16,1,,,
;Not Installed, ,
16,2,,,
;Not Oper., ,
016,3,Rear Lid Handle,Unlock Sw. (E234),Range: Open/Closed
016,4,Rear Lid Lock Unit,(F256),Range: Open/Closed
;
017,1,Remote Control,Buttons,Range: 0 = Not Operated / 1 = Operated\n\n?xxx = Open\nx?xx = Close\nxx?x = Rear Lid\nxxx? = Panic (USA only)
017,2,Immobilizer,Key Recognition,Range: Yes/No
017,3,Rear Lid,Opening Request,Range: Yes/No
017,4,
;OFF, ,
;
018,0,Alarm Sources
;   1 = Driver Door Rotary Switch
;   2 = Passenger Door Rotary Switch
;   3 = Rear Left Door Rotary Switch
;   4 = Rear Right Door Rotary Switch
;   5 = Rear Lid Rotary Switch
;   6 = Hood Contact Switch
;   7 = Ignition (Terminal 15)
;   8 = Interior Monitoring
;   9 = Tire Puncture/Theft (Front Left)
;  10 = Tire Puncture/Theft (Front Right)
;  11 = Tire Puncture/Theft (Rear Left)
;  12 = Tire Puncture/Theft (Rear Right)
;  13 = Tire Puncture/Theft (Spare)
;  14 = Inclination Sensor
;  15 = Backup Horn/Siren
;  16 = Immobilizer
;  17 = Trailer
; 255 = No Alarm
018,1,1st Alarm Source
018,2,2nd Alarm Source
018,3,3rd Alarm Source
018,4,4th Alarm Source
;
019,1,Parking Light,(Terminal 58),Range (Request): ON/OFF
019,3,Parking Light,Left,Range (Request): ON/OFF
019,4,Parking Light,Right,Range (Request): ON/OFF
;
020,1,Rear Fog Light,(Terminal 83b),Range (Request): ON/OFF
020,2,Back-Up Lights,,Range (Request): ON/OFF
020,3,Luminescence,Plate,Range (Return Message): Yes/No
;
021,1,Left Tail Light,(M4),Range: ON/OFF
021,2,Right Tail Light,(M5),Range: ON/OFF
021,3,License Plate,Light (X),Range: ON/OFF
021,4,Rear Fog Lights,(L46/L47),Range: ON/OFF
;
022,1,Left Brake Light,(M9),Range: ON/OFF
022,2,Right Brake Light,(M10),Range: ON/OFF
022,3,High Brake Light,(M25),Range: ON/OFF
022,4,Back-Up Lights,(M16/M17),Range: ON/OFF
;
023,1,Rear Ambient,Illumination,Range: 0.0...100.0 %
023,2,Trunk,Illumination,Range: 0.0...100.0 %
023,3,Rear Light,Reserve Operation,Range: Yes/No
023,4,Trailer,attached,Range: Yes/No/No Commun.
;
024,1,Rear Window,Heating Request,Range: Yes/No
024,2,Rear Window,Heating Relay,Range: ON/OFF
024,4,Open Tank Lid,Request,Range: Yes/No
;
025,1,Comfort Function,,Range: Not Oper./Yes/No
025,2,Sunroof,Enabling,Range: Yes/No
025,3,Sunroof Control,,Range: Not Oper./Open/Close
;
026,0,Rear Windshield
026,1,Rear Wind. (E361),Opening Button,Range: Not Oper./Operated/Not Installed
026,2,Rear Wind. (V312),Unlocking Unit,Range: Open/Closed/Not Installed
026,3,Rear Windshield,Unlocking,Range: ON/OFF
;
027,0,Rear Windshield
027,1,Rear Windsh. Req.,Wiper Interval,Range: Yes/No
027,2,Rear Windsh. Req.,Wipe/Wash Funct.,Range: Yes/No
027,3,Rear Windsh. Act.,Wiper Interval,Range: ON/OFF
027,4,Rear Windsh. Act.,Wipe/Wash Funct.,Range: ON/OFF
;
028,0,Spare Wheel Holder
028,1,Spare Wheel,Unlock Button,Range: Operated/Not Oper./Not Installed
028,2,Spare Wheel,Rotary Trap,Range: Open/Closed/Not Installed
028,3,Spare Wheel,Position Switch,Range: Enganged/Disenganged/Not Installed
028,4,Spare Wheel,Unlocking,Range: Unlocked/Inactive/Not Installed
;
029,0,Rear Lid Closing Assist
029,1,Rear Lid,Closing Assist,Range: ON/OFF/Not Installed
029,2,Rear Lid,Position Switch,Range: Open/Close/Not Installed
029,3,Thermal Protection,Closing Assist,Range: Yes/No/Not Installed
029,4,Thermal Protection,Spare Wheel,Range: Yes/No/Not Installed
;
030,0,Vehicle Inclination Sensor (G384) I
030,1,Inclination Sensor,Status,Range: active/inactive
030,2,Inclination Sensor,Alarm Recognized,Range: Yes/No/Not Installed
030,3,Inclin. Sensor (E360),,Deactivation Switch,Range: Operated/Not Oper./Not Installed
;
031,0,Vehicle Inclination Sensor (G384) II
031,1,Inclination Sensor,Supply Voltage,Range: 0.0...19.0 V\nSpecification: 9.0...14.5 V
;
032,0,Vehicle Inclination Sensor (G384) III
032,1,Curent,Alarm Angle,Specification: -25.0...+25.0 °\nRange: No Value/Not Installed
;
033,0,Vehicle Inclination Sensor (G384) IV
33,1,,,
;Not Installed, ,
33,2,,,
;Not Installed, ,
33,3,,,
;Not Installed, ,
33,4,,,
;Not Installed, ,
;
034,0,Interior Monitoring Sensor (G273)
034,1,Interior Monitoring,Status,Range: active/inactive
034,2,Interior Monitoring,Alarm Recognized,Range: Yes/No/Not Installed
034,3,Inter. Monit. (E267),Deactivation Switch,Range: Operated/Not Oper./Not Installed
;
035,0,Interior Monitoring Sensor (G273)
035,1,Interior Monitoring,Supply Voltage,Range: 0.0...19.0 V\nSpecification: 9.0...14.5 V
035,2,Signal,Terminal 15,Range: Term. 15 ON/Term. 15 OFF
035,3,Interior Monitoring,Alarm Stored,Range: Yes/No/Not Installed
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,0000065 = Standard/Base Value
C02, 
C03,+0000004 = Rear Lid Closing Aid
C04,+0000016 = Sun Roof
C05, 
C06,Note: The coding is the some of the standard/base value and the possible options.
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Selective (Single) Door Locking
A001,3,Current Status
A001,5,Selective (Single) Door Locking
A001,6,0 = All Door Locking
A001,7,1 = Selective (Single) Door Locking
;
A002,0,Auto-Lock
A002,1,Auto-Lock
A002,3,Current Status
A002,5,Auto-Lock
A002,6,The doors will lock automatically when the
A002,7,vehicle reaches a speed of 15 km/h or 10 mph.
A002,8, 
A002,9,Range: 0 = OFF / 1 = ON
;
A003,0,Auto-Unlock
A003,1,Auto-Unlock
A003,3,Current Status
A003,5,Auto-Unlock
A003,6,The doors will unlock automatically when
A003,7,the key is removed from the ignition switch.
A003,8, 
A003,9,Range: 0 = OFF / 1 = ON
;
A005,0,Unlocking Confirmation (Remote Control)
A005,1,Unlocking,Confirmation
A005,2,via,Remote Control
A005,3,Current Status
A005,5,Unlocking Confirmation (Remote Control)
A005,6,Type of confirmation when unlocking
A005,7,the car via remote control.
A005,8, 
A005,9,0 = OFF
A005,10,1 = Blink
A005,11,2 = Beep (Horn)
A005,12,3 = Beep (Horn) & Blink
;
A006,0,Unlocking Confirmation (Key Switch)
A006,1,Unlocking,Confirmation
A006,2,via,Key Switch
A006,3,Current Status
A006,5,Unlocking Confirmation (Key Switch)
A006,6,Type of confirmation when unlocking
A006,7,the car via key switch.
A006,8, 
A006,9,0 = OFF
A006,10,1 = Blink
A006,11,2 = Beep (Horn)
A006,12,3 = Beep (Horn) & Blink
;
A008,0,Locking Confirmation (Remote Control)
A008,1,Locking,Confirmation
A008,2,via,Remote Control
A008,3,Current Status
A008,5,Locking Confirmation (Remote Control)
A008,6,Type of confirmation when locking
A008,7,the car via remote control.
A008,8, 
A008,9,0 = OFF
A008,10,1 = Blink
A008,11,2 = Beep (Horn)
A008,12,3 = Beep (Horn) & Blink
;
A009,0,Locking Confirmation (Key Switch)
A009,1,Locking,Confirmation
A009,2,via,Key Switch
A009,3,Current Status
A009,5,Locking Confirmation (Key Switch)
A009,6,Type of confirmation when locking
A009,7,the car via key switch.
A009,8, 
A009,9,0 = OFF
A009,10,1 = Blink
A009,11,2 = Beep (Horn)
A009,12,3 = Beep (Horn) & Blink
;
A025,0,Comfort Operation (via Remote Control)
A025,1,Comfort Operation
A025,2,Remote Control
A025,3,Current Status
A025,5,Comfort Function (via Remote Control)
A025,6,Enables/Disables the Comfort Operation for
A025,7,Power Windows and Sun Roff via Remote Control.
A025,8, 
A025,9,Range: 0 = OFF / 1 = ON
;
A26,0,Anti-Theft Alarm Delay
A26,5,Anti-Theft Alarm Delay
A26,6,Deactivation of the Anti-Theft Alarm Delay when
A26,7,opening Drivers Door before the Alarm will sound.
A26,8, 
A26,9,Range: 0 = OFF / 1 = ON
;
;A27,0,
;2
;A27,1,
;Heckdeckel
;A27,2,
;Taster
;A27,3,
;Auto-Lock /
;A27,4,
;alte
;
