;
; VCDS Label File
;
; Copyright © 2008-2009 Ross-Tech, LLC
;
; VW Touareg (7LA)
;
; Component: J104 - Brake Electronics (#03) - MK25
;
; P/N: 7L0-907-379-???
;
; includes measuring blocks, basic setting and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 7L-03.LBL
; 7L0-907-379-MK25.LBL   (MK25)
; 7L0-907-379-MK25E1.LBL (MK25E1)
;
; created on 15/Feb/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 11/Dec/2015
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Brake System Bleeding
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Starting Wheel Speed
002,1,Speed Sensor,Front Left (G47),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,2,Speed Sensor,Front Right (G45),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,3,Speed Sensor,Rear Left (G46),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,4,Speed Sensor,Rear Right (G44),Range: 0.0...254.0 km/h (255.0 km/h = standing)
;
003,0,Switches and Warning Lights
003,1,Brake Light,Switch (F),Range: Not Oper./Operated
003,2,Brake System,Warning L. (K118),Range: ON/OFF
003,3,ABS,Warning L. (K47),Range: ON/OFF
003,4,ASR/ESP,Warning L. (K155),Range: ON/OFF
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±2.0 °
004,2,Lateral Acc.,Sensor (G200),Specification: ± 1.5 m/s²
004,3,Rotation Rate,,Specification: ± 2.5 °/s
;
005,0,Brake Pressure
005,1,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
;
006,0,Longitudinal Acceleration (G251)
006,1,Longitudinal Acc.,Sensor (G251),Specification: ± 1.5 m/s²
;
007,0,Brake Pedal Path
007,1,Pedal Path,(Not Corrected)
007,2,Pedal Path,(Corrected)
007,3,Pedal Path,(Offset)
;
011,0,Speed Encoder Errors (Front Left)
011,1,Encoder Errors,(G47) Minimum
011,2,Encoder Errors,(G47) Maximum
011,3,Encoder Errors,(G47) Average
;
012,0,Speed Encoder Errors (Front Right)
012,1,Encoder Errors,(G45) Minimum
012,2,Encoder Errors,(G45) Maximum
012,3,Encoder Errors,(G45) Average
;
013,0,Speed Encoder Errors (Rear Left)
013,1,Encoder Errors,(G46) Minimum
013,2,Encoder Errors,(G46) Maximum
013,3,Encoder Errors,(G46) Average
;
014,0,Speed Encoder Errors (Rear Right)
014,1,Encoder Errors,(G44) Minimum
014,2,Encoder Errors,(G44) Maximum
014,3,Encoder Errors,(G44) Average
;
B060,0,Adjustment of Steering Angle Sensor (G85)
B060,1,Adjustment
B060,2,Adjustment,Status
B060,3,Steering Angle,Sensor (G85)
;
B063,0,Adjustment of Lateral Acceleration Sensor (G200)
B063,1,Adjustment
B063,2,Adjustment,Status
B063,3,Lateral Acc.,Sensor (G200)
;
B066,0,Adjustment of Brake Pressure Sensor (G201)
B066,1,Adjustment
B066,2,Adjustment,Status
B066,3,Brake Pressure,Sensor (G201)
;
B069,0,Adjustment of Longitudinal Acceleration Sensor (G251)
B069,1,Adjustment
B069,2,Adjustment,Status
B069,3,Long. Accel.,Sensor (G251)
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Electronics,,Specification: Engine 1\nRange: Engine 1/Engine 0
125,2,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nRange: Steer. ang. 1/Steer. ang. 0
125,3,All-Wheel-Drive,,Specification: AWD 1\nRange: AWD 1/AWD 0
125,4,Transmission,,Specification: Transm. 1\nRange: Transm. 1/Transm. 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Instrument Cluster,,Specification: Instruments 1\nRange: Instruments 1/Instruments 0
126,2,CAN-Gateway,,Specification: Gateway 1\nRange: Gateway 1/Gateway 0
126,3,Level Control,,Specification: Level 1\nRange: Level 1/Level 0
;
127,0,CAN-Databus Powertrain (Communication)
127,1,Damper Control,,Specification: Damper Ctrl 1\nRange: Damper Ctrl 1/Damper Ctrl 0
127,2,Lock Electronics,,Specification: Lock-El. 1\nRange: Lock-El. 1/Lock-El. 0
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Engine Electronics,,Range: Engine 1/Engine 0
225,2,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0
225,3,All-Wheel-Drive,,Range: AWD 1/AWD 0
225,4,Transmission,,Range: Transm. 1/Transm. 0
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,Instrument Cluster,,Range: Instruments 1/Instruments 0
226,2,CAN-Gateway,,Range: Gateway 1/Gateway 0
226,3,Level Control,,Range: Level 1/Level 0
;
227,0,CAN-Databus Powertrain (Time-Out)
227,1,Damper Control,,Range: Damper Ctrl 1/Damper Ctrl 0
227,2,Lock Electronics,,Range: Lock-El. 1/Lock-El. 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
C01,Model:
C02,+0000001 = Touareg (Through Part Number Index D)
C03,+0000002 = Touareg (From Part Number Index E)
C04,Brakes:
C05,+0000000 = 16" Front Disc Brake (PR-1LB)
C06,+0008192 = 17" Front Disc Brake (PR-1LC/1LD/1LE)
C07,+0016384 = 18" Front Disc Brake (PR-1LF)
C08,Suspension:
C09,+0000000 = Standard Springs/Shocks (PR-1BA/1BE)
C10,+0000128 = 4-Corner Air Suspension (PR-1BS/2BK)
C11,+0000256 = 4-Corner Air Suspension with electr. regluated Shocks (PR-1BK)
C12,Transmission:
C13,+0006144 = Automatic & Manual Transmission (Through Part Number Index C)
C14,+0004096 = Manual Transmission (From Part Number Index D)
C15,+0006144 = Automatic Transmission (From Part Number Index D)
;
;
;---------------------------------------------------
;
; login/coding-ii
;
;---------------------------------------------------
;
; Older versions use 11 instead of 16!
L00,Brake Electronics (J104) Coding-II
L01,40168 = General Basic Setting Enabling
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
; Newer versions use 16 instead of 11!
S00,Brake Electronics (J104) Security Access
S01,40168 = General Basic Setting Enabling
;
