;
; VCDS Label File
;
; Copyright © 2006-2010 Ross-Tech, LLC
;
; Audi TT (8J)
;
; Component: J793 - Tire Pressure Monitoring II (#4C)
;
; P/N: 8J0-907-274-???
;
; includes measuring blocks and coding
;
; created on 16/Aug/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Apr/2010
;
; requires VCDS 10.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Warning Thresholds I
001,1,Position,Front Left
001,2,Pressure Warning,Front Left,Range: 0.0...255.0
001,3,Position,Front Right
001,4,Pressure Warning,Front Right,Range: 0.0...255.0
;
002,0,Warning Thresholds II
002,1,Position,Rear Left
002,2,Pressure Warning,Rear Left,Range: 0.0...255.0
002,3,Position,Rear Right
002,4,Pressure Warning,Rear Right,Range: 0.0...255.0
;
004,0,Warning Thresholds III
004,1,Pressure Drop,Warning,Range: 0.0...255.0
004,2,Tire Brake-Down,Warning,Range: 0.0...255.0
;
125,0,CAN-Databus Communication
125,1,Transmission,Electronics,Range: Transm. 1/Transm. 0
125,2,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
125,3,Brake Electronics,,Range: ABS 1/ABS 0\nSecification: ABS 1
125,4,Engine Electronics,,Range: Engine 1/Engine 0\nSpecification: Engine 1
;
126,0,CAN-Databus Communication && Voltage Supply
126,1,All-Wheel-Drive,,Range: AWD 1/AWD 0\nSpecification: AWD 1
126,2,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
126,3,Status,Terminal 15,Range: Term 15 On/Term 15 Off
126,4,Battery Voltage
;
127,0,Wheel Speed
127,1,Wheel Speed,Front Left
127,2,Wheel Speed,Front Right
127,3,Wheel Speed,Rear Left
127,4,Wheel Speed,Rear Right
;
130,0,Tire Pressure Monitoring System (TPMS)
130,1,Warning Lamp,,Range: Lamp Off/Lamp On
130,2,Calibration,Button,Range: Switch Off/Switch On
;
140,0,CAN-Databus Communication
140,1,CAN-Gateway,(J533),Range: Gateway 1/Gateway 0\Specification: Gateway 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Tire Pressure Monitoring II (J793) Coding
C01,0?xxx00: System
C02,6 = Tire Pressure Monitoring System (PR-7K6) 
C03,0x?xx00: Powertrain
C04,0 = All-Wheel-Drive (AWD) & Manual Transmission
C05,1 = All-Wheel-Drive (AWD) & Direct-Shift-Gearbox (DSG)
C06,2 = Front-Wheel-Drive (FWD) & Manual Transmission
C07,3 = Front-Wheel-Drive (FWD) & Direct-Shift-Gearbox (DSG) 
C08,0xx?x00: Tires
C09,2 = 16"
C10,3 = 17"
C11,4 = 18"/19"
C12,6 = 16" (SST)
C13,7 = 17" (SST/PAX)
C14,8 = 18"/19" (SST/PAX) 
C15,0xxx?00: Country
C16,1 = Rest of World (RoW) 
;
