;
; VCDS Label File
;
; Copyright © 2013+ Ross-Tech, LLC
;
; VW Transporter (7H/7J)
;
; Component: J347 - Interior Monitoring (#45)
;
; P/N: 7H?-951-171-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7H-45.LBL
; 7Hx-951-171.LBL
;
; includes measuring blocks, security access, coding and adaptation
;
; created on 21/Feb/2013 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 21/Feb/2013
;
; requires VCDS 11.11.5 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Interior Monitoring,Status,Range: active/inactive
001,3,Interior Monitoring,Button (E183),Range: operated/not oper.
;
002,2,Interior Monitoring,Sensor (G305),Range: OK/Not OK
002,3,Termin 15,Status,Range: Term. 15 ON/Term. 15 OFF
;
005,1,Inclination Sensor,Staus (G384),Range: active/inactive
005,3,Inclination Sensor,Button (E360),Range: operated/not oper.
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
S00,Interior Monitoring (J345) Security Access
S01,01034 = Coding Enabling
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Interior Monitoring (J345) Coding
C01,00000?x: Options I
C02,0 = Control Module installed longitudinal / Inclination Sensor NOT installed
C03,1 = Control Module installed longitudinal / Inclination Sensor installed
C04,2 = Control Module installed transverse / Inclination Sensor installed
C05,00000x?: Options II
C06,1 = Interior Monitoring Front / Normal Equipment
C07,2 = Interior Monitoring Front & Rear / Normal Equipment
C08,3 = Interior Monitoring Front / Camper Equipment
C09,4 = Interior Monitoring Front & Rear / Camper Equipment
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Interior Monitoring Sensitivity Front
A001,5,Interior Monitoring Sensitivity Front
A001,6,Adjustment of the Front Interior Monitoring Sensitivity.
A001,7, 
A001,8,Range: 50...100 %
A001,9,Factory/Standard Setting: 100 %
;
A002,0,Interior Monitoring Sensitivity Rear
A002,5,Interior Monitoring Sensitivity Rear
A002,6,Adjustment of the Rear Interior Monitoring Sensitivity.
A002,7, 
A002,8,Range: 50...100 %
A002,9,Factory/Standard Setting: 100 %
;
A003,0,Inclination Sensor Sensitivity Longitudinal
A003,5,Inclination Sensor Sensitivity Longitudinal
A003,6,Adjustment of the Longitudinal Inclination Sensor Sensitivity.
A003,7, 
A003,8,Range: 50...100 %
A003,9,Factory/Standard Setting: 100 %
;
A004,0,Inclination Sensor Sensitivity Transverse
A004,5,Inclination Sensor Sensitivity Transverse
A004,6,Adjustment of the Transverse Inclination Sensor Sensitivity.
A004,7, 
A004,8,Range: 50...100 %
A004,9,Factory/Standard Setting: 100 %
;
