;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Audi A4 (8E/8H)
;
; Component: J527 - Steering Column Electronics (#16)
;
; P/N: 8E0-953-549-T
;
; includes measuring blocks, adaptation and coding
;
; created on 09/Oct/2014 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 09/Oct/2014
;
; requires VCDS 12.12.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Ignition Switch,,1xxxx = Terminal P active\nx1xxx = Terminal S active\nxx1xx = Terminal 75 active\nxxx1x = Terminal 15 active\nxxxx1 = Terminal 50 active
; 1xxxx = Terminal P active
; x1xxx = Terminal S active
; xx1xx = Terminal 75 active
; xxx1x = Terminal 15 active
; xxxx1 = Terminal 50 active
001,2,Blinker,Turn Signal,Range: Not Oper./Left/Right\nSignal Type: Input
001,3,Headlight,Flasher,Range: Not Oper./Operated\nSignal Type: Input
001,4,High Beam,,Range: Not Oper./Operated\nSignal Type: Input
;
002,1,Horn,,Range: Not Oper./Operated\nSignal Type: Input
002,2,Wiper Front,,Range: Not Oper./Level/Stage Int./Stage 1/Stage 2\nSignal Type: Input
002,3,Wiper,Interval Stages,Range: Stage 1/Stage 2/Stage 3/Stage 4\nSignal Type: Input
002,4,Washer Front,,Range: Not Oper./Operated\nSignal Type: Input
;
003,1,Wiper Rear,,Range: Not Oper./Operated/Not Installed\nSignal Type: Input
003,2,Washer Rear,,Range: Not Oper./Operated/Not Installed\nSignal Type: Input
003,3,Board Computer,,Range: Not Oper./Operated\nSignal Type: Input
003,4,Sport Button,,Range: Not Oper./Operated/Not Installed\nSignal Type: Input
;
004,0,Cruise Control System (CCS)
004,1,Main Switch,,Range: ON/OFF\nSignal Type: Input/Output
004,2,CCS-Set,,Range: Not Oper./Operated\nSignal Type: Input
004,3,CCS-Status,,Range: Not Oper.\nSignal Type: Input
;
006,0,Multifunction Steering Wheel (MFSW) I
006,1,Communication,,Range: Not Installed/OK/not OK
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Range: Yes/No
;
007,0,Multifunction Steering Wheel (MFSW) II
007,1,Button 1 OR,Button Left,Range: Not Oper./Operated/Not Installed
007,2,Button 2 OR,Button Right,Range: Not Oper./Operated/Not Installed
007,3,Button 3 OR,Wheel Button Left,Range: Not Oper./Operated/Not Installed
007,4,Button 4 OR,Wheel Button Right,Range: Not Oper./Operated/Not Installed
;
008,0,Multifunction Steering Wheel (MFSW) III
008,1,Button 5 OR,Wheel Left,Range: Not Oper./Operated/Not Installed OR Not Oper./Not Installed/Scroll Up/Scroll Down
008,2,Button 6 OR,Wheel Right,Range: Not Oper./Operated/Not Installed OR Not Oper./Not Installed/Volume Up/Volume Down
;
009,1,Dimming,(Terminal 58d),Range: 0.0...100.0 %
009,2,Right Hand Drive,,Range: Yes/No
009,3,Seat Heating,Left,Range: OFF/[Stage]
009,4,Seat Heating,Right,Range: OFF/[Stage]
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
125,2,Central Electronics,(J519),Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
125,3,Heating/Air,Condition (J255),Range: HVAC 1/HVAC 0\nSpecification: HVAC 1
;
126,0,CAN-Databus Comfort (Communication)
126,1,Door Electronics,Driver (J386),Range: Dr. Door 1/Dr. Door 0\nSpecification: Dr. Door 1
126,2,Door Electronics,Passenger (J387),Range: Pas. Door 1/Pas. Door 0\nSpecification: Pas. Door 1
126,3,Door Electronics,Rear Left (J388),Range: RL Door 1/RL Door 0\nSpecification: RL Door 1
126,4,Door Electronics,Rear Right (J389),Range: RR Door 1/RR Door 0\nSpecification: RR Door 1
;
127,0,CAN-Databus Infotainment (Communication)
127,1,Radio (analog),(R),Range: Radio 1/Radio 0\nSpecification: Radio 1
127,2,Telephone,Electronics (R36),Range: Telephone 1/Telephone 0\nSpecification: Telephone 1
127,3,Voice Control,(J507),Specification: VoiceCmd 1\nRange: VoiceCmd 1/VoiceCmd 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,?xxxx: Options I
C02,0 = Navigation not installed
C03,1 = Navigation installed
C04,x??xx: Steering Wheel
C05,24 = RS4 Multifunction Steering Wheel with Radio Control (PR-2FS+9W0+QH0)
C06,34 = RS4 Multifunction Steering Wheel with Radio/Telephone Control (2FS+9ZH/9ZJ+QH0)
C07,44 = RS4 Multifunction Steering Wheel with Radio/Telephone/Voice Control (PR-2FS+9ZH/9ZJ+QH1)
C08,44 = RS4 Multifunction Steering Wheel with Radio/Telephone/Voice Control/Cell Phone/Telematics (PR-2FS+9ZF/9ZG/9ZS+QH0/QH1)
C09,54 = RS4 Multifunction Steering Wheel with Radio/Voice Control (PR-2FS+9W0+QH1)
C10,60 = RS4 Sport Steering Wheel (PR-2PX)
C11,xxx?x: Board Computer & Cruise Control
C12,0 = Board Computer installed / RS4 Steering Wheel (PR-9Q2/9Q4+8T0+2PX)
C13,1 = Board Computer installed / RS4 Multifunction Steering Wheel (PR-9Q2/9Q4+8T0+2FS)
C14,2 = Board Computer & Cruise Control installed / RS4 Steering Wheel (PR-9Q2/9Q4+8T1+2PX)
C15,4 = Board Computer & Cruise Control installed / RS4 Multifunction Steering Wheel (PR-9Q2/9Q4+8T1+2FS)
C16,0xxx?: Rear Wiper (Chassis)
C17,1 = Rear Wiper not installed (Sedan/Cabriolet)
C18,2 = Rear Wiper installed (Avant)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A081,0,Component Protection (Vehicle Identification Number)
A081,5,Component Protection (Vehicle Identification Number)
A081,6,To Start the Vehicle Identification Number (VIN)
A081,7,Learning Process enter/save 00111 as new Value.
;;
