;
; VAG-COM Label File
;
; Audi A6 (4F) / Audi Q7 (4L)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 4F0-910-549-???
;
; includes measuring blocks, coding and selective output test
;
; created on 14/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 16/May/2007
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: Not Oper./Left/Right
001,2,Headlamp Flasher,,Display Range: Not Oper./Operated
001,3,High Beam,,Display Range: Not Oper./Operated
001,4,Front Wiper,,Display Range: Not Oper./Level/Stage Int./Stage 1/Stage 2
;
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: Not Oper./Operated
002,3,Wiping Rear,,Display Range: Not Oper./Operated/Not Installed
002,4,Washing Rear,,Display Range: Not Oper./Operated/Not Installed
;
003,1,Horn,,Display Range: Not Oper./Operated
003,2,Board Computer,,Display Range: Not Oper./Operated
003,3,Steering Column,Adjustment,Display Range: Not Oper./Operated
003,4,Easy-Entry,,Display Range: Not Installed/ON/OFF
;
004,0,Cruise Control System (CCS) / Adaptive Cruise Control (ACC)
004,1,Main Switch,,Display Range: ON/OFF
004,2,CCS/ACC-Set,,Display Range: Not Oper./Operated
004,3,CCS/ACC-Status,,Display Range: Not Oper.
004,4,ACC Time Gap,Adjustment,Display Range: Not Installed/Not Oper.
;
005,0,Multifunction Steering Wheel I
005,1,Communication,,Display Range: Not Installed/OK/not OK
005,2,Software Version
005,3,Hardware Version
005,4,Malfunction,recognized,Display Range: Yes/No
;
006,0,Multifunction Steering Wheel II
006,1,Multi-Function,Button (Left),Display Range: Not Installed/Not Oper./Operated
006,2,Multi-Function,Button (Right),Display Range: Not Installed/Not Oper./Operated
006,3,Thumb Button,(Left),Display Range: Not Installed/Not Oper./Operated
006,4,Thumb Button,(Right),Display Range: Not Installed/Not Oper./Operated
;
007,0,Multifunction Steering Wheel III
007,1,Thumb Wheel,(Left),Display Range: Not Installed/Not Oper.
007,2,Thumb Wheel,(Right),Display Range: Not Installed/Not Oper.
007,3,Tiptronic,(Down),Display Range: Not Installed/Not Oper./Operated
007,4,Tiptronic,(Up),Display Range: Not Installed/Not Oper./Operated
;
008,0,Heated Steering Wheel && Heated Seats
008,1,Steering Wheel,Heater,Display Range: Not Installed/OFF/ON\nSignal Type: Output
008,2,Temperature,,Display Range: Not Installed/Temperature\nSignal Type: Input
008,3,Steering Wheel,Heater Output,Signal Type: Output
008,4,Heated Seats,,Display Range: OFF/Stage\nSignal Type: Input
;
009,0,Dimming
009,1,Dimming,,Display Range: 0.0...100.0 %\nSignal Type: Input
009,2,Dimming,(Discrete),Display Range: 0.0...100.0 %\nSignal Type: Input
009,3,Dimming,(LIN-Databus),Display Range: 0.0...100.0 %\nSignal Type: Input
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,0?xxxxx: Model
C02,0 = Left Hand Steering / 1 = Right Hand Steering
C03,0x?xxxx: Steering Column Adjustment
C04,+1 = Electric Steering Column Adjustment
C05,+2 = Lane Departure Warning
C06,0xx?xxx: Steering Wheel
C07,0 = Standard Steering Wheel
C08,1 = Sport Steering Wheel
C09,2 = Multi-Function Steering Wheel
C10,0xxx?xx: Tiptronic & Heating
C11,+1 = with Tiptronic / +2 = with Steering Wheel Heating
C12,0xxxx?x: Board Computer / Cruise Control System (CCS) / Adaptive Cruise Control (ACC)
C13,0 = No Board Computer - No Cruise Control System (CCS) - No Adaptive Cruise Control (ACC)
C14,1 = with Board Computer
C15,2 = with Cruise Control System (CCS)
C16,3 = with Adaptive Cruise Control (ACC)
C17,4 = with Board Computer and Cruise Control System (CCS)
C18,5 = with Board Computer and Adaptive Cruise Control (ACC)
C19,0xxxxx?: Chassis
C20,1 = Sedan / 2 = Avant (with Rear Wiper)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1752,Heated Steering Wheel (Z36)
;
