;
; VCDS Label File
;
; Copyright © 2004-2010 Ross-Tech, LLC
;
; Audi A3 (8P) / Seat Altea/Toledo (5P) / Seat Leon (1P)
; Skoda Octavia II (1Z) / VW Caddy (2K) / VW Golf/Jetta (1K)
; VW Touran (1T)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 1K0-953-549-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1K-16.LBL
; 1K0-953-549-MY8.LBL (< SW 0101)
; 1K0-953-549-MY9.LBL (SW 0110 >)
;
; includes measuring blocks, coding and selective output test
;
; created on 05/Apr/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 26/May/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: n. operated/left/right
001,2,Headlamp Flasher,,Display Range: n. operated/operated
001,3,High Beam,,Display Range: n. operated/operated
001,4,Front Wiper,,Display Range: n. operated/level/Stage Int./Stage 1/Stage 2
;
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: n. operated/operated
002,3,Wiping Rear,,Display Range: n. operated/operated/not installed
002,4,Washing Rear,,Display Range: n. operated/operated/not installed
;
003,1,Terminal Status,,?xxxx - P-Contact\nx?xxx - S-Contact\nxx?xx - Terminal 75\nxxx?x - Terminal 15\nxxxx? - Terminal 50
003,2,Horn,,Display Range: n. operated/operated
003,3,Multi-Function,Display,Display Range: n. installed/n. operated/Reset/Up/Down
;
004,0,Cruise-Cntrol-System
004,1,Main Switch,,Display Range: n. installed/off/on
004,2,CCS-Set,,Display Range: n. operated/decelerate/accelerate/Reset
;
005,1,Park Position in,Selector Lever,Display Range: n. installed/n.Ok/on/recognized
005,2,Selector Lever,Information (Pos. P),Display Range: n. defined/recognized/on
005,3,Key,Removal Lock,Display Range: n. installed/on/off
005,4,Status Key,Removal Lock,Display Range: n. installed/Ok/n.Ok
;
006,0,Multi-Function Steering Wheel
006,1,Communication,,Display Range: n. intalled/Ok/n.Ok
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Display Range: yes/no
;
007,0,Multifunction Steering Wheel II
007,1,Vehicle Type
; 0 = Volkswagen
; 1 = Audi
; 2 = Seat
; 3 = Skoda
; 4 = Volkswagen Nutzfahrzeuge
; 5 = Bugatti
; 6 = Lamborghini
; 7 = Bentley
; 8 = Rolls Royse
; 14 = Ford
; 15 = Porsche
007,2,Vehicle Version
;
008,0,Multifunction Steering Wheel III
008,3,Tiptronic,(Down),Display Range: Not Installed/Not Oper./Operated
008,4,Tiptronic,(Up),Display Range: Not Installed/Not Oper./Operated
;
010,0,Heated Steering Wheel && Heated Seats
010,1,Steering Wheel,Heater,Display Range: Not Installed/OFF/ON\nSignal Type: Output
010,2,Temperature,,Display Range: Not Installed/Temperature\nSignal Type: Input
010,3,Steering Wheel,Heater Output,Signal Type: Output
010,4,Heated Seats,,Display Range: OFF/Stage\nSignal Type: Input
;
011,0,Dimming
011,1,Dimming,,Display Range: 0.0...100.0 %\nSignal Type: Input
011,2,Dimming,(Discrete),Display Range: 0.0...100.0 %\nSignal Type: Input
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,0?xxxxx: Vehicle Type
C02,0 = Normal / 1 = Special Purpose (e.g Taxi)
C03,0x?xxxx: Transmission
C04,0 = Manual Transmission
C05,1 = Automatic Transmission
C06,0xx?xxx: Steering Wheel
C07,0 = Steering Wheel without Multifunction
C08,1 = 3-Spoke Steering Wheel without Multifunction
C09,2 = 3/4-Spoke Steering Wheel with Multifunction without Cruise & Voice Control
C10,3 = 3/4-Spoke Steering Wheel with Multifunction with Cruise & Voice Control
C11,0xxx?xx: Additional Equipment
C12,+1 = Tiptronic (Shift Paddels)
C13,0xxxx?x: Board Computer / Cruise Control System (CCS)
C14,0 = w/o Board Computer and w/o Cruise Control System (CCS)
C15,1 = with Board Computer and w/o Cruise Control System (CCS)
C16,2 = w/o Board Computer and with Cruise Control System (CCS)
C17,4 = with Board Computer and with Cruise Control System (CCS)
C18,0xxxxx?: Rear Wiper
C19,1 = Rear Wiper not installed
C20,2 = Rear Wiper installed
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T194,Ignition Key Removal Lock
;
