;
; VCDS Label File
;
; Copyright © 2009 Ross-Tech, LLC
;
; Skoda Fabia (6Y) / Skoda Octavia (1U)
;
; Component: R - Radio (#56) - Symphony
;
; P/N: 17S-035-159-??? / 1U0-035-156-??? / 6Y0-035-156-???
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6Y-56.LBL
; 1U0-035-156.LBL
;
; includes measuring blocks, adaptation and coding
;
; created on 15/Oct/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Oct/2009
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,GALA/Speed Signal,,0 = Signal NOT recognized\n1 = Signal recognized
001,2,Supply Voltage,(Terminal 30),Range: 5.0...18.0 V
001,3,Dimming,Terminal 58d (CAN),Specification: 29.0...98.0 %
001,4,Status,S-Contact (CAN),Range: ON/OFF
;
002,0,Speaker/Line-Out (Front)
002,1,Location/Type
002,2,Status
002,3,Location/Type
002,4,Status
;
003,0,Speaker/Line-Out (Rear)
003,1,Location/Type
003,2,Status
003,3,Location/Type
003,4,Status
;
004,0,Remote Feed Antenna
004,1,Type
004,2,Component
004,3,Status
;
005,0,Amplifier / Telephone Mute
005,1,Control Output,Amplifier,0 = OK\n1 = Short to Ground
005,3,Telephone,Mute
005,4,Status,Mute,Range: ON/OFF
;
006,0,Communication Status CD-Changer (R41)
006,1,Component
006,2,Status
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C03,00?xx: Speaker Channels
C04,0 = No passive Speakers (Sound System)
C05,2 = 2 passive Speakers Front and 0 passive Speakers Rear
C06,3 = 0 passive Speakers Front and 2 passive Speakers Rear
C07,4 = 4 passive Speakers
C08,00x?x: Sound System Correction
C09,0 = No Sound System (No Correction)
C10,00xx?: Radio Configuration
C11,+1 = Active/Remote Powered Antenna
C12,+2 = CD-Player/Changer
C13,+4 = CAN-Secondary Display (Board Computer/large Display)
;
