;
; VCDS Label File
;
; Copyright © 2007+ Ross-Tech, LLC
;
; Seat Ibiza/Cordoba (6L) / Skoda Fabia (6Y) / VW Polo (9N)
;
; Component: J519 - Central Electronics I (#09) (from Index C)
;
; P/N: 6Q?-937-049-???
;
; includes measuring blocks, (converted) coding and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6Q-09.LBL
; 6Qx-937-049-B.LBL (through Index B)
; 6Qx-937-049-C.LBL (from Index C)
;
; created on 07/29/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 29/May/2015 by Sebastian Stange (Sebastian@Ross-Tech.com) // Converted Coding added
;
; last modification on 29/May/2015
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Terminal Status
001,1,Terminal S,Status,Range: operated/inactive
001,2,Terminal 50,Status,Range: ON/OFF
001,3,Terminal X,Status,Range: ON/OFF
001,4,Terminal 15,Status,Range: ON/OFF
;
002,1,Voltage,(Terminal 30)
002,2,Load Managem.,Intervention,Range: active/inactive
002,3,Blinker Switch,,Range: ON/OFF
002,4,Emergency,Flasher Button,Range: ON/OFF
;
003,0,Wiper (Front)
003,1,Wiper,,Range: ON/OFF
003,2,Wiper,Stage 1,Range: ON/OFF
003,3,Wiper,Stage 2,Range: ON/OFF
003,4,Wiper,Potentiometer,Range: Not Recognized/Stage 1/Stage 2/Stage 3/Stage 4
;
004,1,Windshield,Washer Pump,Range: ON/OFF
004,2,Rear Windshield,Heating,Range: Not Operated/Operated
004,3,Horn,,Range: Not Operated/Operated
004,4,Hood Contact,Switch,Range: ON/OFF
;
005,0,Door Status
005,1,Driver's Door,Contact Switch,Range: Door open/Door closed
005,2,Passenger Door,Contact Switch,Range: Door open/Door closed
005,3,Rear Left,Contact Switch,Range: Door open/Door closed
005,4,Rear Right,Contact Switch,Range: Door open/Door closed
;
006,0,Trunk Lid Status (II)
006,1,Trunk Contact,Switch (Locking),Range: ON/OFF
006,2,Trunk Contact,Switch (Light),Range: ON/OFF
;
007,0,Trunk Lid Status (II)
007,1,Trunk Lid Handle,Push-Button,Range: Not Operated/Operated
007,2,Trunk Lid Interior,Push-Button,Range: Not Operated/Operated
007,3,Lock,Service Position,,Range: ON/OFF
;
008,1,Headlight Washers,,Range: ON/OFF/Not Installed
008,2,Heated Mirrors,,Range: ON/OFF
008,3,Reverse Gear,,Range: Reverse OFF/Reverse ON
008,4,Heated Front,Windshield,,Range: ON/OFF/Not Installed
;
009,0,Cruise Control System (CCS)
009,1,CCS Main Switch,,Range: Not Operated/Operated
009,2,CCS Main Switch,,Range: Not Operated/Operated
009,3,CCS Switch,SET/(-),Range: Not Operated/Operated
009,4,CCS Switch,RES/(+),Range: Not Operated/Operated
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics (J519) Coding
C01,+00001 = Trailer Hitch installed
C02,+00002 = Trunk Lid Remote Unlocking installed
C03,+00004 = Electric Load Management active
C04,+00008 = Interior Light Control
C05,+00016 = Seat Backrest Recognition installed
C06,+00032 = Heated Front Seats installed
C07,+00128 = Heated Mirrors installed
C08,+00256 = Headlight Washers installed
C09,+00512 = Rain Sensor installed
C10,+01024 = Trunk Lid Remote Unlocking impulse driven
C11,+08192 = Rear Windshield Wiper with Comfort Function installed
C12,+16384 = Electric Fuel Pump Releay installed
C13, 
C14,Note #1: Coding Value is the Sum of the individual Options!
C15,Note #2: You can also use the Coding Assist/Helper!
;
;
;---------------------------------------------------
;
; converted coding
; (short coding displayed as long coding for easier modifications)
;
;---------------------------------------------------
;
;
LC,02,0,Trailer Hitch installed
LC,02,1,Trunk Lid Remote Unlocking installed
LC,02,2,Electric Load Management active
LC,02,3,Interior Light Control
LC,02,4,Seat Backrest Recognition installed
LC,02,5,Heated Front Seats installed
LC,02,7,Heated Mirrors installed
LC,01,0,Headlight Washers installed
LC,01,1,Rain Sensor installed
LC,01,2,Trunk Lid Remote Unlocking impulse driven
LC,01,5,Rear Windshield Wiper with Comfort Function installed
LC,01,6,Electric Fuel Pump Releay installed
LC,01,7=,Additional Coding Options can be found in Byte 02!
LC,00,3=,Coding Details can be found in Byte 01 && Byte 02!
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Terminal 30G Deactivation/Reset
A001,5,Terminal 30G Deactivation/Reset
A001,6,Range: 1-253 (0.66...173 Minutes)
A001,7,Standard: 44 (30 Minutes)
;
A002,0,Front Windshield Heating Activation Time
A002,5,Front Windshield Heating Activation Time
A002,6,Range: 1...253 (0.66...173 Minutes)
A002,7,Special: 254 (infinite)
A002,8,Standard: 29 (20 Minutes)
;
A003,0,Mirror Heating Activation Time
A003,5,Mirror Heating Activation Time
A003,6,Range: 1...253 (0.66...173 Minutes)
A003,7,Standard (through 04/2002): 29 (20 Minutes)
A003,8,Standard (from 05/2002): 254 (infinite)
;
A004,0,Rear Windshield Heating Activation Time
A004,5,Rear Windshield Heating Activation Time
A004,6,Range: 1...253 (0.66...173 Minutes)
A004,7,Standard: 29 (20 Minutes)
A004,8,Special: 254 (infinite)
;
A005,0,Trunk Lid Remote Unlocking
A005,5,Trunk Lid Remote Unlocking
A005,6,Range: 1...253 (0.32-81.6 Seconds)
A005,7,Standard: 3 (1 Seconds)
;
A006,0,Comfort Blinking (Cycles)
A006,5,Comfort Blinking (Cycles)
A006,6,Range: 0...5
A006,7,Standard: 3
;
A007,5,Tear Wiping (Delay)
A007,6,Tear Wiping (Delay)
A007,7,Range: 0...255 Seconds
A007,8,Standard: 5 Seconds
;
A008,0,Headlight Washer Activation
A008,5,Headlight Washer Activation
A008,6,Range: 0...255 Seconds
A008,7,Standard: 5 Seconds
;
A009,0,Rear Windshield Heating
A009,5,Rear Windshield Heating
A009,0 = Normal Functionality
A009,1 = Advanced Functionality
;
