;
; VCDS Label File
;
; Copyright © 2011 Ross-Tech, LLC
;
; Skoda Fabia (6Y) / VW Polo (9N)
;
; Component: J104 - Brake Electronics (#03) - MK60 ABS
;
; P/N: 6Q0-907-37?-???
;
; includes measuring blocks
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6Q-03.LBL
; 6R-03.LBL
; 6Q0-907-37x-ABS.LBL  (ABS/EDS 5.7)
; 6Q0-907-37x-ABS2.LBL (ABS/EDS MK60)
; 6Q0-907-37x-ASR.LBL  (ABS/EDS/ASR 5.7)
; 6Q0-907-37x-ESP.LBL  (ABS/EDS/ASR/ESP 5.7)
; 6R0-907-37x-ABS.LBL  (ABS/EDS 8.0)
; 6R0-907-37x-ASR.LBL  (ABS/EDS/ASR 8.0)
; 6R0-907-37x-ESP.LBL  (ABS/EDS/ASR/ESP 8.0)
;
; created on 22/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 08/Dec/2011
;
; requires VCDS 11.11.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
002,0,Starting Wheel Speed
002,1,Speed Sensor,Front Left (G47),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,2,Speed Sensor,Front Right (G45),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,3,Speed Sensor,Rear Left (G46),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,4,Speed Sensor,Rear Right (G44),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
;
003,0,Switches and Warning Lights
003,1,Brake Light,Switch (F),Range: Not Oper./Operated
003,2,Brake System,Warning L. (K118),Range: ON/OFF
003,3,ABS,Warning L. (K47),Range: ON/OFF
;
011,0,Speed Encoder Errors (Front Left)
;
012,0,Speed Encoder Errors (Front Right)
;
013,0,Speed Encoder Errors (Rear Left)
;
014,0,Speed Encoder Errors (Rear Right)
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Control,Module (ECM),Range: Engine 1/Engine 0\nSpecification: Engine 1
125,4,Transmission,Control Module,Range: Transm. 1/Transm. 0\nSpecification: Transm. 1
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Engine Control,Module (ECM)
225,4,Transmission,Control Module
;
