;
; VAG-COM Label File
;
; Audi A6 (4F) / Audi A8 (4E) / Audi Q7 (4L)
;
; Component: R41 - Media Player (#0E/#1E) - CD/MP3-Changer
;
; P/N: 4E0-910-111-???
;
; includes measuring blocks and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4L-0E.LBL
; 4L-1E.LBL
; 8T-0E.LBL
; 8T-1E.LBL
; 4E0-910-111.LBL
;
; created on 12/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 06/Jul/2007
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltages
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,0000xxx1 = Term. S active\n0000xx1x = Term. 15 active\n0000x1xx = Term. X active\n00001xxx = Term. 50 active
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
;
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,0,Drive/Button Functions
004,1,Drive/Button,Functions,xxxxxxx1 = Eject Button pressed\nxxxxxx1x = CD loading\nxxxxx1xx = Button for CD1 pressed\nxxxx1xxx = Button for CD2 pressed\nxxx1xxxx = Button for CD3 pressed\nxx1xxxxx = Button for CD4 pressed\nx1xxxxxx = Button for CD5 pressed\n1xxxxxxx = Button for CD6 pressed
004,2,Drive,Functions,xxxxxx1 = Playback active\nxxxxx1x = Stop\nxxxx1xx = Pause active\nxxx1xxx = CD loading\nxx1xxxx = CD is ejected\nx1xxxxx = Search forward active\n1xxxxxx = Search back active
;
005,0,Disc Identity
005,1,Disc Identity
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
