;
; VCDS Label File
;
; Copyright © 2005+ planGarage.de for Ross-Tech, LLC
;
; Audi A4 (8E/8H) / Audi A6 (4B) / Audi A8 (4D)
; Skoda Superb (3U / VW Passat (3B)
;
; Component: J431 - Headlight Aim Control (#55) - DYNAMIC REGULATION
;
; P/N: 4B0-907-357-??? / 4Z7-907-357-???
;
; includes measuring blocks, basic settings and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4B-55.LBL
; 4Z-55.LBL
; 4B0-907-357-AUT.LBL
; 4B0-907-357-DYN.LBL
;
; created on 27/Sep/2004 by Sebastian Stange (sst@plangarage.de)
;
; last modification on 10/Mar/2017
;
; requires VCDS 17.1.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage Supply,(Terminal 15),Specifcation: 0.0...15.0 V
001,2,Light Switch,Status,Specification:\n0 = Light OFF\n1 = Light ON
001,3,Vehicle Speed,,Specification: 0...300 km/h
001,4,Acceleration,(Vehicle),Specification: 0.00...7.00 m/s²
;
B001,0,Adjustment Position (Step 1)
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,General
002,1,Front Level,Sensor (G78),Range: 0.0...5.0 V\nSpecification: 1.56...3.45 V\n0.00 V = level sensor faulty\n5.00 V = wiring faulty
002,2,Rear Level,Sensor (G76),Range: 0.0...5.0 V\nSpecification: 0.50...4.50 V\n0.00 V = level sensor faulty\n5.00 V = wiring faulty
002,3,Actuator Motors,Specification,Range: 0.0...100.0 %
002,4,Time Constant,,Range: 0.0...2.0 s
;
B002,0,Adjustment Position learning (Step 2)
B002,1,Status, , 
B002,2, , , 
B002,3, , , 
B002,4, , , 
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Head Light Aim Control (J431) Coding
C01,00001 = Audi A8 (4D)
C02,00005 = Skoda Superb (3U) Front-Wheel-Drive (FWD)
C03,00006 = Skoda Superb (3U) All-Wheel-Drive (AWD)
C04,00007 = VW Passat (3B) Front-Wheel-Drive (FWD)
C05,00008 = VW Passat (3B) All-Wheel-Drive (AWD)
C06,00020 = Audi A6/S6 (4B) (through MY 2000)
C07,00030 = Audi Allroad (4H)
C08,00040 = Audi A6/S6/RS6 (4B) Front-Wheel-Drive (FWD) (from MY 2001)
C09,00050 = Audi A6/S6/RS6 (4B) All-Wheel-Drive (AWD) (from MY 2001)
C10,00060 = Audi A4/S4/RS4 (8E)
C11,00070 = Audi A4/S4/RS4 Cabriolet (8H)
;
