;
; VCDS Label File
;
; Copyright © 2004-2011 Ross-Tech, LLC
;
; Component: J533 - Gateway (#19)
;
; P/N: 6N0-909-901-???
;
; This file is part of a label file package
; make sure you have all of the following files.
;
; 6N-19.LBL
; 6N0-909-901-19.LBL
; 6N0-909-901-6R.CLB
; 6N0-909-901-7L.CLB
;
; includes measuring blocks and coding
;
; created by Davin Swanson
; modified on 14/Mar/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; modified on 30/Aug/2005 by Michael Moore (Moore@Ross-Tech.com)
;
; last modification on 26/Dec/2011
;
; requires VCDS 805.0 / LCode 807.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Electronics,,Range: Engine 1/Engine 0\nSpecification: Engine 1
125,2,Transmission,Electronics,Range: Transm. 1/Transm. 0\nSpecification: Transm. 1
125,3,Brake Electronics,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
125,4,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
126,2,Airbag System,(J234),Range: Airbag 1/Airbag 0\nSpecification: Airbag 1
126,3,Steering Aid,(J500),Range: Steering 1/Steering 0\nSpecification: Steering 1
;
127,0,CAN-Databus Powertrain (Communication)
127,1,All-Wheel-Drive,Electronics (J492),Range: AWD 1/AWD 0\nSpecification: AWD 1
;
128,0,CAN-Databus Powertrain (Communication)
128,1,Battery,Management
128,2,Electrical,Ignition Lock 1
128,3,Level control
;
130,0,CAN-Databus Comfort (Communication)
130,1,CAN-Comfort,Status,Range: 2-Wire/1-Wire\nSpecification: 2-Wire
130,2,Comfort System,(J393),Range: Central 1/Central 0\nSpecification: Central 1
130,3,Door Electronics,Driver (J386),Range: Dr. Door 1/Dr. Door 0\nSpecification: Dr. Door 1
130,4,Door Electronics,Passenger (J387),Range: Pas. Door 1/Pas. Door 0\nSpecification: Pas. Door 1
;
131,0,CAN-Databus Comfort (Communication)
131,1,Door Electronics,Rear Left (J388),Range: RL Door 1/RL Door 0\nSpecification: RL Door 1
131,2,Door Electronics,Rear Right (J389),Range: RR Door 1/RR Door 0\nSpecification: RR Door 1
131,3,Seat Memory,Driver (J521),Range: Memory 1/Memory 0\nSpecification: Memory 1
131,4,Central Electronics,(J519),Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
;
132,0,CAN-Databus Comfort (Communication)
132,2,Steering Wheel,Electronics (J527),Range: St. Wheel 1/St. Wheel 0\nSpecification: St. Wheel 1
132,3,Heating/Air,Condition (J255),Range: A/C 1/A/C 0\nSpecification: A/C 1
132,4,Tire Pressure,Monitoring (J502),Range: Tire 1/Tire 0\nSpecification: Tire 1
;
133,0,CAN-Databus Comfort (Communication)
133,1,Roof,Electronics
133,2,Pax Seat,Memory
133,3,Rear Seat,Memory
133,4,Park Distance,Control
;
134,0,CAN-Databus Comfort (Communication)
134,2,Electrical,Ignition Lock
134,3,Wiper Motor,Control Module
;
135,0,CAN-Databus Comfort (Communication)
135,2,Display Control,Front
135,3,Display Control,Rear
;
136,0,CAN-Databus Comfort (Communication)
136,2,Central,Locking
;
140,0,CAN-Databus Infotainment (Communication)
140,1,CAN-Infotainment,Status,Range: 2-Wire/1-Wire\nSpecification: 2-Wire
140,2,Analog Radio,,Range: Radio 1/Radio 0\nSpecification: Radio 1
140,3,Navigation,,Range: Navigation 1/Navigation 0\nSpecification: Navigation 1
;
141,0,CAN-BUS Status (1 = OK / 0 = not OK)
141,4,Telematics
;
142,0,CAN-BUS Status (1 = OK / 0 = not OK)
142,1,Display Control,Front
;
143,0,CAN-BUS Status (1 = OK / 0 = not OK)
143,1,Digital Sound,Processor
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Engine Electronics
225,2,Transmission,Electronics
225,3,Brake Electronics,(J104)
225,4,Instrument Cluster,(J285)
;
226,0,CAN-Databus Powertrain (Timeout)
226,1,Steering Angle,Sensor (G85)
226,2,Airbag System,(J234)
226,3,Steering Aid,(J500)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Diagnostic Interface for Datenbus (J533) Coding
C01,+00001 = Automatic Transmission (through MY 2001 and all PQ24 | Polo/Fabia/Ibiza/Cordoba)
C02,+00002 = Brake Electronics
C03,+00004 = Airbags (not for VW Transporter/Multivan 70/7D)
C04,+00008 = Steering Aid (only PQ24 | Polo/Fabia/Ibiza/Cordoba)
C05,+00016 = All-Wheel-Drive (only Transporter/Multivan 7H/7J)
C05, 
C06,Note: Recoding (even with the same value) results in refreshing the
C07,Gateway Installation List (e.g. useful/necessary after retrofits).
;
